|  |  |
| --- | --- |
| Transmitted by the experts from CLEPA | Informal document **WP.29-170-04**  (170th WP.29, 15-18 November 2016, agenda item 4.8.1) |

Proposal to amend the Proposal for Supplement 8 to the 06 series of amendments to Regulation No. 16 (Safety-belts, ISOFIX and i-Size) (ECE/TRANS/WP.29/2016/98)

I. Proposal

*Paragraph 12.1.* amend to read:

“12.1. In case a restraint system has been granted~~/refused/~~extended~~/withdrawn~~,2 those can be used for particular types of vehicles compatible with the following dimensional conditions: no interior part in a quoted A-zone as shown below (Figure 2):

Figure 2



*\_\_\_\_\_\_\_\_\_\_\_\_\_*

~~2 Strike out what does not apply.~~

”

II. Justification

The proposal clarifies the subject of paragraph 12.1 and corrects an editorial error concerning the repetition of footnote 2 that exists already in Annex 1B to Regulation 16.

\_\_\_\_\_\_\_\_\_\_\_