|  |  |  |
| --- | --- | --- |
|   | United Nations | ECE/TRANS/WP.29/2017/8 |
| Description: _unlogo | **Economic and Social Council** | Distr.: General22 December 2016Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**171st session**

Geneva, 14-17 March 2017

Item 4.7.1 of the provisional agenda

**1958 Agreement:
Consideration of draft amendments to existing
Regulations submitted by GRRF**

 Proposal for Supplement 17 to Regulation No. 75
(Tyres for L-category vehicles)

**Submitted by the Working Party on Brakes and Running Gear**[[1]](#footnote-2)\*

The text reproduced below was adopted by the Working Party on Brakes and Running Gear (GRRF) at its eighty-second session (ECE/TRANS/WP.29/GRRF/82, para. 34). It is based on ECE/TRANS/WP29/GRRF/2016/37. It is submitted to the World Forum for Harmonization of Vehicle Regulations (WP.29) and to the Administrative Committee (AC.1) for consideration at their March 2017 sessions.

 Supplement 17 to Regulation No. 75 (Tyres for L-category vehicles)

*Paragraph 1.,* amendto read:

 "1. Scope

 This Regulation applies to new pneumatic tyres**\*** for vehicles of category L.1,2 However, it does not apply to tyre types designed exclusively for the "off-road" use, which are marked "NHS" (Not for Highway Service) and to tyre types designed exclusively for competitions.

\* For the purpose of this Regulation "tyres" means "pneumatic tyres"."

*Paragraph 2.1.,* amendto read:

"2.1. "*Type of tyre*" means a category of tyres which do not differ in such essential characteristics as:

(a) The manufacturer's name;

(b) Tyre-size designation;

(c) Category of use (normal: for normal highway service; snow, moped, all terrain (AT), special: for special application such as on- and off-road);

(d) Structure (diagonal or bias-ply, bias**-**belted, radial);

(e) Speed category symbol;

(f) Load-capacity index;

(g) Tyre cross-section."

*Insert a new paragraph 2.2.* to read:

"2.2. "*Manufacturer*" means the person or body who is responsible to the Type Approval Authority (TAA) for all aspects of the type-approval and for ensuring the conformity of production."

*Insert a new paragraph 2.3.* to read:

"2.3. "*Brand name/trademark*" means the identification of the brand or trademark as defined by the tyre manufacturer and marked on the sidewall(s) of the tyre. The brand name/trademark may be the same as that of the manufacturer."

*Insert a new paragraph 2.4.* to read:

"2.4. "*Trade description/commercial name*" means an identification of a range of tyres as given by the tyre manufacturer. It may coincide with the brand name/trademark."

*Paragraphs 2.2. to 2.2.3.* renumber as paragraphs 2.5. to 2.5.3.and in these renumbered paragraphs,replace"pneumatic tyre"by"tyre".

*Paragraph 2.2.4.,* amendto read :

"2.5.4. "*Reinforced*" describes a tyre designed to operate at higher loads and higher inflation pressures than the corresponding standard tyre."

*Paragraphs 2.3. to 2.33.2.* renumber as paragraphs 2.6. to 2.36.2. and in these renumbered paragraphs,replace"pneumatic tyre"by"tyre".

*Paragraph 2.33.3.,* renumber and amendto read :

"2.36.3. For speeds above 210 km/h but not exceeding 270 km/h, the maximum load rating must not exceed the percentage of the mass, associated with the load capacity index of the tyre, indicated in the table below with reference to the speed category symbol of the tyre and the maximum design speed of the vehicle to which the tyre is to be fitted:

|  |  |
| --- | --- |
| *Maximum speed (km/h)\*\*\** | *Maximum Load Rating (%)* |
| *Speed Category Symbol V* | *Speed Category Symbol W\*\** |
| 210 | 100 | 100 |
| 220 | 95 | 100 |
| 230 | 90 | 100 |
| 240 | 85 | 100 |
| 250 | (80)\* | 95 |
| 260 | (75)\* | 85 |
| 270 | (70)\* | 75 |
| \* Applicable only to tyres identified by means of letter code "V" within the size designation and up to the maximum speed specified by the tyre manufacturer.\*\* Applicable also to tyres identified by means of letter code "Z" within the size designation.\*\*\* For intermediate speeds linear interpolation of maximum load rating is allowed. |

"

*Paragraphs 2.33.4. and 2.34.* renumber as paragraphs 2.36.4. and 2.37.

*Paragraph 3.1.,* amendto read:

"3.1. Tyres submitted for approval shall bear on at least one sidewall the following markings:

3.1.1. The manufacturer’s name or the Brand name/trademark;"

*Insert a new paragraph 3.1.2.* to read:

"3.1.2. The trade description/commercial name (see paragraph 2.4. of this Regulation). However, the trade description is not required when it coincides with the brand name/trademark."

*Paragraph 3.1.2.,* renumber and amendto read:

"3.1.3. The tyre-size designation;"

*Paragraphs 3.1.3. to 3.1.3.3.* renumber as paragraphs 3.1.4. to 3.1.4.3.

*Paragraphs 3.1.4. and 3.1.5.,* renumber and amendto read:

"3.1.5. An indication of the tyre's speed category symbol;

3.1.6. The load-capacity index;"

*Paragraphs 3.1.6. to 3.1.15.* renumber as paragraphs 3.1.7. to 3.1.16.

*Paragraphs 4.1. to 4.1.2.,* amendto read:

"4.1. The application for approval of a type of tyre with regard to this Regulation shall be submitted by the tyre manufacturer or by his duly accredited representative. It shall specify:

4.1.1. The tyre-size designation;

4.1.2. The manufacturer’s name;

4.1.2.1. The brand name(s)/trademark(s);

4.1.2.2. The trade description(s)/commercial name(s)."

*Paragraph 4.1.3.,* amendto read:

"4.1.3. The category of use (normal, snow, moped, all-terrain (AT),special);"

*Paragraph 4.1.8.,* amendto read:

"4.1.8. Whether the tyre is "standard" or "reinforced";"

*Paragraph 5.1.* replace "pneumatic tyre" by "tyre".

*Paragraph 5.2.,* amendto read:

"5.2. An approval number shall be assigned to each type approved. Its first two digits (at present 00) shall indicate the series of amendments incorporating the most recent major technical amendments made to the Regulation at the time of issue of the approval. The same Contracting Party shall not assign the same number to another tyre type covered by this Regulation."

*Paragraph 5.3.,* amendto read:

"5.3. Notice of approval or of extension or of refusal or withdrawal of approval or production definitively discontinued of a type of tyre pursuant to this Regulation shall be communicated to the Parties to the 1958 Agreement applying this Regulation, by means of a form conforming to the model in Annex 1 to this Regulation."

*Paragraphs, 5.4., 6.1.3., 6.2.1., 6.3.3.1., as well as in the title of paragraphs 7., 7.1., 7.1.1., 9.1 and 10.,* replace "pneumatic tyre"by"tyre".

*Paragraph 11.,* amendto read:

"11. Names and addresses of Technical Services responsible for conducting approval tests, of test laboratories and of Type Approval Authorities.

11.1. The Contracting Parties to the 1958 Agreement which apply this Regulation shall communicate to the United Nations Secretariat the names and addresses of the Technical Services responsible for conducting approval tests and, where applicable, of the approved test laboratories and of the Type Approval Authorities which grant approval and to which forms certifying approval, or extension of approval, or refusal of approval or withdrawal of approval or production definitively discontinued, issued in other countries, are to be sent.

11.2. The Contracting Parties to the 1958 Agreement which apply this Regulation may designate laboratories of tyre manufacturers as approved test laboratories.

11.3. Where a Contracting Party to the 1958 Agreement applies paragraph 11.2. above, it may, if it so desires, be represented at the tests by one or more persons of its choice."

*Annex 1*

"Communication

… of a type of tyre for motor cycles and mopeds pursuant to Regulation No. 75"

*Item 1.* amendto read:

"1. Manufacturer's name and address : "

*Item 2.* amend to read:

"2. Tyre type designation 3.

2.1. Brand name(s)/trademark(s):

2.2. Trade description(s)/commercial name(s):

 3 A list of brand name(s)/trademark(s) or trade description(s)/commercial name(s) may be annexed to this communication."

*Delete* *item 3.*

*Items 4. to 5.1. renumber as items 3. to 4.1.*

*Item 5.2.* renumber and amendto read:

"4.2. Category of use: normal/snow/moped/all terrain (AT)/special2"

*Items 5.3 to 14. renumber as items 4.3. to 13.*

*Annex 2,* amend to read:

"…

The above approval mark affixed to a tyre shows that the type of tyre concerned has been approved in the Netherlands (E 4) pursuant to Regulation No. 75 under approval number 022439.

…"

*Annex 3,* amend to read:

"…

These markings define a tyre:

…"

*Annex 6,* amend to read:

 "Method of measuring tyres…"

*Replace the table in paragraph 1. with:*

"

| *Tyre version* | *Speed category symbol* | *Inflation Pressure* |
| --- | --- | --- |
| *bar* | *kPa* |
| Standard | F, G, J, K, L, M, N, P, Q, R,S | 2.25 | 225 |
| T, U, H, V, W | 2.80 | 280 |
| Reinforced | F to P | 2.80 | 280 |
| Q, R, S, T, U, H, V, W | 3.30 | 330 |
| Motor cycle Derivatives1 | 4PR | F to M | 3.50 | 350 |
| 6PR | 4.00 | 400 |
| 8PR | 4.50 | 450 |
| Moped | Standard | B | 2.25 | 225 |
| Reinforced | 2.80 | 280 |
| All Terrain (AT) |  | all | 0.25 | 25 |
|  | all | 0.35 | 35 |
|  | all | 0.45 | 45 |

"

*Annex 7,*

*Paragraph 1.2.,* amend to read:

"1.2. Inflate the tyre to the appropriate pressure given in the following table:

Testing inflation pressure

|  |  |  |
| --- | --- | --- |
| *Tyre version* | *Speed Category symbol* | *Inflation pressure* |
| *bar* | *kPa* |
| Standard | F, G, J, K | 2.50 | 250 |
| L, M, N, P | 2.50 | 250 |
| Q, R, S | 3.00 | 300 |
| T, U, H, V | 3.50 | 350 |
| Reinforced | F, G, J, K, L, M, N, P | 3.30 | 330 |
| Q, R, S, T, U, H, V | 3.90 | 390 |
| Motor cycleDerivatives1 | 4PR | F, G, J, K, L, M | 3.70 | 370 |
| 6PR | 4.50 | 450 |
| 8PR | 5.20 | 520 |
| Moped | Standard | B | 2.50 | 250 |
| Reinforced | 3.00 | 300 |
| All Terrain (AT) |  | all | 0.25 | 25 |
|  | all | 0.35 | 35 |
|  | all | 0.45 | 45 |
| 1 From the date of entry into force of Supplement 8 to this Regulation no new approvals for these tyres should be issued pursuant to Regulation No. 75. These tyre sizes are now included in Regulation No. 106. |

 For speeds above 240 km/h, the test pressure is 3.20 bar (320 kPa).

 For other types of tyre, inflate to the pressure specified by the manufacturer."

*Annex 9,*

*Paragraph 3.4.1.,* amend to read:

"3.4.1. Road tyres in bias and bias-belted construction.

|  |  |  |
| --- | --- | --- |
| *Speed category symbol* | *Tyre version* | *Inflation pressure* |
|  |  | *bar* | *kPa* |
| P/Q/R/S | standard | 2.5 | 250 |
| T and above | standard | 2.9 | 290 |

"

1. \* In accordance with the programme of work of the Inland Transport Committee for 2016–2017 (ECE/TRANS/254, para. 159 and ECE/TRANS/2016/28/Add.1, cluster 3.1), the World Forum will develop, harmonize and update Regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)