Proposal for a Corrigendum to the to the 04 series of amendments to Regulation No. 46 (Devices for indirect vision)

The text reproduced below was prepared by the expert from Germany correcting an error in the text of Regulation No. 46 and updates a wrong reference. The modifications to the text of Regulation the 04 series of amendments to Regulation No. 46 are marked in bold for new characters and strikethrough for deleted characters.

**I. Proposal**

*Paragraph 6.3.3.2.,* correct to read:

"6.3.3.2. In case of mirrors, should the mounting of the mirror break during the tests described in paragraph 6.3.2. above for mirrors stuck to the windscreen, the part remaining shall not project beyond the base by more than 10 mm and the configuration remaining after the test shall satisfy the conditions laid down in paragraph ~~6.1.3.~~**6.1.1.3.** of this Regulation."

II. Justification

1. With Supplement 2 to the 04 series of amendments camera-monitor-systems were introduced as devices for indirect vision that can replace mirrors of classes I to IV. Due to that it was necessary to up-date a lot of references in the existing text of the regulation including the first reference in that paragraph and the numbering of the paragraph itself. In case of the second reverence in paragraph 6.3.3.2 it was done by mistake, as numbering and content of paragraph 6.1.1.3 has not been modified by Supplement 2 to the 04 series of amendments.

2. The aim of this corrigendum is to correct the text of the Regulation and to up-date the reference.