|  |  |  |  |
| --- | --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.29/2018/15 | |
| Description: _unlogo | **Economic and Social Council** | | Distr.: General  28 December 2017  Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**174th session**

Geneva, 13-16 March 2018

Item 4.8.1 of the provisional agenda

**1958 Agreement:  
Consideration of draft amendments**

**to existing UN Regulations submitted by GRSG**

Proposal for Supplement 7 to the 01 series of amendments to UN Regulation No. 43 (Safety glazing)

**Submitted by the Working Party on General Safety Provisions**[[1]](#footnote-2)\*

The text reproduced below was adopted by the Working Party on General Safety Provisions (GRSG) at its 113thsession (ECE/TRANS/WP.29/GRSG/92, para. 18). It is based on official document ECE/TRANS/WP.29/GRSG/2017/15 as reproduced in Annex II to the report. It is submitted to the World Forum for Harmonization of Vehicle Regulations (WP.29) and to the Administrative Committee AC.1 for consideration at their March 2018 sessions.

*Annex 21, Table 2,* amend to read:

"

| *Seat-back angle*  *(in °)* | *Horizontal  coordinates*  *X* | *Vertical  coordinates*  *Z* | *Seat-back angle*  *(in °)* | *Horizontal coordinates*  *X* | *Vertical coordinates*  *Z* |
| --- | --- | --- | --- | --- | --- |
| 5  6  7  8  9  10  11  12  13  14  15  16  17  18  19  20  21  22 | - 186 mm  - 177 mm  - 167 mm  - 157 mm  - 147 mm  - 137 mm  - 128 mm  - 118 mm  - 109 mm  - 99 mm  - 90 mm  - 81 mm  - 72 mm  - 62 mm  - 53 mm  - 44 mm  - 35 mm  - 26 mm | 28 mm  27 mm  27 mm  27 mm  26 mm  25 mm  24 mm  23 mm  22 mm  21 mm  20 mm  18 mm  17 mm  15 mm  13 mm  11 mm  9 mm  7 mm | 23  24  25  26  27  28  29  30  31  32  33  34  35  36  37  38  39  40 | - 18 mm  - 9 mm  0 mm  9 mm  17 mm  26 mm  34 mm  43 mm  51 mm  59 mm  67 mm  76 mm  84 mm  92 mm  100 mm  108 mm  115 mm  123 mm | 5 mm  3 mm  0 mm  - 3 mm  - 5 mm  - 8 mm  - 11 mm  - 14 mm  - 18 mm  - 21 mm  - 24 mm  - 28 mm  - 32 mm  - 35 mm  - 39 mm  - 43 mm  - 48 mm  - 52 mm |

**"**

1. \* In accordance with the programme of work of the Inland Transport Committee for 2016–2017 (ECE/TRANS/254, para. 159 and ECE/TRANS/2016/28/Add.1, cluster 3.1), the World Forum will develop, harmonize and update UN regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)