|  |  |
| --- | --- |
| Submitted by the expert from India | Informal document **GRSG-114-20**  (114th GRSG, 9 - 13 April 2018,  Agenda items 4(a) and 4(b)) |

**Comment on ECE/TRANS/WP.29/GRSG/2018/7, Proposal for Supplement 8 to the 01 series of amendments to UN Regulation No. 43 (Safety Glazing)**

Addition to existing text of ECE/TRANS/WP.29/GRSG/2018/7 is shown in bold italic and yellow highlighted text.

**A. Proposals**

1. *Paragraph 5.5.8.,* amend to read:

"5.5.8. XI In the case of a laminated-glass panes**. In addition, the appropriate application will be signified by:**

**/D For *laminated-glass* panes, which are subjected to the 2,260 g ball test and the headform test.**"

1. Document ECE/TRANS/WP.29/GRSG/2018/7 may also be considered for amendment to UN GTR No. 6 (Safety Glazing) after adoption of the document in GRSG.

**B. Justifications**

Ad.1 For proposal 1: Use of specific terminology.

Ad.2 For proposal 2: Provision of optional light weight *Laminated Glass panes* will be advantageous in UN GTR No. 6 as well.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_