|  |  |  |
| --- | --- | --- |
|  | **INF.9** | |
| **Economic Commission for Europe**  Inland Transport Committee  **Working Party on the Transport of Dangerous Goods**  **Joint Meeting of Experts on the Regulations annexed to the**  **European Agreement concerning the International Carriage**  **of Dangerous Goods by Inland Waterways (ADN)**  **Thirty-fourth session**  Geneva, 21-25 January 2019  Item 5 (b) of the provisional agenda  **Proposals for amendments to the Regulations annexed to ADN:**  **other proposals** | | 11 January 2019 |

UN 2057 – TRIPROPYLENE

Transmitted by the Recommended ADN Classification Societies

1. Two amendments to Table C (3.2.3.2) were introduced in ECE/ADN/45 (page 50/51):

|  |
| --- |
| 3.2.3.2 For UN No. 2057 **packing group II**:  *In column (5) Replace "3 +N3" by "3 + N1".*  *In column (6) Replace "N" by "C".*  *In column (8) Replace "3" by "2".*  *In column (13) Replace "3" by "2".* |
| *In* column *(5) Replace "3 +N3" by "3 + N1".*  *In column (6) Replace "N" by "C".*  *In column (8) Replace "3" by "2".*  *In column (13) Replace "3" by "2".* |
|  |

1. The substance has to be carried in a Type C vessel instead of a Type N; but according to 9.3.2.21.1a) the maximum degree of filling has to be 95 % instead of 97 % (type N); the Opening pressure of the high-velocity vent valve in kPa has perhaps also to be modified   
   (50(?) kPa instead of 10 kPa).
2. Consequently, two corrections would be foreseen:

* *In column (11) replace “97” by “95”*
* *In column (10) Replace "10" by "??".*

|  |
| --- |
| *3.2.3.2 For UN No. 2057* ***packing group III***: |
| *In column (5) Replace "3 +N3" by "3 + N1".*  *In column (6) Replace "N" by "C".*  *In column (7) Replace "3" by "2".*  *In column (8) Replace "3" by "2".*  *In column (13) Replace "3" by "2".* |
|  |

1. The substance has to be carried in a Type C vessel instead of a Type N; but according to 9.3.2.21.1a the maximum degree of filling has to be 95 % instead 97 % (type N); the Opening pressure of the high-velocity vent valve in kPa has perhaps also to be modified (50 (?) kPa instead of [--]).
2. Consequently, two corrections would be foreseen:

* *In column (11) Replace "97" by "95".*
* *In column (10) Replace "--" by "??".*