Supplement 1 to the 09 series of amendments to UN Regulation No. 14 (Safety-belt anchorages)

I. Proposal

*Annex 6, key to symbols 3*: amendto read:

"Annex 6

…

3: Two lower anchorages and one upper anchorage which allow the installation of a three-point safety-belt type A, or of safety-belts types Ar, Ar4m or Ar4Nm, where required by ~~the Consolidated Resolution on the Construction of Vehicles (R.E.3) Annex 13, Appendix 1~~ **UN Regulation No. 16, Annex XVI**."

II. Justification

This amendment is needed due to the transfer of provisions on Minimum number of anchorage points and location of lower anchorages from Consolidated Resolution on the Construction of Vehicles (R.E.3) to the UN Regulation No. 16