UNITED

NATIONS

Distr.

Economic and Social	GENERAL

Council	TRANS/WP.29/2001/36
11 April 2001

Original: ENGLISH

ECONOMIC COMMISSION FOR EUROPE

INLAND TRANSPORT COMMITTEE

World Forum for Harmonization of Vehicle Regulations (WP.29)

(One-hundred-and-twenty-fourth session,

26-29 June 2001, agenda item 4.2.9.)

PROPOSAL FOR DRAFT SUPPLEMENT 12

TO THE 02 SERIES OF AMENDMENTS TO REGULATION No. 30

(Pneumatic tyres)

Transmitted by the Working Party on Brakes and Running Gear (GRRF)

Note: The text reproduced below was adopted by GRRF at its forty-ninth session, and is transmitted for consideration to WP.29 and to AC.1. It is based on the text reproduced in the session report (TRANS/WP.29/GRRF/49, para. 64).

__________

This document is a working document circulated for discussion and comments. The use of this document for other purposes is the entire responsibility of the user. Documents are also available via the INTERNET:

http://www.unece.org/trans/main/welcwp29.htm

GE.01-

Insert new paragraphs 3.1.11. and 3.1.11.1., to read:

"3.1.11.	In the case of temporary use spare tyres, the words "TEMPORARY USE ONLY" in upper case characters at least 12.7 mm high.

3.1.11.1.	In addition, in the case of "T" type temporary use spare tyres, the legend "INFLATE TO 420 kPa (60 psi)" in upper and lower case characters as shown and at least 12.7 mm high."

Annex 7, paragraph 1.2., the table, add for "Speed category" "L, M and N" the value "2.4" in the column "Radial tyres Standard", and the value "2.8" in the column "Radial tyres Reinforced".

_________