UNITED

NATIONS

Distr.

GENERAL

TRANS/WP.29/656/Corr.1	16 February 1999

ENGLISH ONLY

INLAND TRANSPORT COMMITTEE

Working Party on the Construction of Vehicles

DRAFT SUPPLEMENT 2 TO REGULATION No. 67

(Equipment for liquefied petroleum gas)

Corrigendum 1

Note: The text reproduced below was prepared by the secretariat to correct editorial errors. Correction to paragraph 2.5.3.1. is based on document TRANS/WP.29/1998/63, correction to para. 6.14.8.2. on document TRANS/WP.29/1998/31 and correction to para. 6.14.8.2. on document TRANS/WP.29/1998/63, text of annex 3, para. 7.4.

__________

GE.99-

Insert paragraph 2.5.3.1., (new, English only), to read:

"2.5.3.1.	"Pressure relief device" means a device aimed to protect the container from burst which can occur in case of fire, by venting the LPG contained."

Paragraphs 5.4.1. and 16.4.1., footnote 1/, amend to read:

"...... 31 for Bosnia and Herzegovina, 32 for Latvia,

33-36 (vacant) ......."

Paragraph 6.14.8.2., correct the value of "2,500 ± 100 kPa" to read

"2,700 ± 100 kPa".

Paragraph 6.14.8.5., correct the value of "110 ± 10 C" to read "120 ± 10 C".

___________