UNITED

NATIONS

Distr.

Economic and Social	GENERAL

Council	TRANS/WP.29/713
13 April 2000

ENGLISH

Original: ENGLISH

and FRENCH

ECONOMIC COMMISSION FOR EUROPE

INLAND TRANSPORT COMMITTEE

World Forum for Harmonization of Vehicle Regulations (WP.29)

CORRIGENDUM 1 TO THE 01 SERIES OF AMENDMENTS TO REGULATION No. 21

(Interior fittings )

Note: The text reproduced below was adopted by the Administrative Committee (AC.1) of the amended 1958 Agreement at its fourteenth session, following the recommendation by WP.29 at its one-hundred-and-twentieth session. It is based on document TRANS/WP.29/2000/27 as modified (TRANS/WP.29/703, para. 181).

Paragraph 5.3.4.1., correct to read:

"5.3.4.1.	Components mounted on the roof, but which are not part of the roof structure, such as grab handles, lamps and sun visors, etc. shall have a radius of curvature not less than 3.2 mm. In addition, the width of the projecting parts shall not be less than the amount of their downward projection; alternatively these projecting parts shall pass the energy-dissipating test in accordance with the requirements of annex 4."

_____________

GE.00-