UNITED

NATIONS

Distr.

Economic and Social	GENERAL

Council	TRANS/WP.29/720
18 April 2000

ENGLISH

Original: ENGLISH

and FRENCH

ECONOMIC COMMISSION FOR EUROPE

INLAND TRANSPORT COMMITTEE

World Forum for Harmonization of Vehicle Regulations (WP.29)

DRAFT SUPPLEMENT 6	TO REGULATION No. 38

(Rear fog lamps)

Note: The text reproduced below was adopted by the Administrative Committee (AC.1) of the amended 1958 Agreement at its fourteenth session, following the recommendation by WP.29 at its one-hundred-and-twentieth session. It is based on document TRANS/WP.29/2000/12, not amended TRANS/WP.29/703, para. 165).

__________

GE.00-

Paragraph 9., amend to read (footnote */ not modified)

"9.	COLOUR OF LIGHT EMITTED

The colour of the light emitted inside the field of the light distribution grid defined at paragraph 3 of annex 3, which shall be measured by using a source of light at a colour temperature of

2856 K, */ must lie within the limits of the following trichromatic

co-ordinates:

limit towards yellow: y ≤ 0.335

limit towards purple: z ≤ 0.008

Outside this field no sharp variation of colour shall be observed.

However, for lamps equipped ....."

___________