UNITED

NATIONS

Distr.

Economic and Social	GENERAL

Council	TRANS/WP.29/729
5 May 2000

ENGLISH

Original: ENGLISH and

FRENCH

ECONOMIC COMMISSION FOR EUROPE

INLAND TRANSPORT COMMITTEE

World Forum for Harmonization of Vehicle Regulations (WP.29)

DRAFT SUPPLEMENT 2	TO THE 01 SERIES OF AMENDMENTS TO REGULATION No. 80

(Strength of seats and their anchorages)

Note: The text reproduced below was adopted by the Administrative Committee (AC.1) of the amended 1958 Agreement at its fourteenth session, following the recommendation by WP.29 at its one-hundred-and-twentieth session. It is based on document TRANS/WP.29/2000/30, not amended (TRANS/WP.29/703, para. 184).

__________

Paragraph 2.21., amend to read:

"2.21.	"Reference zone" means the space between two vertical longitudinal planes, 400 mm apart and symmetrical with respect to the H-point, and defined by rotation from vertical to horizontal of the headform apparatus, described in Regulation No. 21, annex 1. The apparatus shall be positioned as described in that annex of Regulation No. 21 and set to its maximum length of 840 mm and its minimum length of 736 mm for residual limitation of said space."

__________

GE.00-