UNITED

NATIONS

Distr.

Economic and Social	GENERAL

Council	TRANS/WP.29/753
12 December 2000

ENGLISH

Original: ENGLISH

and FRENCH

ECONOMIC COMMISSION FOR EUROPE

INLAND TRANSPORT COMMITTEE

World Forum for Harmonization of Vehicle Regulations (WP.29)

CORRIGENDUM 1 TO SUPPLEMENT 1 TO THE 01 SERIES OF AMENDMENTS

TO REGULATION No. 53

(Installation of lighting and light-signalling devices

for category L3 vehicles)

Note: The text reproduced below was adopted by the Administrative Committee (AC.1) of the amended 1958 Agreement at its sixteenth session, following the recommendation by WP.29 at its one-hundred-and-twenty-second session. It is based on document TRANS/WP.29/2000/43, not amended (TRANS/WP.29/743, para. 157).

__________

Paragraph 6.1.3.3., correct to read:

"..... of the passing lamp must not exceed 200 mm. The distance between the edge of the illuminating surface of any independent driving lamp and the ground must be from 500 mm to 1,300 mm."

__________

GE.00-