**Economic Commission for Europe**

Inland Transport Committee

**Working Party on the Transport of Dangerous Goods**

**107th session 6 November 2019**

Geneva, 11-15 November 2019

Item 8 of the provisional agenda

**Any other business**

**Draft corrigendum to ECE/TRANS/275 (ADR 2019)**

**Note by the secretariat**

**Introduction**

The Working Party may wish to note the following corrections to ADR. These are corrections to the publication only (correct in the notified texts) or which do not concern the French version (authentic text of the ADR). These corrections will be published in corrigenda after the meeting.

**Corrections to the English version**

Chapter 2.2, 2.2.51.1.5

*For* 2.2.51.1.9 *read* 2.2.51.1.10

Chapter 2.2, 2.2.9.3, in the list of entries, for M11, for UN 3359

*For* FUMIGATED UNIT *read* FUMIGATED TRANSPORT UNIT

*[also applies to the Russian version]*

Chapter 2.3, at the end of footnote 1

*Delete* and No. L 143 of 03.06.2008, p.55

Chapter 3.2, table A, for UN No 1744, in Column (10)

*Delete* TU43

Chapter 4.1, 4.1.4.1, packing instruction P502, under Single packagings / Composite packagings / glass receptacle with outer steel, aluminium, fibre or plywood drum

*For* 6PD1 or 6PG1 *read* 6PG1 or 6PD1

Chapter 4.1, 4.1.4.1, packing instruction P504, under Single packagings / Composite packagings / glass receptacle with outer steel, aluminium, fibre or plywood drum

*For* 6PD1 or 6PG1 *read* 6PG1 or 6PD1

Chapter 4.3, 4.3.4.1.3, in the Table, under Class 8, for UN No. 1790, in column "Name and description"

*For* Hydrofluoric acid, solution, with more than 85% hydrofluoric acid *read* Hydrofluoric acid with more than 85% hydrogen fluoride

Chapter 5.3, 5.3.2.1.8

*For* Orange-coloured plates which does *read* Orange-coloured plates which do

Chapter 5.3, 5.3.3

*For* Where dimensions are not specified, all features shall be in approximate proportion to those shown. For tank-containers or portable tanks with a capacity of not more than 3 000 litres and with an available surface area insufficient to affix the prescribed marks, the minimum dimensions of the sides may be reduced to 100 mm.

*read* For tank-containers or portable tanks with a capacity of not more than 3 000 litres and with an available surface area insufficient to affix the prescribed marks, the minimum dimensions of the sides may be reduced to 100 mm. Where dimensions are not specified, all features shall be in approximate proportion to those shown.

**Corrections à la version française**

Chapitre 3.2, tableau A, titre de la colonne (10)

*Substituer* au texte existant

Instructions

Chapitre 3.2, tableau A, pour le No ONU 1744, dans la colonne (10)

*Supprimer* TU43

Chapitre 3.2, tableau A, pour le No ONU 2071, dans la colonne (5)

*Supprimer* 193

Chapitre 3.2, tableau A, pour le No ONU 2071, dans la colonne (6)

*Insérer* 193

Chapitre 3.2, tableau A, pour le No ONU 3459, dans la colonne (2)

*Au lieu de* ITROBROMOBENZENES *lire* NITROBROMOBENZENES

Chapitre 3.2, tableau A, pour le No ONU 3498, dans la colonne (3b)

*Au lieu de* 8 *lire* C1

Chapitre 3.3, disposition spéciale 583, dans le tableau, dans le titre de la dernière colonne, après « Nom technique »

*Ajouter* un appel à la note de bas de tableau a.

Chapitre 5.3, 5.3.2.3.2, numéro d’identification du danger X83

*Au lieu de* présentant un degré mineur de corrosivité *lire* faiblement corrosive

Chapitre 6.2, 6.2.4.1, tableau, sous « Pour la conception et la fabrication », pour la norme « EN 1251-2:2000 », dans le Nota

*Au lieu de* La norme EN 1252-1:1998 à laquelle il est fait référence dans cette norme est également applicable

*lire* Les normes EN 1252-1:1998 et EN 1626 auxquelles il est fait référence dans cette norme sont également applicables

Chapitre 6.8, 6.8.3.4, dans le titre avant 6.8.3.4.10, à la fin

*Ajouter* réfrigérés