E/ECE/324

Rev.1/Add.23/Rev.2/Amend.1

E/ECE/TRANS/505

18 July 2001

AGREEMENT

CONCERNING THE ADOPTION OF UNIFORM TECHNICAL PRESCRIPTIONS

FOR WHEELED VEHICLES, EQUIPMENT AND PARTS WHICH CAN BE FITTED AND/OR

BE USED ON WHEELED VEHICLES AND THE CONDITIONS FOR RECIPROCAL RECOGNITION

OF APPROVALS GRANTED ON THE BASIS OF THESE PRESCRIPTIONS */

(Revision 2, including the amendments entered into force on 16 October 1995)

__________

Addendum 23: Regulation No. 24

Revision 2 - Amendment 1

Supplement 1 to the 03 series of amendments - Date of entry into force: 27 March 2001

UNIFORM PROVISIONS CONCERNING:

I:	THE APPROVAL OF COMPRESSION IGNITION (C.I.) ENGINES WITH REGARD TO THE EMISSION OF VISIBLE POLLUTANTS

II:	THE APPROVAL OF MOTOR VEHICLES WITH REGARD TO THE INSTALLATION OF C.I. ENGINES OF AN APPROVED TYPE

III:	THE APPROVAL OF MOTOR VEHICLES EQUIPPED WITH C.I. ENGINES WITH REGARD TO THE EMISSION OF VISIBLE POLLUTANTS BY THE ENGINE

IV:	THE MEASUREMENT OF POWER OF C.I. ENGINE

__________

UNITED NATIONS

Paragraph 5.4.1., footnote 1/, amend to read:

"1/	1 for Germany, 2 for France, 3 for Italy, 4 for the Netherlands, 5 for Sweden, 6 for Belgium, 7 for Hungary, 8 for the Czech Republic, 9 for Spain, 10 for Yugoslavia, 11 for the United Kingdom, 12 for Austria, 13 for Luxembourg, 14 for Switzerland, 15 (vacant), 16 for Norway, 17 for Finland, 18 for Denmark, 19 for Romania, 20 for Poland, 21 for Portugal, 22 for the Russian Federation, 23 for Greece, 24 for Ireland, 25 for Croatia, 26 for Slovenia, 27 for Slovakia, 28 for Belarus, 29 for Estonia, 30 (vacant), 31 for Bosnia and Herzegovina, 32 for Latvia, 33 (vacant), 34 for Bulgaria,

35-36 (vacant), 37 for Turkey, 38-39 (vacant), 40 for The former Yugoslav Republic of Macedonia, 41 (vacant), 42 for the European Community (Approvals are granted by its Member States using their respective ECE symbol), 43 for Japan, 44 (vacant), 45 for Australia, 46 for Ukraine and 47 for South Africa. Subsequent numbers shall be assigned to other countries in the chronological order in which they ratify or accede to the Agreement Concerning the Adoption of Uniform Technical Prescriptions for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these Prescriptions, and the numbers thus assigned shall be communicated by the Secretary-General of the United Nations to the Contracting Parties to the Agreement."

Annex 8, paragraph 3.3., amend to read:

"3.3.	Light source

The light source shall be an incandescent lamp with a colour temperature in the range of 2800 to 3250 K or a green light- emitting diode (LED) with a spectral peak between 550 and 570 nm. The light source shall be protected against sooting by means that do not influence the optical path length beyond the manufacturer's specifications."

____________