|  |  |  |  |
| --- | --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.29/2021/56 | |
| _unlogo | |  | | --- | | Informal Document GRPE-82-10  This Informal Document has been prepared to provide GRPE with details of the changes to the original version of UN Regulation No. 154 which have been included in the Working Document submitted to the 183rd WP.29 (ECE/TRANS/WP.29/2021/56). That document shows the final text proposal, whereas this Informal Document shows the changes made through the use of tracked changes. It is for reference purposes only. |   **Economic and Social Council** | | Distr.: General  22 December 2020  Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**183rd session**

Geneva, 9-11 March 2021

Item 4.11. of the provisional agenda

**1958 Agreement:  
Consideration of additional proposals for amendments to existing   
UN Regulations submitted by the Working Parties subsidiary   
to the World Forum, if any**

Proposal for Supplement 1 to the original version of UN Regulation No. 154

Submitted by the representatives of the European Commission and Japan [[1]](#footnote-2)\*, [[2]](#footnote-3)\*\*

The text reproduced below is a proposal for Supplement 1 to the original version of UN Regulation No 154 on uniform provisions concerning the approval of light duty passenger and commercial vehicles with regards to criteria emissions, emissions of carbon dioxide and fuel consumption and/or the measurement of electric energy consumption and electric range (WLTP). It corrects errors and clarifies provisions based on requirements introduced in the Amendment 6 to UN GTR No. 15. This document is subject to review by GRPE during its January 2021 session. This document is submitted to the World Forum for Harmonization of Vehicle Regulations (WP.29) and its Administrative Committee for the 1958 Agreement (AC.1) for consideration and vote at their March 2021 sessions.

*Paragraph 2.1.,* amend to read:

|  |  |
| --- | --- |
| "… |  |
| SSV | Subsonic venturi |
| UBE | Usable Battery (REESS) Energy |
| USFM | Ultrasonic flow meter |
| VH | Vehicle High |
| VL | Vehicle Low |
| VPR | Volatile particle remover |
| …" |  |

*Paragraph 4.1.2.(a),* amend to read:

"(a) In the case of vehicles equipped with positive ignition engines, a declaration by the manufacturer of the minimum percentage of misfires out of a total number of firing events that would either result in emissions exceeding the OBD thresholds given in paragraph 6.8.2., if that percentage of misfire had been present from the start of a Type 1 test as described in Annexes Part B to this Regulation, or that could lead to an exhaust catalyst, or catalysts, overheating prior to causing irreversible damage;"

*Paragraph 5.2.2.,* amend to read:

"5.2.2. Example of an Approval Number to this Regulation:

E11\*[XXX]R01/01/02\*0123\*01

The first extension of the Approval numbered 0123, issued by the United Kingdom to Series of Amendments 01, Supplement 01, which is a Level 2 Approval."

*Paragraph 5.10.4.,* amend to read:

"5.10.4. When tested with a defective component in accordance with Appendix 1 to Annex C5 to this Regulation, the OBD system malfunction indicator shall be activated. The OBD system malfunction indicator may also activate during this test at levels of emissions below the OBD thresholds specified in paragraph 6.8."

*Paragraph 6.3.2.2.(b),* amend to read:

"(b) Type of traction REESS (type of cell, capacity, nominal voltage, nominal power, type of coolant (air, liquid));"

*Paragraph 6.3.2.3.(b),* amend to read:

"(b) Type of traction REESS (type of cell, capacity, nominal voltage, nominal power, type of coolant (air, liquid));"

*Paragraph 6.3.2.4.(c),* amend to read:

"(c) Type of traction REESS (type of cell, capacity, nominal voltage, nominal power, type of coolant (air, liquid));"

*Add a new paragraph 6.3.11.,* to read:

"6.3.11. For Level 1A only

KCO2 correction factor family for OVC-HEVs and NOVC-HEVs

It is allowed to merge two or more interpolation families into the same KCO2 correction factor family at which KCO2 shall be determined with vehicle H of one of the included interpolation families. The interpolation family that is used for the vehicle H selection shall be agreed by the responsible authority.

At the request of the responsible authority, the manufacturer shall provide evidence on the justification and technical criteria for merging these interpolation families for example in the following cases:

Two or more interpolation families are merged:

(a) Which were split because the maximum interpolation range of 20 g/km CO2 is exceeded (in case vehicle M measured: 30g/km);

(b) Which were split due to different engine power ratings of the same physical combustion engine  
(different power only related to software);

(c) Which were split because the n/v ratios are just outside the tolerance of 8%;

(d) Which were split, but still fulfil all the family criteria of a single IP family;

(e) Which were split because there is different number of powered axles.

Different electric energy converters between recharge-plug-in and traction REESS shall not be considered as a criterion in the context of the correction factor family."

*Paragraph 6.8.2., Table 4A, note 1,* amend to read:

"1 Positive ignition particulate mass OBD thresholds apply only to vehicles with direct injection engines"

*Paragraph 8.2.3.2., Figure 8/1,* amend to read:

"Figure 8/1

**Flowchart of the CoP test procedure for the Type 1 test**

Test of three vehicles

Computation of test statistic in accordance with Appendix 2

Test another vehicle, up to a maximum sample as specified

CoP family is rejected

CoP family is accepted

YES

YES

NO

Is a pass decision reached for all criteria emission, CO2 emission, fuel efficiency and/or electric energy consumption where applicable and in accordance with Table 8/1?

NO

YES

Evaluation of the test statistic shall be omitted for those criteria emission, CO2 emission, fuel efficiency and/or electric energy consumption, where applicable and in accordance with Table A8/1, for which a pass decision is reached

NO

Does the test statistic of Appendix 2 agree with the criteria for passing the family for any criteria emission, CO2 emission, fuel efficiency and/or electric energy consumption, where applicable and in accordance with Table 8/1?

Does the test statistic of Appendix 2 agree with the criteria for failing the family for any criteria emission, CO2 emission, fuel efficiency and/or electric energy consumption, where applicable and in accordance with Table 8/1?

"

*Paragraph 12.2.,* amend to read:

"12.2. This paragraph is only applicable for Level 1A

For Approvals to Level 1A only, until 1 September 2022 in the case of category M and category N1 class I vehicles, and 1 September 2023 in the case of category N1 class II and III and category N2 vehicles, Contracting Parties may accept Type Approvals to EU legislation as evidence of compliance with the provisions of this Regulation as detailed in (a) to (d) below:

(a) Type 1/I tests performed in accordance with Annex 4a to UN Regulation No 83, 07 series of amendments before 1 September 2017 in the case of category M and category N1 class I vehicles, and 1 September 2018 in the case of category N1 class II and III and category N2 vehicles shall be accepted by the approval authority for the purposes of producing deteriorated or defective components to simulate failures for assessing the requirements of Annex C5 to this Regulation;

(b) With respect to vehicles of a WLTP interpolation family which fulfil the extension rules specified in paragraph 2 of Annex 13 of UN Regulation No. 83, 07 series of amendments, procedures performed in accordance with Section 3 of Annex 13 to UN Regulation No. 83,.07 series of amendments before 1 September 2017 in the case of category M and category N1 class I vehicles, and 1 September 2018 in the case of category N1 class II and III and category N2 vehicles shall be accepted by the approval authority for the purposes of fulfilling the requirements of Appendix 1 to Annex B6 of this Regulation;

(c) Durability demonstrations where the first type 1/I test was performed and completed in accordance with Annex 9 to UN Regulation No. 83, 07 series of amendments before 1 September 2017 in the case of category M and category N1 class I vehicles, and 1 September 2018 in the case of category N1 class II and III and category N2 vehicles shall be accepted by the approval authorities for the purposes of fulfilling the requirements of Annex C4 to this Regulation.

(d) Evaporative emissions tests conducted on the basis of the test procedure set out in Annex VI of Regulation (EC) No 692/2008 as amended by Regulation (EC) No 2016/646 which were used to approve evaporative emissions families in the European Union before 31 August 2019 shall be accepted by the approval authorities for the purposes of fulfilling the requirements of Annex C3 to this Regulation."

*Appendix 1*

*Paragraph 2.3.1.,* amend to read:

"2.3.1. CO2 mass emission values for CoP / Fuel efficiency values for CoP

For Level 1A:

In the case the interpolation method is not applied, the CO2 mass emission value according to step 7 of Table A7/1 of Annex B7 shall be used for verifying the conformity of production.

In the case the interpolation method is applied, the CO2 mass emission value MCO2,c,ind for the individual vehicle according to step 10 of Table A7/1 of Annex B7 shall be used for verifying the conformity of production.

For Level 1B:

In the case the interpolation method is not applied, the fuel efficiency value FEc,8 according to step 8 of Table A7/1 of Annex B7 shall be used for verifying the conformity of production.

In the case the interpolation method is applied, the fuel efficiency value FEc,ind for the individual vehicle according to step 10 of Table A7/1 of Annex B7 shall be used for verifying the conformity of production."

*Appendix 3*

*Paragraph 1.9.,* amend to read:

"1.9. …

In the case that multiple vehicles have been tested, the CRI shall be calculated for each vehicle, and the resulting values shall be averaged. The manufacturer will provide statistical evidence to the responsible authority that the fit is sufficiently statistically justified."

*Appendix 6*

*Paragraph 6.2.,* amend to read:

"6.2. The manufacturer shall demonstrate that use of the sensors referred to in paragraph 6.1. and any other sensors on the vehicle, results in the activation of the driver warning system as referred to in paragraph 3., the display of a message indicating an appropriate warning (e.g. “emissions too high — check urea”, “emissions too high — check AdBlue”, “emissions too high — check reagent”), and the activation of the driver inducement system as referred to in paragraph 8.3., when the situations referred to in paragraphs 4.2., 5.4., or 5.5. occur.

For the purposes of this paragraph these situations are presumed to occur if the applicable NOx OBD threshold set out in Table 4 of paragraph 6.8.2. is exceeded.

NOx emissions during the test to demonstrate compliance with these requirements shall be no more than 20 per cent higher than the OBD thresholds."

*Paragraphs 8.6. to 8.8.,* amend to read:

"8.6. Detailed written information fully describing the functional operation characteristics of the driver inducement system shall be provided to the Type Approval Authority at the time of approval.

8.7. As part of the application for type approval under this Regulation, the manufacturer shall demonstrate the operation of the driver warning and inducement systems."

*Annexes Part A*

*Annex A2 Addendum*

*Paragraph 2.5.3.8.,* amend to read:

"2.5.3.8. Electric energy consumption

2.5.3.8.1. Electric Energy Consumption EC

|  |  |
| --- | --- |
| EAC(Wh) |  |

…"

*Annexes Part B*

*Annex B2*

*Add new paragraph 6.,* to read:

"6. Calculation tools

Examples of gear shift calculating tools can be found in the same webpage as this Regulation.[[3]](#footnote-4)

The following tools are provided:

(a) ACCESS based tool,

(b) Matlab code tool

(c) NET core tool

These tools were validated by the comparison of calculation results between the ACCESS tool, the Matlab code and the .NET core code for 115 different vehicle configurations supplemented by additional calculations for 7 of them with additional options like "apply speed cap", "suppress downscaling", "choose other vehicle class cycle" and "choose individual nmin\_drive values".

The 115 vehicle configurations cover extreme technical designs for transmission and engines and all vehicle classes.

All three tools deliver identical results with respect to gear use and clutch operation and although only the text in Annexes B1 and B2 is legally binding the tools have achieved a status that qualifies them as reference tools."

*Annex B4*

*Paragraph 4.2.2.1., Table A4/2,* amend to read:

"Table A4/2

**Energy efficiency classes according to rolling resistance coefficients (RRC) for C1, C2 and C3 tyres and the RRC values to be used for those energy efficiency classes in the interpolation, kg/tonne**

| *Energy efficiency class* | *Range of RRC for C1 tyres* | *Range of RRC for C2 tyres* | *Range of RRC for C3 tyres* |
| --- | --- | --- | --- |
| 1 | RRC ≤ 6.5 | RRC ≤ 5.5 | RRC ≤ 4.0 |
| 2 | 6.5 < RRC ≤ 7.7 | 5.5 < RRC ≤ 6.7 | 4.0 < RRC ≤ 5.0 |
| 3 | 7.7 < RRC ≤ 9.0 | 6.7 < RRC ≤ 8.0 | 5.0 < RRC ≤ 6.0 |
| 4 | 9.0 < RRC ≤ 10.5 | 8.0 < RRC ≤ 9.2 | 6.0 < RRC ≤ 7.0 |
| 5 | 10.5 < RRC ≤ 12.0 | 9.2 < RRC ≤ 10.5 | 7.0 < RRC ≤ 8.0 |
| 6 | RRC > 12.0 | RRC > 10.5 | RRC > 8.0 |
| *Energy efficiency class* | *Value of RRC to be used for interpolation for C1 tyres* | *Value of RRC to be used for interpolation for C2 tyres* | *Value of RRC to be used for interpolation for C3 tyres* |
| 1 | RRC = 5.9\* | RRC = 4.9\* | RRC = 3.5\* |
| 2 | RRC = 7.1 | RRC = 6.1 | RRC = 4.5 |
| 3 | RRC = 8.4 | RRC = 7.4 | RRC = 5.5 |
| 4 | RRC = 9.8 | RRC = 8.6 | RRC = 6.5 |
| 5 | RRC = 11.3 | RRC = 9.9 | RRC = 7.5 |
| 6 | RRC = 12.9 | RRC = 11.2 | RRC = 8.5 |

\* For Level 1A only: In case the actual RRC value is lower than this value, the actual rolling resistance value of the tyre or any higher value up to the RRC value indicated here shall be used for interpolation.

"

*Paragraph 4.5.5.2.1.,* amend to read:

"4.5.5.2.1. Correction to reference conditions

where:

…"

*Annex B6*

*Paragraph 1.2.3.9., Table A6/1 column headings,* amend to read:

"

| *Powertrain* | *Level 1A only*  *MCO2 (b)*  *(g/km)* | *Level 1A:*  *FC*  *(kg/100 km)* | *Level 1B;*  *FE (km/l or km/kg)* | *Electric energy consumption(c)*  *(Wh/km)* | *All electric range /  Pure Electric Range (c)*  *(km)* |
| --- | --- | --- | --- | --- | --- |

…"

*Paragraph 2.3.2.4.,* amend to read:

"2.3.2.4. Vehicle M is a vehicle within the interpolation family between the vehicles L and H with a cycle energy demand which is preferably closest to the average of vehicles L and H.

The limits of the selection of vehicle M (see Figure A6/4) are such that neither the difference in CO2 emission values between vehicles H and M nor the difference in CO2 emission values between vehicles M and L is greater than the allowed CO2 range in accordance with paragraph 2.3.2.2. of this annex. The defined road load coefficients and the defined test mass shall be recorded.

Figure A6/4

**Limits for the selection of vehicle M**



For Level 1A

The linearity of the corrected measured and averaged CO2 mass emission for vehicle M, MCO2,c,6,M according to step 6 of Table A7/1 of Annex B7, shall be verified against the linearly interpolated CO2 mass emission between vehicles L and H over the applicable cycle by using the corrected measured  and averaged CO2 mass emission MCO2,c,6,H of vehicle H and MCO2,c,6,L of vehicle L, according to step 6 of Table A7/1 of Annex B7, for the linear CO2 mass emission interpolation.

For Level 1B

An additional averaging of tests using the CO2-output of step 4a is necessary (not described in Table A7/1). The linearity of the corrected measured and averaged CO2 mass emission for vehicle M, MCO2,c,4a,M according to step 4a of Table A7/1 of Annex B7, shall be verified against the linearly interpolated CO2 mass emission between vehicles L and H over the applicable cycle by using the corrected measured  and averaged CO2 mass emission MCO2,c,4a,H values of vehicle H and MCO2,c,4a,L of vehicle L, according to step 4a used in of Table A7/1 of Annex B7, for the linear CO2 mass emission interpolation.

For Level 1A and Level 1B

The linearity criterion for vehicle M (see Figure A6/5) shall be considered fulfilled, if the CO2 mass emission of the vehicle M over the applicable WLTC minus the CO2 mass emission derived by interpolation is less than 2 g/km or 3 per cent of the interpolated value, whichever value is lower, but at least 1 g/km.

Figure A6/5

…"

*Paragraph 2.8.1.,* amend to read:

"2.8.1. The test cell temperature at the start of the test shall be within ±3 °C of the set point of 23 °C. The engine oil temperature and coolant temperature, if any, shall be within ±2 °C of the set point of 23 °C."

*Paragraph 3.4.1.,* amend to read:

"3.4.1. ...

is the fuel energy according to the following equation:

Where

…"

*Table A6.App2/3*, amend to read:

"Table A6.App2/3

**Willans factors (as applicable)**

|  | | | *Naturally aspirated* | *Pressure-charged* |
| --- | --- | --- | --- | --- |
| Positive ignition | Petrol (E0) | l/MJ | 0.0733 | 0.0778 |
| gCO2/MJ | 175 | 186 |
| Petrol (E10) | l/MJ | 0.0756 | 0.0803 |
| gCO2/MJ | 174 | 184 |
| CNG (G20) | m³/MJ | 0.0719 | 0.0764 |
| gCO2/MJ | 129 | 137 |
| LPG | l/MJ | 0.0950 | 0.101 |
| gCO2/MJ | 155 | 164 |
| E85 | l/MJ | 0.102 | 0.108 |
| gCO2/MJ | 169 | 179 |
| Compression ignition | Diesel (B0) | l/MJ | 0.0611 | 0.0611 |
| gCO2/MJ | 161 | 161 |
| Diesel (B7) | l/MJ | 0.0611 | 0.0611 |
| gCO2/MJ | 161 | 161 |

"

*Annex B7*

*Paragraph 1.4., Table A7/1, Step Nos. 4a to 4b,* amend to read:

"

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4a | Output step 2  Output step 3 | Mi,c,2, g/km;  MCO2,c,3, g/km. | Emissions test procedure for all vehicles equipped with periodically regenerating systems, Ki.  Annex B6, Appendix 1.  Mi,c,4a = Ki × Mi,c,2  or  Mi,c,4a = Ki + Mi,c,2  and  MCO2,c,4a = KCO2 × MCO2,c,3  or  MCO2,c,4a = KCO2 + MCO2,c,3  Additive offset or multiplicative factor to be used according to Ki determination.  If Ki is not applicable:  Mi,c,4a = Mi,c,2  MCO2,c,4a = MCO2,c,3 | Mi,c,4a, g/km;  MCO2,c,4a, g/km. |
| 4b | Output step 3  Output step 4a | MCO2,p,3, g/km;  MCO2,c,3, g/km;  MCO2,c,4a, g/km. | If Ki is applicable, align CO2 phase values to the combined cycle value:  for every cycle phase p;  where:  If Ki is not applicable:  MCO2,p,4 = MCO2,p,3 | MCO2,p,4, g/km. |

"

*Paragraph 1.4., Table A7/1, Step No. 6,* amend to read:

"

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6 | For Level 1A  Output step 5 | For every test:  Mi,c,5, g/km;  MCO2,c,5, g/km;  MCO2,p,5, g/km. | Averaging of tests and declared value.  Paragraphs 1.2. to 1.2.3. inclusive of Annex B6. | Mi,c,6, g/km;  MCO2,c,6, g/km;  MCO2,p,6, g/km.  MCO2,c,declared, g/km. |
| For Level 1B  Output step 5 | FEc,5, km/l; | Averaging of tests and declared value.  Paragraphs 1.2. to 1.2.3. inclusive of Annex B6.  The conversion from FEc,declared to MCO2,c,declared shall be performed for the applicable cycle according to paragraph 6. of Annex B7. For that purpose, the criteria emission over the applicable cycle shall be used. | FEc,declared, km/l  FEc,6, km/l  MCO2,c,declared, g/km. |

"

*Paragraph 1.4., Table A7/1, Step No. 9,* amend to read:

"

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 9  Interpolation family result.  For Level 1A  Final criteria emission result | Output step 8 | For each of the test vehicles H and L:  Mi,c,8, g/km;  MCO2,c,8, g/km;  MCO2,p,8, g/km;  FCc,8, l/100 km;  FCp,8, l/100 km;  FEc,8, km/l.  FEp,8, km/l | For Level 1A;  If in addition to a test vehicle H a test vehicle L and, if applicable vehicle M was also tested, the resulting criteria emission value shall be the highest of the two or, if applicable, three values and referred to as Mi,c.  In the case of the combined THC + NOx emissions, the highest value of the sum referring to either the vehicle H or vehicle L or, if applicable, vehicle M is to be taken as the type approval value.  Otherwise, if no vehicle L was tested,  Mi,c = Mi,c,8  Level 1A and Level 1B  For CO2, FE and FC, the values derived in step 8 shall be used, and CO2 values shall be rounded according to paragraph 6.1.8. of this Regulation to two places of decimal, and FE and FC values shall be rounded according to paragraph 6.1.8. of this Regulation to three places of decimal. | Mi,c, g/km;  MCO2,c,H, g/km;  MCO2,p,H, g/km;  FCc,H, l/100 km;  FCp,H, l/100 km;  FEc,H, km/l;  FEp,H, km/l;  and if a vehicle L was tested:  MCO2,c,L, g/km;  MCO2,p,L, g/km;  FCc,L, l/100 km;  FCp,L, l/100 km;  FEc,L, km/l;  FEp,L, km/l. |

"

*Annex B8*

*Paragraph 3.1.2.,* amend to read:

"3.1.2. Forced cooling as described in paragraph 2.7.2. of Annex B6 is only permitted for the charge-sustaining Type 1 test for OVC-HEVs according to paragraph 3.2. of this annex and for testing NOVC-HEVs according to paragraph 3.3. of this annex."

*Paragraph 3.4.4.2.1.,* amend to read:

"3.4.4.2.1. Speed trace

The shortened Type 1 test procedure consists of two dynamic segments ( and ) combined with two constant speed segments ( and ) as shown in Figure A8/2.

Figure A8/2

**Shortened Type 1 test procedure speed trace**



"

*Paragraph 4.1.1.1., Table A8/5, Step Nos. 4b to 8* amend to read:

*"*

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4b | Output step 3 | , g/km; , g/km; | If Ki is applicable, align CO2 phase values to combined cycle value:  for every cycle phase p;  where:  If Ki is not applicable: | , g/km. |
| Output step 4a | , g/km. |
| 4c | Output step 4a | Mi,CS,c,4a, g/km;  MCO2,CS,c,4a, g/km. | In the case these values are used for the purpose of conformity of production, the criteria emission values and CO2 mass emission values shall be multiplied with the run-in factor RI determined according to paragraph 8.2.4. of this Regulation:  Mi,CS,c4c = RIC (j) × Mi,CS,c,4a  MCO2,CS,c,4c = RICO2 (j) x MCO2,CS,c,4a  In the case these values are not used for the purpose of conformity of production:  Mi,c,4c = Mi,c,4a  MCO2,c,4c = MCO2,c,4a | Mi,CS,c,4c;  MCO2,CS,c,4c |
| Calculate fuel efficiency (FEc,4c\_temp) according to paragraph 6.14.1. of Annex B7.  In the case this value is used for the purpose of conformity of production, the fuel efficiency value shall be multiplied with the run in factor determined according to paragraph 8.2.4. of this Regulation:  FEc,4c = RIFE (j) x FEc,4c\_temp  In the case these values are not used for the purpose of conformity of production:  FEc,4c = FEc,4c\_temp | FEc,4c, km/l; |
| 5  Result of a single test. | Output step 4b and 4c | , g/km; , g/km; | For Level 1A:  ATCT correction of MCO2,CS,c,4c and MCO2,CS,p,4 in accordance with paragraph 3.8.2. of Annex B6a.  For Level 1B:  MCO2,c,5 = MCO2,c,4c  MCO2,p,5 = MCO2,p,4 | , g/km;, g/km. |
| , g/km;FEc,4c, km/l; | Apply deterioration factors calculated in accordance with Annex C4 to the criteria emissions values.  In the case these values are used for the purpose of conformity of production, the further steps (6 to 9) are not required and the output of this step is the final result. | , g/km;  FEc,5, km/l; |
| 6  results of a Type 1 test for a test vehicle. | For Level 1A Output step 5 | For every test: , g/km;, g/km;, g/km. | Averaging of tests and declared value according to paragraphs 1.2. to 1.2.3. inclusive of  Annex B6. | , g/km;, g/km;, g/km; , g/km. |
| For Level 1B  Output step 5 | FEc,5, km/l; | Averaging of tests and declared value.  Paragraphs 1.2. to 1.2.3. inclusive of Annex B6.  The conversion from FEc,declared to MCO2,c,declared shall be performed for the applicable cycle. For that purpose, the criteria emission over the complete cycle shall be used. | FEc,declared, km/l  MCO2,c,declared, g/km. |
| 7  results of a Type 1 test for a test vehicle. | For Level 1A:  Output step 6 | , g/km;, g/km; , g/km. | Alignment of phase values. Paragraph 1.2.4. of Annex B6,  and: | , g/km; , g/km. |
| For Level 1B: Output step 5 Output step 6 | MCO2,CS,c,5, g/km;  MCO2,CS,p,5, g/km;  MCO2,CS,c,declared, g/km. | Alignment of phase values.  Paragraph 1.2.4. of Annex B6. | MCO2,CS,p,7, g/km. |
| For Level 1A only  8  Interpo-lation family result.  Final criteria emission result.  If the interpolation method is not applied, step No. 9 is not required and the output of this step is the final CO2 result. | Output step 6 | For each of the test vehicles H and L and, if applicable, vehicle M:  , g/km; | If in addition to a test vehicle H a test vehicle L and, if applicable vehicle M was also tested, the resulting criteria emission value shall be the highest of the two or, if applicable, three values and referred to as  In the case of the combined THC+NOx emissions, the highest value of the sum referring to either the vehicle H or vehicle L or, if applicable, vehicle M is to be taken as the type approval value.  Otherwise, if no vehicle L or if applicable vehicle M was tested,  In the case that the interpolation method is applied, intermediate rounding shall be applied according to paragraph 6.1.8. of this Regulation:  CO2 values derived in step 7 of this table shall be rounded to two places of decimal. Also, the output for CO2 is available for vehicles H and vehicle L and, if applicable, for vehicle M.  In the case that the interpolation method is not applied, final rounding shall be applied according to paragraph 6.1.8. of this Regulation:  CO2 values derived in step 7 of this table shall be rounded to the nearest whole number. | , g/km; , g/km; , g/km; |
| Output step 7 | For each of the test vehicles H and L and, if applicable, vehicle M: , g/km; , g/km. |

"

*Paragraph 4.5.1.1.5.,* amend to read:

"4.5.1.1.5. Vehicle M

Vehicle M is a vehicle within the interpolation family between vehicles L and H with a cycle energy demand which is preferably closest to the average of vehicles L and H.

The limits of the selection of vehicle M (see Figure A8/5) are such that neither the difference in CO2 mass emission between vehicles H and M nor the difference in charge-sustaining CO2 mass emission between vehicles M and L is higher than the allowed charge-sustaining CO2 range according to paragraph 4.5.1.1.2. of this annex. The defined road load coefficients and the defined test mass shall be recorded.

Figure A8/5

**Limits for the selection of vehicle M**



For Level 1A

The linearity of the corrected measured and averaged charge-sustaining CO2 mass emission for vehicle M, MCO2,c,6,M according to step 6 of Table A8/5 of Annex B8, shall be verified against the linearly interpolated charge-sustaining CO2 mass emission between vehicles L and H over the applicable cycle by using the corrected measured  and averaged charge-sustaining CO2 mass emission MCO2,c,6,H of vehicle H and MCO2,c,6,L of vehicle L, according to step 6 of Table A8/5 of Annex B8, for the linear CO2 mass emission interpolation.

For Level 1B

An additional averaging of tests using the charge-sustaining CO2-output of step 4a is necessary (not described in Table A8/5). The linearity of the corrected measured and averaged charge-sustaining CO2 mass emission for vehicle M, MCO2,c,4a,M according to step 4a of Table A8/5 of Annex B8, shall be verified against the linearly interpolated CO2 mass emission between vehicles L and H over the applicable cycle by using the corrected measured  and averaged charge-sustaining CO2 mass emission MCO2,c,4a,H of vehicle H and MCO2,c,4a,L of vehicle L, according to step 4a used in of Table A8/5 of Annex B8, for the linear CO2 mass emission interpolation.

For Level 1A and Level 1B

The linearity criterion for vehicle M shall be considered fulfilled if the charge-sustaining CO2 mass emission of vehicle M over the applicable WLTC minus the charge-sustaining CO2 mass emission derived by interpolation is less than 2 g/km or 3 per cent of the interpolated value, whichever value is less, but at least 1 g/km. See Figure A8/6.

Figure A8/6

…"

*Paragraph 4.6.1., Table A8/8, Step No. 16,* amend to read:

"

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 16  Interpolation family result.  If the interpola-tion method is not applied, step No. 17 is not required and the output of this step is the final result. | Output step 15 | If applicable: ECDC,CD,COP, Wh/km; | In the case that the interpolation method is applied, intermediate rounding shall be performed according to paragraph 6.1.8. of this Regulation:  MCO2,CD shall be rounded to the second place of decimal.  ECAC,CD,final and ECAC,weighted,final shall be rounded to the first place of decimal.  If applicable:  ECDC,CD,COP shall be rounded to the first place of decimal.  FCCD and FECD shall be rounded to the third place of decimal.  Output is available for vehicles H and for vehicle L and, if applicable, for vehicle M.  In case that the interpolation method is not applied, final rounding shall be applied according to paragraph 6.1.8. of this Regulation:  ECAC,CD , ECAC,weighted and MCO2,CD shall be rounded to the nearest whole number.    If applicable:  ECDC,CD,COP shall be rounded to the nearest whole number.    FCCD and FECD shall be rounded to the first place of decimal. | If applicable: ECDC,CD,COP,final, Wh/km;  For Level 1A, ECAC,CD,final, Wh/km;  MCO2,CD,final, g/km;  ECAC,weighted,final, Wh/km;  FCCD,final, l/100 km;  For Level 1B,  FECD,final, km/l; |
| Output step 14 | ECAC,CD,declared, Wh/km;  ECAC,weighted, Wh/km;  FECD,declared, km/l;  MCO2,CD,declared, g/km. |
| Output step 13 | FCCD,ave, l/100 km; |

"

*Paragraph 4.6.2., Table A8/9, Step No. 7,* amend to read:

"

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 7 | Output step 1 | EAC, Wh; | Calculation of the electric energy consumption based on EAER according to paragraphs 4.3.3.1. and 4.3.3.2. of this annex.  Output is available for each CD test.  In the case that the interpolation method is applied, the output is available for each vehicle H, vehicle L and, if applicable, vehicle M. | EC, Wh/km;  ECp, Wh/km; |
| Output step 3 | EAER, km;  EAERp, km; |

"

*Paragraph 4.6.3.2., Table A8/9b, Step No. 6,* amend to read:

"

|  |  |  |  |
| --- | --- | --- | --- |
| 6 | Output step 1 | EAC, Wh; | Calculation of the electric energy consumption based on EAER according to paragraphs 4.3.3.1. and 4.3.3.2. of this annex.  Output is available for each CD test.  In the case that the interpolation method is applied, the output is available for each vehicle H, vehicle L and, if applicable, vehicle M. |
| Output step 2 | EAER, km;  EAERp, km; |

"

*Annex B8, Appendix 2*

*Paragraph 2.1.,* amend to read:

"2.1. The CO2 mass emission correction coefficient KCO2, the fuel consumption correction coefficients Kfuel,FCHV, as well as, if required by the manufacturer, the phase-specific correction coefficients KCO2,p and Kfuel,FCHV,p shall be developed based on the applicable charge-sustaining Type 1 test cycles.

In the case that vehicle H was tested for the development of the correction coefficient for CO2 mass emission for NOVC-HEVs and OVC-HEVs, the coefficient may be applied to vehicles that fulfil the same interpolation family criteria. For interpolation families which fulfil the criteria of the KCO2 correction family, defined in paragraph 6.3.11. of this Regulation, the same KCO2 value may be applied."

*Add a new paragraph 4.*, to read:

"4. As an option for the manufacturer, it is allowed to apply ΔMCO2,j defined in paragraph 4.5. of Appendix 2 to Annex B6 with the following modification:

is the efficiency of the alternator

0.67 in case is negative (corresponds to a discharge)

1.00 in case is positive (corresponds to a charge)

4.1. In this case, the corrected charge-sustaining CO2 mass emission defined in paragraphs 4.1.1.3., 4.1.1.4. and 4.1.1.5. of this annex shall be replaced by ΔMCO2,j instead of . "

*Annex B8, Appendix 3*

*Paragraph 3.,* amend to read:

" 3. REESS voltage

3.1. External REESS voltage measurement

During the tests described in paragraph 3. of this annex, the REESS voltage shall be measured with the equipment and accuracy requirements specified in paragraph 1.1. of this annex. To measure the REESS voltage using external measuring equipment, the manufacturers shall support the responsible authority by providing REESS voltage measurement points and safety instructions.

3.2. Nominal REESS voltage

For NOVC-HEVs, NOVC-FCHVs, OVC-HEVs and OVC-FCHVs, instead of using the measured REESS voltage according to paragraph 3.1. of this appendix, the nominal voltage of the REESS determined according to IEC 60050-482 may be used.

3.3. Vehicle on-board REESS voltage data

As an alternative to paragraphs 3.1. and 3.2. of this appendix, the manufacturer may use the on-board voltage measurement data. The accuracy of these data shall be demonstrated to the responsible authority.

Table A8 App3/1

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| *Test events* | *Para. 3.1.* | *Para. 3.2.* | | *Para. 3.3.* |
| *60V or more* | *Less than 60V* |
| NOVC-HEV | shall not to be used | shall be used | | shall not to be used |
| OVC-HEV CS condition |
| NOVC-FCHV |
| OVC-FCHV CS condition |
| REESS energy change-based correction procedure (Appendix 2) |
| OVC-HEV CD condition | shall be used | shall not to be used | allowed to use | allowed to use |
| OVC-FCHV CD condition |
| PEV |

"

*Annex B8, Appendix 6*

*Paragraph 1.3.,* amend to read:

"1.3. On the basis of technical evidence provided by the manufacturer and with the agreement of the responsible authority, the dedicated driver-selectable modes, such as "mountain mode" or "maintenance mode" which are not intended for normal daily operation but only for special limited purposes, shall not be considered. Irrespective of the driver-selectable mode selected for the Type 1 test according to paragraph 2. and 3. of this appendix, the vehicle shall comply with the criteria emissions limits in all remaining driver-selectable modes used for forward driving."

*Paragraph 3.2.,* amend to read:

"3.2. If there is no predominant mode or if there is a predominant mode but this mode does not enable the vehicle to follow the reference test cycle under charge-sustaining operating condition, the mode for the test shall be selected according to the following conditions:

(a) If there is only one mode which allows the vehicle to follow the reference test cycle under charge-sustaining operating conditions, this mode shall be selected;

(b) If several modes are capable of following the reference test cycleunder charge-sustaining operating conditions and none of those modes is a configurable start mode, the vehicle shall be tested for criteria emissions, CO2 emissions in the best case mode and worst case mode. Best and worst case modes shall be identified by the evidence provided on the CO2 emissions in all modes. CO2 emissions shall be the arithmetic average of the test results in both modes. Test results for both modes shall be recorded.

At the request of the manufacturer, the vehicle may alternatively be tested with the driver-selectable mode in the worst case position for CO2 emissions.

(c) If several modes are capable of following the reference test cycleunder charge-sustaining operating conditions and at least two or more of those modes are a configurable start mode, the worst case mode for CO2 emissions and fuel consumption shall be selected from these configurable start modes."

*Annex C4*

*Paragraph 1.5.,* amend to read:

"1.5. This paragraph is applicable for Level 1A only

At the request of the manufacturer, the Technical Service may carry out the Type 1 test before the whole vehicle or bench ageing durability test has been completed using the assigned deterioration factors in Table 3A in paragraph 6.7.2. of this Regulation. On completion of the whole vehicle or bench ageing durability test, the Technical Service may then amend the type approval results recorded in Annex A2 to this Regulation by replacing the assigned deterioration factors in the above table with those measured in the whole vehicle or bench ageing durability test."

*Annex C5*

*Paragraph 3.3.5.,* amend to read:

"3.3.5. Manufacturers may demonstrate to the Type Approval Authority that certain components or systems need not be monitored if, in the event of their total failure or removal, emissions do not exceed the OBD thresholds set out in paragraph 6.8.2. of this Regulation.

3.3.5.1. For Level 1A only

The following devices should however be monitored for total failure or removal (if removal would cause the applicable emission limits in paragraph 6.3.10. of this Regulation to be exceeded):

(a) A particulate trap fitted to compression ignition engines as a separate unit or integrated into a combined emission control device;

(b) A NOx after treatment system fitted to compression ignition engines as a separate unit or integrated into a combined emission control device;

(c) A Diesel Oxidation Catalyst (DOC) fitted to compression ignition engines as a separate unit or integrated into a combined emission control device.

3.3.5.2. For Level 1A only

The devices referred to in paragraph 3.3.5.1. of this annex shall also be monitored for any failure that would result in exceeding the applicable OBD thresholds set out in in paragraph 6.8.2. of this Regulation. "

*Paragraph 4.2.2.,* amend to read:

"4.2.2. For Level 1A

The Type Approval Authority will not accept any deficiency request that does not respect the OBD thresholds set out in paragraph 6.8.2. of this Regulation.

For Level 1B

The responsible authority shall reject any deficiency request that does not respect the OBD thresholds set out in regional legislation multiplied by a factor required by regional legislation up to a maximum factor of two."

1. \* In accordance with the programme of work of the Inland Transport Committee for 2020 as outlined in proposed programme budget for 2020 (A/74/6 (part V sect. 20) para 20.37), the World Forum will develop, harmonize and update UN Regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)
2. \*\* This document was scheduled for publication after the standard publication date owing to circumstances beyond the submitter's control. [↑](#footnote-ref-3)
3. [link to be inserted after final notification] [↑](#footnote-ref-4)