|  |  |  |  |
| --- | --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.29/GRSG/2021/4 | |
| _unlogo | **Economic and Social Council** | | Distr.: General  29 January 2021  Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**Working Party on General Safety Provisions**

**121st session**

Geneva, 12-16 April 2021

Item 4 (b) of the provisional agenda

**Awareness of the proximity of Vulnerable Road Users:**

**UN Regulation No. 151 (Blind Spot Information Systems)**

Proposal for Supplement 3 to UN Regulation No. 151 (Blind Spot Information Systems)

Submitted by the experts from VRU-Proxi Informal Working Group (VRU-Proxi)[[1]](#footnote-2)\*

The text was reproduced below was prepared by the experts from the VRU-Proxi Informal Working Group (VRU-Proxi) to propose an amendment to the UN Regulation on uniform provisions concerning the approval of motor vehicles with regard to the Blind Spot Information Systems. The modifications to the existing text of the draft Regulation are marked in bold for new or strikethrough for deleted characters.

I. Proposal

*Paragraph 5.3.1.4.*, amend to read:

"5.3.1.4. The BSIS shall give an information signal at last point of information, for a bicycle moving with a speed between 5 km/h and 20 km/h, at a lateral separation between bicycle and vehicle of between 0.9 and 4.25 metres, which could result in a collision between bicycle and vehicle with an impact position 0 to 6 m with respect to the vehicle front right corner, if typical steering motion would be applied by the vehicle driver.

**The information signal shall not be visible before the first point of information. It shall be given between the first point of information and the last point of information.**

**It shall also give an information signal if a bicycle is moving with a speed between 5 km/h and 20 km/h at a lateral separation of between 0.25 m up to 0.9 m and longitudinally located between [front right corner of the vehicle and 1.0 m] behind the centre of the most forward front wheel while driving straight.**

However, the information signal is not required when the relative longitudinal distance between bicycle and front right corner of the vehicle is more than 30 m to the rear or 7 m to the front."

II. Justification

1. Supplement 1 to the original version of UN Regulation No. 151 (ECE/TRANS/WP.29/GRSG/2019/25) has amended the paragraph 5.3.1.4. The intention of such an amendment was to add an explicit requirement for the maximum detection distance. There was no intention to delete the requirements from paragraph 5.3.1.4. on the information signal boundaries and on the detection area around the front wheel.

2. The opportunity was taken, by reintroducing the requirement on the detection area around the front wheel, to clarify it. The longitudinal location of this detection area still needs to be consolidated.

1. \* In accordance with the programme of work of the Inland Transport Committee for 2021 as outlined in proposed programme budget for 2021 (A/75/6 (Sect.20), para 20.51), the World Forum will develop, harmonize and update UN Regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)