**Proposal for a new Supplement to the 01 series of amendments to UN Regulation No. 154 (Worldwide harmonized Light vehicles Test Procedures (WLTP))**

The modifications to the current text of the Regulation are marked in bold for new or strikethrough for deleted characters.

**I. Proposal**

**[Editorial note: References to “*if PN measurement is required*” throughout the UNR (x16) are not required in the 01 series of amendments (Level 2) as Level 2 requires PN to be measured. If we decide to remove these references do we need to itemise them separately to update the UNR or can a mass change be made?**

**This comment is being made in-line with an equivalent comment in a separate Informal Document relating to the original version, in which there is a proposal to now require PN for Level 1B]**

*Paragraph 6.3.10., Table 1B,* amend to read:

"Table 1B

**Emissions limits for the Type 1 test which apply to the emissions from the first 3 phases of a WLTP test**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | *technically permissible maximum laden mass*  *(GVW) (kg)* |  | *Limit values* | | | | | | | | | | | | | | |
| *Mass of carbon monoxide (CO)* | | |  | | *Mass of non-methane hydrocarbons*  *(NMHC)* | | *Mass of oxides  of nitrogen*  *(NOx)* | | |  | | *Mass of  particulate matter*  *(PM)* | | ***Particle Number***  ***(PN)*** | |
| *L1*  *(mg/km)* | | |  | | *L3*  *(mg/km)* | | *L4*  *(mg/km)* | | |  | | *L5*  *(mg/km)* | | ***L6***  ***(#/km)*** | |
| *Category* | | *Class* |  | *G, O* | | *D* |  |  | *G,O* | *D* | *G* | *D* | *O* |  |  | *G\*1, O* | *D* | ***G\*1, O*** | ***D*** |
| M | | — | All | 1,150 | | 630 |  |  | 100 | 24 | 50 | 150 | 150 |  |  | 5 | 5 | **6.0 × 1011** | **6.0 × 1011** |
| N1~~,~~ ~~N~~~~2~~ | | —\*2 | GVW≤ 1,700 | 1,150 | | 630 |  |  | 100 | 24 | 50 | 150 | 150 |  |  | 5 | 5 | **6.0 × 1011** | **6.0 × 1011** |
| — | 1,700 < GVW ≤ 3,500 | 2,550 | | 630 |  |  | 150 | 24 | 70 | 240 | 240 |  |  | 7 | 7 | **6.0 × 1011** | **6.0 × 1011** |
| —\*3 | All | 4,020 | | — |  |  | 100 | — | 50 | — | 150 |  |  | 5 | — | **6.0 × 1011** | **—** |
|  | |  |  |  | |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | G Petrol, LPG  D Diesel  O Other fuel  1 For petrol or LPG, particulate mass **and particle number** limits shall apply only to vehicles with direct injection engines.  2 Except vehicles having engine displacement less than or equal to 0.660 litre, vehicle length less than or equal to 3.40m, vehicle width less than or equal to 1.48m, and vehicle height less than or equal to 2.00m, seats less than or equal to 3 in addition to a driver, and payload less than or equal to 350kg.  3 Vehicles having engine displacement less than or equal to 0.660 litre, vehicle length less than or equal to 3.40m, vehicle width less than or equal to 1.48m, and vehicle height less than or equal to 2.00m, seats less than or equal to 3 in addition to a driver, and payload less than or equal to 350kg."  **Justification:** Japan regional new requirement (introduction of PN limit) and correction of previous error (relating to N2). | | | | | | | | | | | | | | | | | | |

*Paragraph 6.7.2. Table 3b,* amend to read:

"Table 3b

Additive Deterioration factors **\*5** (for emissions measurements to be compared against the limits in Table 1B)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| *~~Engine Category~~* | *~~Assigned additive deterioration factors~~* | | | | | | |
| *~~CO~~* |  | *~~NMHC~~* | *~~NO~~~~x~~* |  | *~~PM~~* |  |
| ~~Gasoline fuel and LPG~~ | ~~0.11~~ |  | ~~0.12~~ | ~~0.21~~ |  | ~~0.00~~ |  |
| ~~Compression-ignition~~ | ~~As there are no assigned deterioration factors for compression ignition vehicles, manufacturers shall use the whole vehicle ageing durability test procedures to establish deterioration factors.~~ | | | | | | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | ***Technically Permissible Maximum Laden Mass***  ***(GVW) (kg)*** | ***Assigned additive deterioration factors*** | | | | | | | | | | |
| ***Mass of carbon monoxide (CO)*** | | ***Mass of non-methane hydrocarbons***  ***(NMHC)*** | | ***Mass of oxides  of nitrogen***  ***(NOx)*** | | | ***Mass of  particulate matter***  ***(PM)*** | | ***Particle Number***  ***(PN)*** | |
| ***L1***  ***(mg/km)*** | | ***L3***  ***(mg/km)*** | | ***L4***  ***(mg/km)*** | | | ***L5***  ***(mg/km)*** | | ***L6***  ***(#/km)*** | |
| ***Category*** | ***Class*** |  | ***G*** | ***D, O*** | ***G*** | ***D,O*** | ***G*** | ***D*** | ***O*** | ***G\*1*** | ***D, O*** | ***G\*1*** | ***D, O*** |
| **M** | **—** | **All** | **127** | **\*4** | **12** | **\*4** | **11** | **\*4** | **\*4** | **0** | **\*4** | **0** | **\*4** |
| **N1** | **—\*2** | **GVW≤ 1,700** | **127** | **12** | **11** | **0** | **0** |
| **—** | **1,700 < GVW ≤ 3,500** | **281** | **18** | **15** | **0** | **0** |
| **—\*3** | **All** | **327** | **—** | **9** | **—** | **8** | **—** | **0** | **—** | **0** | **—** |

**G Petrol, LPG**

**D Diesel**

**O Other fuel**

**1 For petrol or LPG, particulate mass and particle number limits shall apply only to vehicles with direct injection engines.**

**2 Except vehicles having engine displacement less than or equal to 0.660 litre, vehicle length less than or equal to 3.40m, vehicle width less than or equal to 1.48m, and vehicle height less than or equal to 2.00m, seats less than or equal to 3 in addition to a driver, and payload less than or equal to 350kg.**

**3 Vehicles having engine displacement less than or equal to 0.660 litre, vehicle length less than or equal to 3.40m, vehicle width less than or equal to 1.48m, and vehicle height less than or equal to 2.00m, seats less than or equal to 3 in addition to a driver, and payload less than or equal to 350kg.**

**4 As there are no assigned deterioration factors for compression ignition vehicles, manufacturers shall use the whole vehicle ageing durability test procedures to establish deterioration factors.**

**5 In case that limit value is different from the value defined in Table 1B, the assigned additive deterioration factor shall be calculated using the following equation and shall be rounded according to approval authority instruction:**

**the assigned additive deterioration factor = Limit value \* A \* (Useful life – 3,000)/(80,000 – 3,000)**

**where :**

**A 0.11 for CO, 0.12 for NMHC, 0.21 for NOx and 0.00 for PM and PN**"

**Justification:** Japan regional new requirement (introduction of PN limit) and relevant sections of the UNR and editorial correction.

*Appendix 2*

*Paragraph 3.4.,* amend to read:

"**3.4.** ~~For vehicles referred to in paragraph 5.11. of this Regulation the accuracy x~~~~i,OBFCM~~ ~~of the OBFCM device shall be determined for each single test i in accordance with the formulae in paragraph 4.2. of Appendix 5.~~

**For vehicles referred to in paragraph 5.11. of this Regulation the conformity of production of OBFCM devices as defined in paragraph 2.1. of Appendix 5 shall be evaluated as follows:**

**(1) For each single test i performed for the purposes of paragraph 3. of this Appendix the accuracy xi of the OBFCM device shall be determined in accordance with paragraph 4.2. of Appendix 5.**

**(2) The conformity of production of the OBFCM devices shall be evaluated according to the requirements of paragraph 3.3.1., but applying a factor A value of [1.05].**

**(3) If for the last test N performed for the purposes of paragraph 3. the decision (iii) of paragraph 3.3.1. with regard to the conformity of production of the OBFCM devices is reached, the sequence of tests shall be continued until a final decision (i) or (ii) of paragraph 3.3.1. is reached.**

**The Type Approval authority shall keep a record of the determined accuracies of OBFCM device at each test as well as the decision according to paragraph 3.3.1. after each test.** "

**Justification:** From the time that OBFCM provisions have been introduced in the Euro 6 legislation the OBFCM accuracy has been monitored for Conformity of Production in order to collect data to establish an accuracy requirement.

*Annex A1*

*Insert new paragraph 3.3.2.10.;* to read:

"

|  |  |
| --- | --- |
| 3.3.2.10. | Type of coolant : air/liquid (1) |

"

*Insert new paragraph 3.3.10.;* to read:

"

|  |  |
| --- | --- |
| 3.3.10. | Electric energy converters |
| 3.3.10.1 | Electric energy converter between the electric machine and traction REESS |
| 3.3.10.1.1 | Make : .......................... |
| 3.3.10.1.2 | Type : .......................... |
| 3.3.10.1.3 | Nominal power : .......................... W |
| 3.3.10.2 | Electric energy converter between the traction REESS and low voltage  power supply |
| 3.3.10.2.1 | Make : .......................... |
| 3.3.10.2.2 | Type : .......................... |
| 3.3.10.2.3 | Nominal power : .......................... W |
| 3.3.10.3 | Electric energy converter between the recharge-plug-in and traction REESS |
| 3.3.10.3.1 | Make : .......................... |
| 3.3.10.3.2 | Type : .......................... |
| 3.3.10.3.3 | Nominal power : .......................... W |

"

*Insert new paragraph 3.4.4.7.;* to read:

"

|  |  |
| --- | --- |
| 3.4.4.7. | Type of coolant : air/liquid (1) |

"

*Insert new paragraph 3.4.5.6.;* to read:

"

|  |  |
| --- | --- |
| 3.4.5.6. | Cooling system:  Motor: liquid/air (1)  Controller: liquid/air (1) |
| 3.4.5.6.1. | Liquid-cooling equipment characteristics: |
| 3.4.5.6.1.1. | Nature of the liquid .......................... circulating pumps: yes/no (1) |
| 3.4.5.6.1.2. | Characteristics or make(s) and type(s) of the pump: .......................... |
| 3.4.5.6.1.3. | Thermostat: setting: .......................... |
| 3.4.5.6.1.4. | Radiator: drawing(s) or make(s) and type(s): .......................... |
| 3.4.5.6.1.5. | Relief valve: pressure setting: .......................... |
| 3.4.5.6.1.6. | Fan: characteristics or make(s) and type(s): .......................... |
| 3.4.5.6.1.7. | Fan duct: .......................... |
| 3.4.5.6.2. | Air-cooling equipment characteristics |
| 3.4.5.6.2.1. | Blower: characteristics or make(s) and type(s): .......................... |
| 3.4.5.6.2.2. | Standard air ducting: .......................... |
| 3.4.5.6.2.3. | Temperature regulating system: yes/no (1) |
| 3.4.5.6.2.4. | Brief description: .......................... |
| 3.4.5.6.2.5. | Air filter: .......................... make(s): .......................... type(s): |
| 3.4.5.6.3. | Temperatures admitted by the manufacturer (maximum) |
| 3.4.5.6.3.1. | Motor outlet: ..........................° C |
| 3.4.5.6.3.2. | controller inlet: ..........................° C |
| 3.4.5.6.3.3. | at motor reference point(s): ..........................° C |
| 3.4.5.6.3.4. | at controller reference point(s): ..........................° C |

"

*Insert new paragraph 3.4.11.;* to read:

"

|  |  |
| --- | --- |
| 3.4.11. | Electric energy converters |
| 3.4.11.1 | Electric energy converter between the electric machine and traction REESS |
| 3.4.11.1.1 | Make : .......................... |
| 3.4.11.1.2 | Type : .......................... |
| 3.4.11.1.3 | Nominal power : .......................... W |
| 3.4.11.2 | Electric energy converter between the traction REESS and low voltage  power supply |
| 3.4.11.2.1 | Make : .......................... |
| 3.4.11.2.2 | Type : .......................... |
| 3.4.11.2.3 | Nominal power : .......................... W |
| 3.4.11.3 | Electric energy converter between the recharge-plug-in and traction REESS |
| 3.4.11.3.1 | Make : .......................... |
| 3.4.11.3.2 | Type : .......................... |
| 3.4.11.3.3 | Nominal power : .......................... W |

"

**Justification:** additions to the Information Document to add the type of coolant of the motor, the type of coolant of the REESS, and the electric energy converters in the vehicle as these are IP family criteria for HEVs and PEV but the information is not currently declared in the Information Document.

*Annex A1, Appendix 1, Part I, Paragraph 2.1.1.2.1.,* amend to read:

"2.1.1.2.1. CO2 emission of vehicles with at least one combustion engine, of NOVC-HEV and of OVC-HEV in the case of a charge-sustaining Type 1 test

For each driver selectable mode tested the points below have to be repeated (predominant mode or best case mode and worst case, mode if applicable)

Test 1

| *CO2 emission* | *Low* | *Medium* | *High* | *Extra High* | *Combined* |
| --- | --- | --- | --- | --- | --- |
| Measured value MCO2,p,1 **/MCO2,c,2** |  |  |  |  | ~~-~~  [Editorial note: the "-" above has been struck-through] |
| Speed and distance corrected value MCO2,p,~~1b~~**2b** / MCO2,c,2**b** |  |  |  |  |  |
| RCB correction coefficient: (5) |  |  |  |  |  |
| MCO2,p,3 / MCO2,c,3 |  |  |  |  |  |
| Regeneration factors (Ki)  Additive |  | | | | |
| Regeneration factors (Ki)  Multiplicative |  | | | | |
| MCO2,c,4 | - | | | |  |
| AFKi= MCO2,c,3 / MCO2,c,4 | - | | | |  |
| MCO2,p,4 / MCO2,c,4 |  |  |  |  | - |
| ATCT correction (FCF) (4) |  | | | | |
| Temporary values MCO2,p,5 / MCO2,c,5 |  |  |  |  |  |
| Declared value | - | - | - | - |  |
| dCO21 \* declared value | - | - | - | - |  |

"

*Annex A1, Appendix 1, Part II, Paragraph 2.1.2.,* amend to read:

"**2.1.2. CO2 emission of vehicle with at least one combustion engine, of NOVC-HEV and of OVC-HEV in case of a charge-sustaining tests**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| *CO2 emission (g/km)* | *Low* | *Medium* | *High* | *Extra High* | *Combined* |
| Measured value MCO2,p,1 **/ MCO2,c,2** |  |  |  |  | ~~-~~  [Editorial note: the "-" above has been struck-through] |
| Measured Speed and distance corrected value MCO2,p,~~1b~~ **2b** / MCO2,c,2**b** |  |  |  |  |  |
| RCB correction coefficient (2) |  |  |  |  |  |
| MCO2,p,3 / MCO2,c,3 |  |  |  |  |  |

"

*Annex A1, Appendix 1, Part II, Paragraph 2.2.2.,* amend to read:

"**2.2.2. CO2 emission of vehicle with at least one combustion engine, of NOVC-HEV and of OVC-HEV in case of a charge-sustaining tests**

| *CO2 emission (g/km)* | *Low* | *Medium* | *High* | *Extra High* | *Combined* |
| --- | --- | --- | --- | --- | --- |
| Measured value MCO2,p,1 **/ MCO2,c,2** |  |  |  |  | ~~-~~  [Editorial note: the "-" above has been struck-through] |
| Measured Speed and distance corrected value MCO2,p,~~1b~~**2b** / MCO2,c,2**b** |  |  |  |  |  |
| RCB correction coefficient (2) |  |  |  |  |  |
| MCO2,p,3 / MCO2,c,3 |  |  |  |  |  |

"

**Justification:** Editorial corrections and correction of errors

*Annex B2*

*Paragraph 6. (as introduced by Supp.1),* amend to read:

"6. Calculation tools

Examples of gear shift calculating tools can be found in the same webpage as this Regulation.[[1]](#footnote-1)

The following tools are provided:

(a) ACCESS based tool,

(b) Matlab code tool

(c) NET ~~core~~ **framework** tool

**(d) Python based tool**

These tools were validated by the comparison of calculation results between the ACCESS tool, the Matlab code**,** ~~and~~ the .NET ~~core~~ **framework** code **and the Python based tool** for 115 different vehicle configurations supplemented by additional calculations for 7 of them with additional options like "apply speed cap", "suppress downscaling", "choose other vehicle class cycle" and "choose individual nmin\_drive values".

The 115 vehicle configurations cover extreme technical designs for transmission and engines and all vehicle classes.

All ~~three~~ **four** tools deliver identical results with respect to gear use and clutch operation and although only the text in Annexes B1 and B2 is legally binding the tools have achieved a status that qualifies them as reference tools."

**Justification:** addition of a new verified tool and editorial correction

*Annex B3*

*Paragraph 7., Table A3/19,* amend to read:

"7. Technical data on fuels for Type 4 test on evaporative emissions

Table A3/19

**Petrol reference fuel for Type 4 test**

| *Parameter* | *Unit* | *Limits* | | *Test method* |
| --- | --- | --- | --- | --- |
| *Minimum* | *Maximum* |
| Research octane number, RON |  | 95.0 | 98.0 | EN ISO 5164  JIS K2280 |
| Density at 15 °C | kg/m3 | 743.0 | 756.0 | EN ISO 12185  JIS K2249-1,2,3 |
| Vapour pressure | kPa | 56.0 | 60.0 | EN 13016-1  JIS K2258-1,2 |
| Distillation: |  |  |  |  |
| – evaporated at 70 °C | % v/v | 34.0 | 46.0 | EN ISO 3405 |
| – evaporated at 100 °C | % v/v | 54.0 | 62.0 | EN ISO 3405 |
| – evaporated at 150 °C | % v/v | 86.0 | 94.0 | EN ISO 3405 |
| Hydrocarbon analysis: |  |  |  |  |
| – olefins | % v/v | 6.0 | 13.0 | EN 22854  **JIS K2536-1,2** |
| – aromatics | % v/v | 25.0 | 32.0 | EN 22854  **JIS K2536-1,2,3** |
| – benzene | % v/v | - | 1.00 | EN 22854 EN 238  JIS K2536-2,3,4 |
| Oxygen content | % m/m | 3.3 | 3.7 | EN 22854  JIS K2536-2,4,6 |
| Sulphur content | mg/kg | — | 10 | EN ISO 20846  EN ISO 20884  JIS K2541-1,2,6,7 |
| Lead content | mg/l | Not detected | | EN 237  JIS K2255 |
| Ethanol | % v/v | 9.0 | 10.0 | EN 22854  JIS K2536-2,4,6 |
| MTBE |  | Not detected | | JIS K2536-2,4,5,6a |
| Methanol |  | Not detected | | JIS K2536-2,4,5,6a |
| Kerosene |  | Not detected | | JIS K2536-2,4a |
| a Other method that is traceable to national or international standard may be used. " | | | | |

**Justification:** Editorial correction

*Annex B4*

*Paragraph 4.3.2.5.3.,* amend to read:

"4.3.2.5.3. Aerodynamic drag modelling

The aerodynamic drag coefficient (Y) shall be modelled as a ~~four-term~~ **five-term** polynomial as a function of yaw angle Y as in the equation below:

…"

**Justification:** correction of error

*Annex B6*

*Table A6/1, amend to read:*

"*…*

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| NOVC-FCHV | - | FCCS  Paragraph 4.2.1.2.1. of Annex B8.  . | FECS  Paragraph 4~~,~~**.**2~~,~~**.**1.2.1. of Annex B8. | - | - |

…"

**Justification:** correction of error

*Paragraph 2.6.1.4.,* amend to read:

"2.6.1.4. Gaseous fuel vehicles

Between the tests on the first gaseous reference fuel and the second gaseous reference fuel, for vehicles with positive ignition engines fuelled with LPG or NG/biomethane or so equipped that they can be fuelled with either petrol or LPG or NG/biomethane, the vehicle shall be preconditioned again before the test on the second reference fuel. ~~Between the tests on the first gaseous reference fuel and the second gaseous reference fuel, for vehicles with positive ignition engines fuelled with LPG or NG/biomethane or so equipped that they can be fuelled with either petrol or LPG or NG/biomethane, the vehicle shall be preconditioned again before the test on the second reference fuel.~~"

**Justification:** Editorial correction

*Annex B6, Appendix 2*

*Table A6.App2/1,* amend to read:

"Table A6.App2/1

**Energy content of fuel (as applicable)**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Fuel | Petrol  (E0) | Petrol (E10) | Ethanol (E85) | Diesel (B0) | Diesel (B7) | LPG | CNG |
| Heat value | 8.92  kWh/l | 8.64 kWh/l | 6.41 kWh/l | 9.85  kWh/l | 9.79 kWh/l | 12.86 x ρ kWh/l | 11.39 ~~MJ/m³~~ **kWh/m3** |

ρ = test fuel density at 15°C (kg/l) "

**Justification:** correction of error

*Annex B6 Appendix 2 Paragraph 3.4.,* amend to read:

"3.4. Correction of CO2 mass emission over the whole cycle ~~as a function of the correction criterion c~~

3.4.1. **Reserved**

~~Calculation of the correction criterion c~~

~~The correction criterion c is the ratio between the absolute value of the electric energy change ∆E~~~~REESS,j~~ ~~and the fuel energy and shall be calculated using the following equations:~~

~~where:~~

~~c is the correction criterion;~~

~~ΔE~~~~REESS,j~~ ~~is the electric energy change of all REESSs over period j determined according to paragraph 4.1. of this appendix, Wh;~~

~~is, in this paragraph, the whole applicable WLTP test cycle;~~

~~is the fuel energy according to the following equation:~~

~~where:~~

~~is the energy content of the consumed fuel over the applicable WLTP test cycle, Wh;~~

~~is the heating value according to Table A6.App2/1, kWh/l;~~

~~is the non-balanced fuel consumption of the Type 1 test, not corrected for the energy balance, determined according to paragraph 6. of Annex B7, and using the results for criteria emissions and CO~~~~2~~ ~~calculated in step 2 in Table A7/1, l/100 km;~~

~~d is the distance driven over the corresponding applicable WLTP test cycle, km;~~

~~conversion factor to Wh.~~

3.4.2. The correction shall be applied if is negative (corresponding to REESS discharging)

At the request of the manufacturer, the correction may be omitted and uncorrected values may be used if:

(a) is positive (corresponding to REESS charging);

(b) the manufacturer can prove to the responsible authority by measurement that there is no relation between and mass emission and and fuel consumption respectively."

**Justification:** When GTR No. 15 was transposed to UNR154 it was decided not to apply correction criterion c for REESS energy change-based correction procedure under paragraph 3.4.2. of Appendix 2 to Annex B6. Accordingly, paragraph 3.4.1. is no longer necessary and should therefore be deleted, with the heading for paragraph 3.4. also needing to be updated to reflect this change.

*Annex B7*

*Table A7/1, Step 4c,* amend to read:

"

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4c | Output step 4a | Mi,c,4a, g/km;  MCO2,c,4a, g/km. | In the case these values are used for the purpose of conformity of production, the criteria emission values and CO2 mass emission values shall be multiplied with the run-in factor determined according to paragraph 8.2.4. of this Regulation:  Mi,c,4c = RIC (j) × Mi,c,4a  MCO2,c,4c = RICO2 (j) x MCO2,c,4a  In the case these values are not used for the purpose of conformity of production:  Mi,c,4c = Mi,c,4a  MCO2,c,4c = MCO2,c,4a | Mi,c,4c;  MCO2,c,4c |
| Calculate fuel efficiency (FEc,4c\_temp)　according to paragraph 6. of Annex B6.  In the case this value is used for the purpose of conformity of production, **the criteria emission values and** the fuel efficiency value shall be multiplied with the run in factor determined according to paragraph 8.2.4. of this Regulation:  **Mi,c,4c = RIC (j) × Mi,c,4a**  FEc,4c = RIFE (j) x FEc,4c\_temp  In the case these values are not used for the purpose of conformity of production:  FEc,4c = FEc,4c\_temp | **Mi,c,4c;**  FEc,4c, km/l; |

"

**Justification:** Japan regional new requirement (introduction of PN limit) and relevant sections of the UNR.

*Paragraph 3.2.1.1.4.,* amend to read:

"3.2.1.1.4. Flow-weighted arithmetic average concentration calculation

The following calculation method shall be applied for CVS systems that are not equipped with a heat exchanger or for CVS systems with a heat exchanger that ~~do~~ **does** not comply with paragraph 3.3.5.1. of Annex B5.

…"

**Justification:** Editorial correction

*Paragraph 3.2.3.2.2.1.,* amend to read:

"3.2.3.2.2.1. Mass of an individual vehicle

The test masses of vehicles H and L shall be used as input for the interpolation method.

TMind, in kg, shall be the ~~individual~~ test mass of ~~the~~ **an individual** vehicle according to paragraph 3.2.25. of this Regulation.

If the same test mass is used for test vehicles L and H, the value of shall be set to the mass of test vehicle H for the interpolation method."

**Justification:** Editorial correction

*Paragraph 3.2.3.2.2.3.2.1.,* amend to read:

"3.2.3.2.2.3.2.1. The manufacturer shall ~~submit the declared~~ **declare the** scope of applicable vehicles for the alternative method **to the responsible authority** and the declared scope shall be documented ~~to~~ **in** relevant test reports when evidence of equivalency is shown to the responsible authority. The responsible authority may request the confirmation of equivalency for the alternative method by selecting the vehicle from the scope declared by the manufacturer after equivalency was demonstrated. The result shall fulfil an accuracy for Δ(CD×Af) of ±0.015 m². This procedure shall be based on wind tunnel measurements fulfilling the criteria of this Regulation. If this procedure is not satisfied, the approval of the alternative method is regarded as invalidated."

**Justification:** Editorial correction

*Paragraph 7.4.2.3.,* amend to read:

"7.4.2.3. ...

For the city cycle during which the combustion engine starts to consume fuel, the drive indices IWR and RMSSE shall not be calculated individually. Instead, depending on the number of completed city cycles before the city cycle during which the combustion engine start**s**, the incomplete city cycle shall be combined with the previous city cycles as follows and shall be considered as one cycle in the context of the drive trace index calculations.

…"

**Justification:** Editorial correction

*Annex B8*

*Table A8/5, Step 4c,* amend to read:

"

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4c | Output step 4a | Mi,CS,c,4a, g/km;  MCO2,CS,c,4a, g/km. | In the case these values are used for the purpose of conformity of production, the criteria emission values and CO2 mass emission values shall be multiplied with the run-in factor RI determined according to paragraph 8.2.4. of this Regulation:  Mi,CS,c4c = RIC (j) × Mi,CS,c,4a  MCO2,CS,c,4c = RICO2 (j) x MCO2,CS,c,4a  In the case these values are not used for the purpose of conformity of production:  Mi,c,4c = Mi,c,4a  MCO2,,4c = MCO2,c,4a | Mi,CS,c,4c;  MCO2,CS,c,4c |
| **In the case these values are used for the purpose of conformity of production, the criteria emission values shall be multiplied with the run-in factor RI determined according to paragraph 8.2.4. of this Regulation:**  **Mi,CS,c4c = RIC (j) × Mi,CS,c,4a**  Calculate fuel efficiency (FEc,4c\_temp) according to paragraph 6.14.1. of Annex B6.  In the case this value is used for the purpose of conformity of production, the fuel efficiency value shall be multiplied with the run in factor determined according to paragraph 8.2.4. of this Regulation:FEc,4c = RIFE (j) x FEc,4c\_temp  In the case these values are not used for the purpose of conformity of production:  FEc,4c = FEc,4c\_temp | **Mi,CS,c,4c;**  FEc,4c, km/l; |

"

**Justification:** Japan regional new requirement (introduction of PN limit) and relevant sections of the UNR.

*Paragraph 4.4.1.1.,* amend to read:

"4.4.1.1. All-electric range AER

The all-electric range AER for OVC-HEVs shall be determined from the charge-depleting Type 1 test described in paragraph 3.2.4.3. of this annex as part of the Option 1 test sequence and ~~is~~ referenced in paragraph 3.2.6.1. of this annex as part of the Option 3 test sequence by driving the applicable WLTP test cycle according to paragraph 1.4.2.1. of this annex. The AER is defined as the distance driven from the beginning of the charge-depleting Type 1 test to the point in time where the combustion engine starts consuming fuel."

**Justification:** Editorial correction

*Paragraph 4.4.2.1.1.,* amend to read:

"…

is the weighted electric energy consumption for the applicable WLTP test cycle of the shortened Type 1 test procedure ~~Type 1 test~~, Wh/km;

…"

**Justification:** Editorial correction

*Paragraph 4.4.3.,* amend to read:

"4.4.3. Charge-depleting cycle range for OVC-HEVs

The charge-depleting cycle range RCDC shall be determined from the charge-depleting Type 1 test described in paragraph 3.2.4.3. of this annex as part of the Option 1 test sequence and ~~is~~ referenced in paragraph 3.2.6.1. of this annex as part of the Option 3 test sequence. The is the distance driven from the beginning of the charge-depleting Type 1 test to the end of the transition cycle according to paragraph 3.2.4.4. of this annex."

**Justification:** Editorial correction

*Paragraph 4.4.4.1.,* amend to read:

"…

is the charge-depleting cycle range according to ~~paragraph 4.4.2.~~ **paragraph 4.4.3.** of this annex, km;

…"

**Justification:** correction of error

*Paragraph 4.5.1.1.2.,* amend to read:

"4.5.1.1.2. The maximum difference in charge-sustaining CO2 **emissions** allowed over the applicable cycle …"

*Table A8/8, step 5*, amend to read:

"

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| For results after 4 phases  5 | Output step 1 | Mi,CD,j, g/km;  PMCD,c, mg/km;  PNCD,j, particles per kilometer. | Calculation of combined values for emissions for nveh cycles; ~~in the case of interpolation for n~~~~veh,L~~ ~~cycles for each vehicle~~ **in the case that the interpolation method is applied, nveh,L cycles shall be used for nveh,H cycles and nveh,M cycles, if applicable**.  Output is available for each test.  In the case that the interpolation method is applied, the output is available for vehicle H, L and, if applicable, M. | Mi,CD,c, g/km;  PMCD,c, mg/km;  PNCD,c, particles per kilometer. |

"

**Justification:** Editorial correction

*Annex B8 Appendix 2*

*Paragraph 2.2.,* amend to read:

"2.2. ....

The correction coefficients determined by the manufacturer shall be reviewed and approved by the responsible authority prior to ~~its~~ **their** application.

If the set of at least five tests …"

**Justification:** Editorial correction

*Paragraph 3.1.1.3.4.,* amend to read:

"3.1.1.3.4. To obtain a set of applicable WLTP test cycles required for the determination of the correction coefficients **according to paragraph 2.2. of this appendix**, the test may be followed by a number of consecutive sequences ~~required according to paragraph 2.2. of this appendix~~ **in accordance with the requirements of** paragraph 3.1.1.1. to paragraph 3.1.1.3.**3.** inclusive of this appendix."

**Justification:** Editorial correction

*Annex C3*

*Paragraph 4.2.3.4.,* amend to read:

"4.2.3.4. Calculations

The calculation of net hydrocarbon mass change within the enclosure is used to determine the chamber's hydrocarbon background and leak rate. Initial and final readings of hydrocarbon concentration, temperature and barometric pressure are used ~~in the following formula~~ to calculate the mass change.

The calculation shall be undertaken in accordance **with the equation** in ~~paragraph 7.~~ **either paragraph 7.1. or alternatively paragraph 7.1.1.** of this annex, using the following value for V.

V is the net enclosure volume, m3."

**Justification:** Editorial correction. A draft of GTR19 Amendment 3 had an equation in paragraph 4.2.3.4. which was then deleted as it was duplicated in paragraph 7. Paragraph 4.2.3.4. was not then updated to reflect this deletion – hence the need to now update.

*Paragraph 8.,* amend to read:

"8. Test report

…

(e) Measurement of first diurnal, DL1st day;

(f) Measurement of second diurnal, DL2nd day;

…"

**Justification:** Editorial correction. "1st day” and “2nd day” made sub-script.

*Annex C5*

*Appendix 1*

*Insert new paragraph 2.4.*, to read:

"2.4. For OVC-HEVs, testing shall be carried out under charge-sustaining conditions."

**Justification:** introduce provision that was not transposed from UN Regulation No. 83 07 series of amendments

*Paragraph 7.3.2.(g).,* amend to read:

"(g) Manufacturers may request to use special denominator conditions for certain components or systems and this request can be approved only if it can be demonstrated to the Type Approval Authority by submitting data and/or an engineering evaluation that **those** other conditions are necessary to allow for reliable detection of malfunctions."

**Justification:** Editorial correction

**II. Justification**

See justifications provided following each proposed amendment, or group of amendments.

1. [link to be inserted after final notification] [↑](#footnote-ref-1)