|  |  |
| --- | --- |
| Transmitted by the experts of ETRTO | Informal document **GRBP-74-35-Rev.1**  (74th GRBP, 15 – 17 September 2021,  agenda item 5) |

1. **Proposal to amend document ECE/TRANS/WP.29/GRBP/2021/15**

The changes compared to document ECE/TRANS/WP.29/GRBP/2021/15 are marked in **bold** for added text and strike through for deleted text, all in red font.

Insert a new paragraph 3.2.6.2., to read:

"**~~3.2.6.1.~~ 3.2.6.2. The inscription "ET" and/or "POR" if the tyre is classified in the category of use "Special use. In addition, they may also bear the inscription M+S or M.S or M&S.**

**ET means Extra Tread and POR means Professional Off Road.**"

New paragraph 3.5.1., to be amended as:

**"3.5.1. The markings shall be situated in the lower area of the tyre on at least one of its sidewalls, except for the inscriptions mentioned in ~~paragraph~~ paragraphs 3.2.1. and 3.2.6.1..”**

1. **Justifications**
2. Paragraph numbering is corrected in paragraph 3.2.6.2.
3. Exceptions of markings situated in the lower area of the tyre sidewall in Paragraph 3.5.1. are now fully aligned with UN Regulation No. 30 and UN Regulation No. 117.