|  |  |  |
| --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.29/2021/102 |
| _unlogo | **Economic and Social Council** | Distr.: General2 September 2021Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**185th session**

Geneva, 23-25 November 2021

Item 4.7.7. of the provisional agenda

**1958 Agreement:
Consideration of draft amendments to existing
UN Regulations submitted by GRSG**

 Proposal for Supplement 3 to the original version of UN Regulation No. 151 (Blind Spot Information Systems (BSIS))

 Submitted by the Working Party on General Safety Provisions [[1]](#footnote-2)\*

The text reproduced below was adopted by the Working Party on General Safety Provisions at its 121st session, held in April 2021 (ECE/TRANS/WP.29/GRSG/100, para. 43). It is based on ECE/TRANS/WP.29/GRSG/2021/4, as amended by GRSG-121-07. It is submitted to the World Forum for Harmonization of Vehicle Regulations (WP.29) and the Administrative Committee of the 1958 Agreement (AC.1) for consideration and vote at their November 2021 sessions.

*Paragraph 5.3.1.4.*, amend to read:

"5.3.1.4. The BSIS shall give an information signal at last point of information, for a bicycle moving with a speed between 5 km/h and 20 km/h, at a lateral separation between bicycle and vehicle of between 0.9 and 4.25 metres, which could result in a collision between bicycle and vehicle with an impact position 0 to 6 m with respect to the vehicle front right corner, if typical steering motion would be applied by the vehicle driver.

The information signal shall not be visible before the first point of information. It shall be given between the first point of information and the last point of information.

It shall also give an information signal if a bicycle is moving with a speed between 5 km/h and 20 km/h, at a lateral separation of between 0.25 m up to 0.9 m and longitudinally located between -0.6 m and +0.6 m in reference to the centre of the most forward front wheel while driving straight.

However, the information signal is not required when the relative longitudinal distance between bicycle and front right corner of the vehicle is more than 30 m to the rear or 7 m to the front."

1. \* In accordance with the programme of work of the Inland Transport Committee for 2021 as outlined in proposed programme budget for 2021 (A/75/6 (part V sect. 20) para 20.51), the World Forum will develop, harmonize and update UN Regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)