Proposal for Supplement 01 to the 03 series of amendments to UN Regulation No. 67

Submitted by the experts of Liquid Gas Europe

The text reproduced below was prepared by the expert from Liquid Gas Europe. The modifications to the current text of the regulation are marked in bold characters and strikethrough for deleted characters.

1. **Proposal**

*Paragraph 6.3.6.,* amend to read:

“6.3.6. …

(b) A pressure relief valve provided that it complies to paragraph 6.~~15~~**17**.8.3. below, or

…”

*Annex 3 to Annex 13, change references to par. 6.15. (and subparagraphs) to par. 6.17. (and subparagraphs) (50 occurrences)*

*Annex 16 - Paragraphs 18.3.1. and 18.3.2.,* amend to read:

“18.3.1. Perform for both samples the flow test according to paragraph 6.~~15~~**17**.8.3. of this Regulation.

18.3.2. Requirements:

Both aged and non-aged samples "a" and "b" shall comply with the flow requirements as per paragraph 6.~~15~~**17**.8.3. of this Regulation.

The non-metallic material of the samples "a" and "b" shall show no cracks, deformation or any visual damage.”

1. **Justification**

Modifications to UNECE Regulation no. 67 aims to correct the references to previous par. 6.15., renumbered as par. 6.17. by Supplement 15 to 01 series of Amendments to Regulation 67 (doc. ECE/TRANS/WP.29/2018/18).

**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**