|  |  |  |
| --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.29/2022/24 |
| _unlogo | **Economic and Social Council** | Distr.: General23 December 2021Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**186th session**

Geneva, 8-11 March 2022

Item 4.8.4 of the provisional agenda

**1958 Agreement:
Consideration of draft amendments to existing
UN Regulations submitted by GRSG**

 Proposal for supplement 1 to the 02 series of amendments of
UN Regulation No. 125

 Submitted by the Working Party on General Safety Provisions [[1]](#footnote-2)\*

The text reproduced below was adopted by the Working Party on General Safety Provisions (GRSG) at its 122nd session (ECE/TRANS/WP.29/GRSG/101, para. 99). It is based on ECE/TRANS/WP.29/GRSG/2021/31. It is submitted to the World Forum for Harmonization of Vehicle Regulations (WP.29) and to the Administrative Committee (AC.1) for consideration at their March 2022 sessions.

*Paragraph 5.1.3.4.,* amend to read:

“5.1.3.4. An obstruction between a plane through V2, and declined at least 1° below the horizontal and a plane through V2 and declined 4° below the horizontal will be tolerated if the conical projection of this obstruction, starting from V2, on an area "S" as defined in paragraph 5.1.3.4.1. below does not exceed 20 per cent of this area.

*Paragraph 5.1.3.5.*, amend to read:

"5.1.3.5.The transparent field of vision as defined in paragraph 5.1.1. may be overlaid by information of a Field of Vision Assistant. The provisions of paragraph 5.1.3.5.1. to 5.1.3.5.5. and of paragraph 5.1.3.6. are applying to information from an FVA if overlaid in the transparent field of vision andabove and on the sides of area S in the transparent area.

The information displayed by the FVA may be non-driving related, hence different to that listed in paragraph 5.1.3.5.1. and not submitted to the provisions of paragraph 5.1.3.5.1. to 5.1.3.5.5., as long as the parking gear/brake has not been released for the first time after the activation of the vehicle master control switch.”

*Annex 5,* amend to read:

"Annex 5

 Field of Vision Assistant

# Examples for Warning / Highlight / Information as specified in paragraph 5.3.5.1.:

|  |  |
| --- | --- |
|  | Examples |
| Warning/Highlight hazardous traffic situation | Abrupt braking situationsOncoming traffic in turning manoeuvresOncoming Traffic Jam/vehicle break down.Vehicles leaving the lane or entering the own driving path |
| Warning/highlight vulnerable road users or other road users which may be overseen | PedestriansCyclistsCrossing road usersRoad users in blind spot or road users covered by other objectsAnimals |
| Information to maintain the distances to surrounding road user and infrastructure | Distance to vehicle in frontLane keep assist, lane change assist, speed limits changes |
| Information to find and maintain the correct driveway and to follow the road instructions | Navigation Information, symbols and arrows during automatic lane change(Directions, Remaining distance to target, border crossings)Highlighting stop lines and pedestrian crosswalks |
| Information to support driver’s setting | Highlighting edges of the position of the FVA area during adjustment |

"

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. \* In accordance with the programme of work of the Inland Transport Committee for 2022 as outlined in proposed programme budget for 2022 (A/76/6 (part V sect. 20) para 20.76), the World Forum will develop, harmonize and update UN Regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)