**Proposal for a new Supplement to the 01 series of Amendments to UN Regulation No. 101**

This document aims to harmonize the requirements of the new 08 series of UN Regulation No. 48 with the vehicle settings for dynamometer operation of UN Regulation No. 101.

The modifications to the current text of the Regulation are marked in bold for new or strikethrough for deleted characters. The red text shows the differences between this document and the first version GRPE-85-19.

**I. Proposal**

*In Annex 5, Paragraph 5.1.2.,* amendto read:

"5.1.2. ~~The daytime running lamps of the vehicle as defined in paragraph 2. of Regulation No. 48 shall be switched on during the test cycle if the vehicle is required to be equipped with daytime running lamps as indicated in paragraph 5.22. of Regulation No. 48. The vehicle tested shall be equipped with the daytime running lamp system that has the highest electrical energy consumption among the daytime running lamp systems, which are fitted by the manufacturer to vehicles in the group represented by the type approved vehicle. The manufacturer shall supply appropriate technical documentation to the Type Approval Authorities in this respect.~~

**The vehicle to be tested shall be equipped with the daytime running lamp system that has the highest electrical energy consumption of the daytime running lamp systems, which are fitted by the manufacturer to vehicles in the group represented by the type-approved vehicle. The manufacturer shall supply appropriate technical documentation to the type-approval authorities in this respect.**

**The daytime running lamps as defined in paragraph 2 of Regulation No. 48 shall be switched ON during the test cycle.**"

*In Annex 5,* add new Paragraph 5.1.2.1.to read:

"**5.1.2.1 Where the rear position lamps and other lamps according to 5.11 of the 08 series of amendments of UN Regulation No. 48 are switched OFF when the ambient light conditions outside the vehicle exceed 7,000 lux (as defined in paragraph 6.19.7.5 of 08 series of amendments of UN Regulation No. 48), ~~subject to agreement with the type approval authority, the manufacturer may request~~ a function replicating the ambient light conditions outside the vehicle exceeding 7,000 lux ~~is~~ may be incorporated into the ~~chassis~~ vehicle’s dynamometer operation mode.**"

**II. Justification**

1. The new 08 series of UN Regulation No. 48 is aiming to introduce the possibility to switch OFF rear position lamps and other lamps when ambient light conditions outside the vehicle are above 7,000 lux in order to avoid unnecessary fuel consumption.
2. The vehicle settings for the dynamometer operation shall be independent of the light conditions in the laboratory. Thus, a trip is proposed to represent ambient light conditions with an illuminance of above 7,000 lux.
3. The text in paragraph 5.1.2. is aligned with modifications done on paragraph 3.2.7. of Annex 4A – Type I test in UN Regulation No. 83.