|  |  |  |
| --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.29/GRSP/2023/4 |
| _unlogo | **Economic and Social Council** | Distr.: General24 February 2023Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**Working Party on Passive Safety**

**Seventy-third session**

Geneva, 15–19 May 2023

Item 7 of the provisional agenda

**UN Regulation No. 17 (Strength of seats)**

 Proposal for Supplement 1 to the 10 Series of Amendments to UN Regulation No. 17 (Strength of seats) [[1]](#footnote-2)\*

 Submitted by the expert from Germany

The text reproduced below was prepared by the expert from Germany after consultation with a group of interested experts consisting of representatives from France, Japan, the Netherlands, the European Association of Automotive Suppliers (CLEPA) and the International Organization of Motor Vehicle Manufacturers (OICA). This proposal supersedes ECE/TRANS/WP.29/GRSP/2022/20 presented at the seventy-second session of the Working Party on Passive Safety (GRSP). The proposal aims to bring the current text of the UN Regulation No. 17 in line with its scope, to ensure that only safe head restraints will be fitted to seats in all seating positions and all vehicle categories, specified in the scope. The modifications to the current text of the UN Regulation are marked in bold for new or strikethrough for deleted characters.

 **I. Proposal**

*Paragraph 1,* amend to read:

 "1. Scope

 This Regulation applies to:

(a) Vehicles of categories M1 and N[[2]](#footnote-3) with regard to the strength of seats and their anchorages and with regard to their head restraints;

(b) Vehicles of categories M2 and M31 with regard to seats not covered by Regulation No. 80, in respect of the strength of seats and their anchorages, and in respect of their head restraints;

(c) Vehicles of category M1 with regard to the design of the rear parts of seat backs and the design of devices intended to protect the occupants from the danger resulting from the displacement of luggage in a frontal impact.

 It does not apply to vehicles with regard to side-facing or rearward-facing seats, or to any head restraint fitted to these seats, with the exception vehicles of category M2 and M3 of classes A and I, subject to the provisions of paragraph 5.1.1.

**Vehicles of other categories may also be approved under this Regulation, in respect of the strength of seats and their anchorages, and in respect of their head restraints.**"

*Paragraphs 5.4. to 5.4.2.2.1.9*., amend to read:

"5.4. Mounting of head restraints

5.4.1. A head restraint shall be mounted on every outboard front seat in every vehicle of category M1. ~~Seats fitted with head restraints, intended for fitment in other seating positions and in other categories of vehicles may also be approved to this Regulation~~.

5.4.2. A head restraint shall be mounted on every outboard front seat in every vehicle of category M2 with a maximum mass not exceeding 3500 kg and of category N1; head restraints mounted in such vehicles shall comply with the requirements of Regulation No. 25, as amended by 04 series of amendments.

**Alternatively, seats fitted with head restraints in these categories of vehicles may comply with the requirements of this Regulation**.~~"~~

*Insert a new paragraph 5.4.3*., to read:

"**5.4.3. Notwithstanding paragraphs 5.4.1. and 5.4.2. above, all forward-facing seats fitted with a head restraint or intended to be fitted with a head restraint in other seating positions and in other categories of vehicles covered by the scope of this UN** **Regulation shall comply with the requirements of this Regulation.**"

 **II. Justification**

1. The scope of UN Regulation No. 17 contains provisions for all seats, their anchorages and their head restraints in vehicles of categories M and N beside seats in M2 and M3 vehicles, approved under UN Regulation No. 80 and excludes only side-facing and rearward-facing seats. The scope is also the right place to enable an optional approval for seats in other categories of vehicles.

2. Paragraphs 5.4.1. and 5.4.2. of the current text of the UN Regulation define seating positions in defined vehicle categories which have mandatorily to be equipped with head restraints.

3. Paragraphs 5.5. to 5.10. of the current UN Regulation specify requirements for all seating positions in a vehicle.

4. Paragraph 5.5.1. clearly requires, that the presence of the head restraint shall not be an additional cause of danger to occupants of the vehicle. In particular, it shall not present in any position of use, any dangerous roughness or sharp edge liable to increase the risk or seriousness of injury to the occupants.

5. The aim of this proposal is to bring the current text of the UN Regulation No. 17 in line with its scope, to ensure, that only safe head restraints will be fitted to seats in all seating positions and in all vehicle categories specified in the scope.

1. \* In accordance with the programme of work of the Inland Transport Committee for 2023 as outlined in proposed programme budget for 2023 (A/77/6 (Sect. 20), table 20.6), the World Forum will develop, harmonize and update UN Regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)
2. As defined in the Consolidated Resolution on the Construction of Vehicles (R.E.3.), document ECE/TRANS/WP.29/78/Rev.6, para. 2 - [www.unece.org/trans/main/wp29/wp29wgs/wp29gen/wp29resolutions.html](http://www.unece.org/trans/main/wp29/wp29wgs/wp29gen/wp29resolutions.html) [↑](#footnote-ref-3)