**Proposal for amendments to ECE/TRANS/WP.29/GRPE/2023/02, the 08 series of amendments to UN Regulation No. 83 (Emissions of M1, M2, N1 and N2 vehicles))**

This document proposes some amendments to the above paper which OICA members request to be integrated at first adoption of the new Regulation as proposed by ECE/TRANS/WP.29/GRPE/2023/02 within the 87th session of GRPE. The modifications to the current text of the Regulation are marked in bold for new or strikethrough for deleted characters.

I. Proposal

*paragraph 2.1.*, amendto read:

"2.1. "Vehicle type" means a group of vehicles that ~~do not differ in the following respects:~~ **fulfil the requirements for a vehicle type with regard to emissions in accordance with paragraph 3.0.1. of UN Regulation No. 154.**

~~2.1.1. The equivalent inertia determined in relation to the reference mass as prescribed in Table A4a/3 of Annex 4a of the 07 series of amendments to this Regulation; and~~

~~2.1.2. The engine and vehicle characteristics as defined in Annex 1 to this Regulation.~~"

*paragraph 2.37.*, amendto read:

"2.37. "Portable emissions measurement system" (PEMS) means a portable emissions measurement system meeting the requirements specified in~~Appendix 1 to Annex IIIA~~ **Annex 4 of UN Regulation No. [XYZ]**."

*paragraph 3.3.*, amendto read:

"3.3. **Reserved** ~~For the tests described in paragraph 5. of this Regulation a vehicle representative of the vehicle type to be approved shall be submitted to the Technical service responsible for the approval tests.~~"

*paragraph 7.1.*, amendto read:

"7.1. Extensions for ~~tailpipe~~ **idling** emissions (Type 2 test)"

*paragraph 7.2.2.2.*, amendto read:

"7.2.2.2. To determine whether type approval can be extended, for each of the transmission ratios used in the Type 6 test, the proportion,

(E) = **|**(V2 – V1)**|**/V1

shall be determined where, at an engine speed of 1,000 min –1, V1 is the speed of the vehicle-type approved and V2 is the speed of the vehicle type for which extension of the approval is requested."

*paragraph (a) to Appendix 3a of Annex 1*, amendto read:

"(a) a declaration of the manufacturer that the vehicle does not contain any defeat device not covered by one of the exceptions in paragraph ~~5.1.3.~~ **5.1.7.** of this Regulation;"

*item (i) to paragraph (d) to Appendix 3a of Annex 1*, amendto read:

"(i) why any of the exception clauses from the defeat device prohibition in paragraph ~~5.1.3.~~ **5.1.7.** of this Regulation apply;"

*paragraph (f) to Appendix 3a of Annex 1*, amendto read:

"(f) a description of the hierarchical relations among the AES (i.e., when more than one AES can be active concurrently, an indication of which AES is primary in responding, the method by which strategies interact, including data flow diagrams and decision logic and how does the hierarchy assure emissions from all AES are controlled to the lowest practical level**)**;"

*item “Versioning table” of Table A1/1 to Appendix 3a of Annex 1*, amendto read:

"…

|  |  |
| --- | --- |
| Versioning table | Content of each version modifications~~: and with~~ **and which** part is modified |

…"

**II. Justification**

1. The proposed definition of a vehicle type for the 08 series of amendments to UN Regulation No. 83 could lead to the case that vehicles which fall within a single *“Vehicle type with regard to emissions”* in accordance with UN Regulation No. 154 would not fulfil the requirements to be covered by a single type-approval according to the 08 series of amendments to UN Regulation No. 83. Therefor it is proposed to align the vehicle type definition of the 08 series of amendments to UN Regulation No. 83 to the type definition of UN Regulation No. 154.
2. The definition for “Portable emissions measurement system (PEMS)” refers to requirements specified in Appendix 1 to Annex IIIA. However, UN Regulation No. 83 in its 08 series of amendments does not contain an Annex IIIA. The definition got carried over unchanged from COMMISSION REGULATION (EU) 2017/1151 as amended by 2018/1832, where Appendix 1 to Annex IIIA refers to “Test procedure for vehicle emissions testing with a Portable Emissions Measurement System (PEMS)”. The chapter with the same headline is included within Annex 4 to the new UN Regulation [XYZ] on RDE.
3. Paragraph 3.3. and 3.3.6 are almost a word-by-word duplication. However, paragraph 3.3.6. gives a more precise reference to Table A, therefor paragraph 3.3. should be amended as described above.
4. The description of paragraph 7.1. is referring to “tailpipe emissions” and more precisely in detail to the Type 2 test. The Type 2 test however provides the procedure to determine idling emissions as it is also described within paragraph 1. of the regulation.
5. The formula specified in paragraph 7.2.2.2. of the 08 series of amendments to UN Regulation No. 83 got carried over from the 07 series of amendments to UN Regulation No. 83, however within the 07 series of amendments the absolute value of (V2 – V1) is used as the numerator which fits better to the prescribed tolerances of (E).
6. Paragraph (a) and item (i) of paragraph (d) to Appendix 3a of Annex 1 refer to paragraph 5.1.3. of the 08 series of amendments to UN Regulation No. 83. However, the content of paragraph 5.1.3. is “Reserved”. The description of the “Extended Documentation Package” got carried over from COMMISSION REGULATION (EU) 2017/1151 as amended by 2023/443, where the corresponding paragraphs refer to Article 5(2) of Regulation (EC) No 715/2007. The same content and requirements of Article 5(2) of Regulation (EC) No 715/2007 are contained within 5.1.7. of the 08 series of amendments to UN Regulation No. 83.
7. Addition of a closing bracket.
8. Correction of misspelling.