**Proposal for a new Supplement to the 05 series of amendments to UN Regulation No. 49 (Emissions of compression ignition and positive ignition (LPG and CNG) engines)**

This document aims at permitting the use of hydrogen (H2) as fuel for emissions type approval of heavy-duty vehicles. The modifications to the current text of the Regulation are marked in bold for new or strikethrough for deleted characters.

I. Proposal

*Paragraph 1.1.,* amend to read:

"Table A

**Applicability**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *Vehicle category1* | *Positive-ignition engines* | | | | *Dual-fuel*  *engines* | *Compression-ignition engines* | | |
| *Petrol* | *NGa* | *LPGb* | ***H2e*** | *Diesel* | *Ethanol* | ***H2e*** |
| M1 | R49 or R83c | R49 or R83c | R49 or R83c | **R49 or R83c** | R49d | R49 or R83c | R49 or R83c | **R49 or R83c** |
| M2 | R49 or R83c | R49 or R83c | R49 or R83c | **R49 or R83c** | R49 or R83c | R49 or R83c | **R49 or R83c** |
| M3 | R49 | R49 | R49 | **R49** | R49 | R49 | **R49** |
| N1 | R49 or R83c | R49 or R83c | R49 or R83c | **R49 or R83c** | R49 or R83c | R49 or R83c | **R49 or R83c** |
| N2 | R49 or R83c | R49 or R83c | R49 or R83c | **R49 or R83c** | R49 or R83c | R49 or R83c | **R49 or R83c** |
| N3 | R49 | R49 | R49 | **R49** | R49 | R49 | **R49** |
| 1 As defined in the Consolidated Resolution on the Construction of Vehicles (R.E.3), document  ECE/TRANS/WP.29/78/Rev.3, para.2.  a Natural Gas.  b Liquefied Petroleum Gas.  c Regulation No. 83 applies for vehicles with a reference mass ≤ 2,610 kg and by extension of an approval for vehicles with a reference mass ≤ 2,840 kg.  d The provisions related to dual-fuel engines and vehicles contained into Regulation No. 49 only apply for vehicles and engines within the scope of the revision 5 of that Regulation.  **e Hydrogen fuel specified by paragraph 4.6.3.3. (a) or (c)**  **f Hydrogen fuel specified by paragraph 4.6.3.3. (b) or (d)** | | | | | | | | |

Table B

**Requirements**

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | *Positive-ignition engines* | | | | *Dual-fuel*  *engines c* | *Compression-ignition engines* | | | |
|  | *Petrol* | *NG* | *LPG* | **H2d** | *Diesel* | *Ethanol* | **H2e** | |
| Gaseous pollutants | - | Yes | Yes | **Yesf** | Yes | Yes | Yes | **Yesf** | |
| Particulates | - | Yesa | Yesa | **Yes** | Yes | Yes | Yes | **Yes** | |
| Smoke | - | - | - | **-** | Yes | Yes | Yes | **-** | |
| Durability | - | Yes | Yes | **Yes** | Yes | Yes | Yes | **Yes** | |
| In-service-conformity | - | Yes | Yes | **Yes** | Yes | Yes | Yes | **Yes** | |
| OBD | - | Yesb | Yesb | **Yesb** | Yes | Yes | Yes | **Yes** | |
| a Only applicable to stage C in Table 2 of paragraph 5.2.1.  b Application dates according to paragraph 5.4.2.  c According to the requirements of Annex 11.  **d Hydrogen fuel specified by paragraph 4.6.3.3. (a) or (c)**  **e Hydrogen fuel specified by paragraph 4.6.3.3. (b) or (d)**  **f Measurement of CH4 and CO2 is not required and the manufacturer, technical service**  **or Type Approval Authority may choose to measure the total hydrocarbon (THC) emissions**  **instead of measuring the non-methane hydrocarbon emissions.**" | | | | | | | | |

*Paragraph 2.1.37.,* amend to read:

"2.1.37. Gas engine" means a positive-ignition engine which is fuelled with NG **~~,or~~** LPG **or H2 show in paragraph 4.6.3.3.(a) (T) or 4.6.3.3.(b) (TD);**"

*Paragraph 2.2.2.,* amend to read:

"2.2.2.Symbols for chemical component

|  |  |
| --- | --- |
| CH4 | Methane |
| C2H6 | Ethane |
| C2H5OH | Ethanol |
| C3H8 | Propane |
| CO | Carbon Monoxide |
| DOP | Di-Octylphtalate |
| CO2 | Carbon Dioxide |
| **H2** | **Hydrogen** |
| HC | Hydrocarbons |
| NMHC | Non-Methane Hydrocarbons |
| NOx | Oxides of Nitrogen |
| NO | Nitric Oxide |
| NO2 | Nitrogen Dioxide |
| **O2** | **Oxygen** |
| PT | Particulates" |

*Paragraph 2.2.4.,* amend to read:

"2.2.4. Symbols for the fuel composition

|  |  |
| --- | --- |
| wALF | hydrogen content of fuel, per cent mass |
| wBET | carbon content of fuel, per cent mass |
| wGAM | sulphur content of fuel, per cent mass |
| wDEL | nitrogen content of fuel, per cent mass |
| wEPS | oxygen content of fuel, per cent mass |
| α | molar hydrogen ratio **~~(H/C)~~** |
| β | molar carbon ratio **~~(C/C)~~** |
| γ | molar sulphur ratio **~~(S/C)~~** |
| δ | molar nitrogen ratio **~~(N/C)~~** |
| ε | molar oxygen ratio **~~(O/C)~~** |
| referring to a fuel Cβ Hα Oε Nδ Sγ  β = 1 for carbon based fuels, β = 0 for hydrogen fuel" | |

*Paragraph 2.2.4.,* amend to read:

"2.2.5. Standards referenced by this Regulation

|  |  |
| --- | --- |
| ISO 15031-1 | ISO 15031-1: 2001 Road vehicles - Communication between vehicle and external equipment for emissions related diagnostics - Part 1: General information. |
|  |  |
| ISO 15031-2 | ISO/PRF TR 15031-2: 2004 Road vehicles - Communication between vehicle and external equipment for emissions related diagnostics - Part 2: Terms, definitions, abbreviations and acronyms. |
|  |  |
| ISO 15031-3 | ISO 15031-3: 2004 Road vehicles - Communication between vehicle and external equipment for emissions related diagnostics - Part 3: Diagnostic connector and related electrical circuits, specification and use. |
|  |  |
| SAE J1939-13 | SAE J1939-13: Off-Board Diagnostic Connector. |
|  |  |
| ISO 15031-4 | ISO DIS 15031-4.3: 2004 Road vehicles - Communication between vehicle and external equipment for emissions related diagnostics - Part 4: External test equipment. |
|  |  |
| SAE J1939-73 | SAE J1939-73: Application Layer – Diagnostics. |
|  |  |
| ISO 15031-5 | ISO DIS 15031-5.4: 2004 Road vehicles - Communication between vehicle and external equipment for emissions related diagnostics - Part 5: Emissions-related diagnostic services. |
|  |  |
| ISO 15031-6 | ISO DIS 15031-6.4: 2004 Road vehicles - Communication between vehicle and external equipment for emissions related diagnostics - Part 6: Diagnostic trouble code definitions. |
|  |  |
| SAE J2012 | SAE J2012: Diagnostic Trouble Code Definitions Equivalent to ISO/DIS 15031-6, April 30, 2002. |
|  |  |
| ISO 15031-7 | ISO 15031-7: 2001 Road vehicles - Communication between vehicle and external equipment for emissions related diagnostics - Part 7: Data link security. |
|  |  |
| SAE J2186 | SAE J2186: E/E Data Link Security, dated October 1996. |
|  |  |
| ISO 15765-4 | ISO 15765-4: 2001 Road vehicles - Diagnostics on Controller Area Network (CAN) - Part 4: Requirements for emissions-related systems. |
|  |  |
| SAE J1939 | SAE J1939: Recommended Practice for a Serial Control and Communications Vehicle Network. |
|  |  |
| ISO 16185 | ISO 16185: 2000 Road vehicles – engine family for homologation. |
|  |  |
| ISO 2575 | ISO 2575: 2000 Road vehicles – Symbols for controls, indicators and tell-tales. |
|  |  |
| ISO 16183 | ISO 16183: 2002 Heavy duty engines - Measurement of gaseous emissions from raw exhaust gas and of particulate emissions using partial flow dilution systems under transient test conditions. |
|  |  |
| **ISO 14687** | **ISO 14687-2019 Hydrogen fuel quality** – **Product specification.**" |

*Insert a new paragraph 3.5.,* to read:

"**3.5. Application for type approval of engines fuelled with hydrogen**

**3.5.1. In case of an application for type approval of engines fuelled with hydrogen, hydrogen shall be the fuel the engine is designed to run on primarily. Requirements for dual-fuel hydrogen engines have not yet been established under this regulation.**"

*Paragraph 4.1.1.,* amend to read:

"4.1.1. In the case of diesel, ethanol, **~~or~~** LNG20, **or Hydrogen** fuel the parent engine meets the requirements of this Regulation on the reference fuel specified in Annex 5."

*Insert a new paragraph 4.6.3.3.,* to read:

"**4.6.3.3. For hydrogen fuelled engines the approval mark shall contain a letter(s) after the national symbol, the purpose of which is to distinguish the fuel type and the working principal for which the approval has been granted. This letter(s) will be as follows:**

**(a) T in case of a PI engine being approved and calibrated for gaseous hydrogen**

**(b) TD in case of a CI engine being approved and calibrated for gaseous hydrogen**

**(c) U in case of a PI engine being approved and calibrated for liquefied hydrogen**

**(d) UD in case of a CI engine being approved and calibrated for liquefied hydrogen**"

*Insert a new paragraph 5.1.10.,* to read:

"**5.1.10. Provisions for engines fuelled with hydrogen**

**5.1.10.1. In case of an application for type approval of engines fuelled with hydrogen, the emission measurement system shall comply with the highest exhaust water content expected during emission testing. In particular it shall be ensured that the temperatures of all sample gas carrying components of the emission measurement system, except for sample dryers, remain at least 10 K above the dew point of the sample gas at the corresponding position.**"

*Paragraph 5.2.1.,* amend to read:

"5.2.1. Limit values

The specific mass of the carbon monoxide, of the total hydrocarbons, of the oxides of nitrogen and of the particulates, as determined on the ESC test, and of the smoke opacity, as determined on the ELR test, shall not exceed the amounts shown in Table 1.

The specific mass of the carbon monoxide, of the non-methane hydrocarbons, of the methane, of the oxides of nitrogen and of the particulates as determined on the ETC test shall not exceed the amounts shown in Table 2.

**Table 1  
Limit values — ESC and ELR tests**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| *Row* | *Mass of carbon monoxide*  *(CO) g/kWh* | *Mass of hydrocarbons*  *(HC) g/kWh* | *Mass of nitrogen oxides*  *(NOx) g/kWh* | *Mass of particulates*  *(PT) g/kWh* | *Smoke****b***  *m−1* |
| A (2000) | 2.1 | 0.66 | 5.0 | 0.10 // 0.13*a* | 0.8 |
| B1 (2005) | 1.5 | 0.46 | 3.5 | 0.02 | 0.5 |
| B2 (2008) | 1.5 | 0.46 | 2.0 | 0.02 | 0.5 |
| C (Enhanced Environmentally Friendly Vehicle (EEV)) | 1.5 | 0.25 | 2.0 | 0.02 | 0.15 |
| *a* For engines having a swept volume of less than 0.75 dm³ per cylinder and a rated power speed of more than 3,000 min-1  ***b* Not applicable for engines fuelled with hydrogen show in paragraph 4.6.3.3.** | | | | | |

*a*

**Table 2  
Limit values — ETC test**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| *Row* | *Mass of carbon monoxide*  *(CO) g/kWh* | *Mass of non-methane hydrocarbons*  *(NMHC) g/kWh* | *Mass of*  *(CH4)a*  *g/kWh* | *Mass of nitrogen oxides*  *(NOx) g/kWh* | *Mass of particulates (PT)*  *(PT)b g/kWh* |
| A (2000) | 5.45 | 0.78 | 1.6 | 5.0 | 0.16 // 0.21c |
| B1 (2005) | 4.0 | 0.55 | 1.1 | 3.5 | 0.03 |
| B2 (2008) | 4.0 | 0.55 | 1.1 | 2.0 | 0.03 |
| C (EEV) | 3.0 | 0.40 | 0.65 | 2.0 | 0.02 |
| *a* For NG engines only.  *b* Not applicable for gas fuelled engines at stages B1 and B2*.*  *c* For engines having a swept volume of less than 0.75 dm³ per cylinder and a rated power speed of more than 3,000 min-1  ***d* For engines where all the fuels used have a molar carbon to hydrogen ratio of 0 as defined in paragraph 8. of Annex 4A, the measurement of CH4 is not required and the manufacturer, technical service or Type Approval Authority may choose to measure the total hydrocarbon (THC) emissions instead of measuring the non-methane hydrocarbon emissions. In that case, the emission limit for the total hydrocarbon emissions is the same as shown in paragraph 5.2. of this Regulation for non-methane hydrocarbon emissions.**" | | | | | |

*Paragraph 7.2.1.,* amend to read:

"7.2.1. **~~Diesel~~ CI** engines"

*Paragraph 7.2.2.,* amend to read:

"7.2.2. **~~Gas~~ PI** engines"

*Insert a new paragraph 8.3.2.6.,* to read

"***8.3.2.6.* For hydrogen fuelled engines, all these tests may be conducted with the applicable market fuels. However, at the manufacturer’s request, the reference fuels described in Annex 5 to this Regulation may be used.**"

*Paragraph 8.3.2.6.,* amend to read:

"8.3.2.**~~6~~7**. Tests for conformity of production of a gas fuelled engine laid out for operation on one specific fuel composition shall be performed on the fuel for which the engine has been calibrated."

*Annex 1,* amend to read:

"Annex 1. Information document

This information document is related to the approval according to Regulation No. 49. It is referring to measures to be taken against the emission of gaseous and particulate pollutants from compression-ignition engines **include fuelled with hydrogen(TD/UD)** for use in vehicles, and the emission of gaseous pollutants from positive-ignition engines fuelled with natural gas **~~or~~** liquefied petroleum gas **hydrogen(T/U)** for use in vehicles.

Vehicle type/parent engine/engine type1

0. General

0.1. Make (name of undertaking):

0.2. Type and commercial description (mention any variants):

0.3. Means and location of identification of type, if marked on the vehicle:

0.4. Category of vehicle (if applicable):

0.5. Category of engine: diesel/NG fuelled/LPG fuelled/ethanol fuelled **/hydrogen fuelled**1

0.6. Name and address of manufacturer:

0.7. Location of statutory plates and inscriptions and method of affixing:

0.8. In the case of components and separate technical units, location and method of affixing of the ECE approval mark:

0.9. Address(es) of assembly plant(s):"

*Annex 1-* *Appendix1 paragraph 1.14.,* amend to read:

"1.14. Fuel: Diesel/LPG/NG-H/NG-L/NG-HL/ethanol/LNG/LNG20**/Hydrogen (T) /Hydrogen (TD) /Hydrogen (U) /Hydrogen (UD)**2,5"

*Annex 1-* *Appendix1 paragraph 3.1.,* amend to read:

"3.1. **~~Diesel~~** **Compression-ignition (C.I.)**  engines, including dual-fuel engines"

*Annex 1-* *Appendix1 paragraph 3.2.,* amend to read:

"3.2. **~~Gas fuelled~~** **Positive-ignition (P.I.)**  engines, including dual-fuel engines"

*Annex 1-* *Appendix1 paragraph 9.3.,* amend to read:

"9.3. **~~Diesel~~ Compression-ignition (C.I.)** /**~~gas~~ positive-ignition (P.I.)**  engines"

*Annex 1-* *Appendix2 paragraph 2.1.,* amend to read:

"2.1. Name of **~~diesel~~ compression-ignition (C.I.)** engine family:"

*Annex 1-* *Appendix2 paragraph 2.2.,* amend to read:

"2.2. Name of **~~gas~~** **positive-ignition (P.I.)** engine family:"

*Annex 1-* *Appendix3 paragraph 1.14.,* amend to read:

"1.14. Fuel: Diesel/LPG/NG-H/NG-L/NG-HL/ethanol/LNG/LNG20**/Hydrogen (T) /Hydrogen (TD) /Hydrogen (U) /Hydrogen (UD)**2,5"

*Annex 1-* *Appendix3 paragraph 3.1.,* amend to read:

"3.1. **~~Diesel~~** **Compression-ignition (C.I.)**  engines, including dual-fuel engines"

*Annex 1-* *Appendix3 paragraph 3.2.,* amend to read:

"3.2. **~~Gas fuelled~~** **Positive-ignition (P.I.)**  engines, including dual-fuel engines"

*Annex 1-* *Appendix1 paragraph 6.3.1.,* amend to read:

"6.3.1. **~~Diesel~~ Compression-ignition (C.I.)** /**~~gas~~ positive-ignition (P.I.)**  engines;4"

*Annex 2A,* amend to read:

"…of a compression-ignition (C.I.) engine type or family (Diesel or Ethanol **or Hydrogen (TD) or Hydrogen (UD)**), or a positive-ignition (P.I.) engine type or family (NG or LPG **or Hydrogen (T) or Hydrogen (U)**),2 as a separate technical unit with regard to the emission of pollutants pursuant to Regulation No. 49, 05 series of amendments"

*Annex 2A, paragraph 11.4.,* amend to read:

"

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| *ETC test* | | | | | |
| *DF:* | *CO* | *NMHC* | *CH4* | *NOx* | *PT* |
| *Emissions* | *CO (g/kWh)* | *NMHC (g/kWh) 2,4* | *CH4 (g/kWh) 2,4* | *NOx (g/kWh)* | *PT (g/kWh)2* |
| Measured with regeneration: |  |  |  |  |  |
| Measured without regeneration: |  |  |  |  |  |
| Measured/weighted: |  |  |  |  |  |
| Calculated with DF: |  |  |  |  |  |

"

*Annex 2A, foot note,* amend to read:

"1 Distinguishing number of the country which has granted/extended/refused/withdrawn approval (see approval provisions in the Regulation).

2 Strike out what does not apply.

3 For each member of the family.

**4 For engines where all the fuels used have a molar carbon to hydrogen ratio of 0 as defined in paragraph 8. of Annex 4A, the measurement of CH4 is not required and the manufacturer, technical service or Type Approval Authority may choose to measure the total hydrocarbon (THC) emissions instead of measuring the non-methane hydrocarbon emissions. In that case, the emission limit for the total hydrocarbon emissions is the same as shown in paragraph 5.2. of this Regulation for non-methane hydrocarbon emissions.** "

*Annex 2B, paragraph 9.4.,* amend to read:

"

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| *ETC test* | | | | | |
| *DF:* | *CO* | *NMHC* | *CH4* | *NOx* | *PT* |
| *Emissions* | *CO*  *(g/kWh)* | *NMHC*  *(g/kWh)2,4* | *CH4*  *(g/kWh) 2,4* | *NOx*  *(g/kWh)* | *PT*  *(g/kWh) 2* |
| Measured with regeneration: |  |  |  |  |  |
| Measured without regeneration: |  |  |  |  |  |
| Measured/weighted: |  |  |  |  |  |
| Calculated with DF: |  |  |  |  |  |

"

*Annex 2B, foot note,* amend to read:

"1 Distinguishing number of the country which has granted/extended/refused/withdrawn approval (see approval provisions in the Regulation).

2 Strike out what does not apply.

3 **For engines where all the fuels used have a molar carbon to hydrogen ratio of 0 as defined in paragraph 8. of Annex 4A, the measurement of CH4 is not required and the manufacturer, technical service or Type Approval Authority may choose to measure the total hydrocarbon (THC) emissions instead of measuring the non-methane hydrocarbon emissions. In that case, the emission limit for the total hydrocarbon emissions is the same as shown in paragraph 5.2. of this Regulation for non-methane hydrocarbon emissions.**"

*Annex 4A, Appendix 1, paragraph 5.,* amend to read:

"5. Calculation of the gaseous emissions

**Calculation of hydrocarbons and/or non-methane hydrocarbons is based on the following molar carbon/hydrogen/oxygen ratios (C/H/O) of the fuel:**

**CH1.85 for diesel,**

**CH3O0.5 for ethanol for dedicated C.I. engines,**

**CH2.525 for LPG (liquefied petroleum gas),**

**CH2.93 for NG (Non-Methane Hydrocarbons (NMHC)).**

**CH4 for NG**

**H2 for hydrogen.**"

*Annex 4A, Appendix 1, paragraph 5.2.,* amend to read:

"5.2. Dry / wet correction

The measured concentration shall be converted to a wet basis according to the following formulae, if not already measured on a wet basis. The conversion shall be done for each individual mode.

The *ugas*-values and molar ratios as described in paragraphs A.5.2. and A.5.3. of Appendix 5 to Annex 11 shall be used for dual-fuel engines, operating in dual-fuel mode,

dry

W

wet

c

k

c





For the raw exhaust gas:

**(a)**



or**:**

**(b)**



or**:**

**(c)**



with

kf = 0.055594 x wALF + 0.0080021 x wDEL + 0.0070046 x wEPS

and

kw1 = 

Where:

Ha = intake air humidity, g water per kg dry air

wALF = hydrogen content of the fuel, per cent mass

qmf,i = instantaneous fuel mass flow rate, kg/s

qmad,i = instantaneous dry intake air mass flow rate, kg/s

pr = water vapour pressure after cooling bath, kPa

pb = total atmospheric pressure, kPa

wDEL = nitrogen content of the fuel, per cent mass

wEPS = oxygen content of the fuel, per cent mass

α = molar hydrogen ratio of the fuel

cCO2 = dry CO2 concentration, per cent

cCO = dry CO concentration, per cent

**(a) and (b) are principally identical with the factor 1.008 in (a) and (c) being an approximation for the more accurate denominator in (b). (c) is not applicable, if one of the fuels used has a molar carbon to hydrogen ratio of 0. (a) to (c) are not applicable in the case that water injection is used.**

For the diluted exhaust gas:

**(d)**

1

2

1

200

%

1

W

CO

w

We

K

c

K

























**

or**:**

**(e)**





































200

%

1

1

2

1

2

CO

d

W

We

c

K

K

**

**(d) and (e) are not applicable if one of the fuels used has a molar carbon to hydrogen ratio of 0.**

…"

*Annex 4A, Appendix 1, paragraph 5.5.Table 6,* amend to read:

# "Table 6

# **Values of ugas in the raw and dilute exhaust gas for various exhaust components**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| *Fuel* |  | *NOx* | *CO* | *THC/NMHC* | *CO2* | *CH4* | *Density* |
| Diesel | Exhaust raw | 0.001587 | 0.000966 | 0.000479 | 0.001518 | 0.000553 | 1.2943 |
| Exhaust dilute | 0.001588 | 0.000967 | 0.000480 | 0.001519 | 0.000553 | 1.293 |
| Ethanol | Exhaust raw | 0.001609 | 0.000980 | 0.000805 | 0.001539 | 0.000561 | 1.2757 |
| Exhaust dilute | 0.001588 | 0.000967 | 0.000795 | 0.001519 | 0.000553 | 1.293 |
| CNG | Exhaust raw | 0.001622 | 0.000987 | 0.000523 | 0.001552 | 0.000565 | 1.2661 |
| Exhaust dilute | 0.001588 | 0.000967 | 0.000584 | 0.001519 | 0.000553 | 1.293 |
| Propane | Exhaust raw | 0.001603 | 0.000976 | 0.000511 | 0.001533 | 0.000559 | 1.2805 |
| Exhaust dilute | 0.001588 | 0.000967 | 0.000507 | 0.001519 | 0.000553 | 1.293 |
| Butane | Exhaust raw | 0.001600 | 0.000974 | 0.000505 | 0.001530 | 0.000558 | 1.2832 |
| Exhaust dilute | 0.001588 | 0.000967 | 0.000501 | 0.001519 | 0.000553 | 1.293 |
| Hydrogen | Exhaust raw | 0.001729 | 0.001053 | 0.000075 | 0.001654 | 0.000603 | 1.1872 |
| *Notes:*  - u values of raw exhaust based on ideal gas properties at λ = 2. dry air, 273 K, 101.3 kPa  - u values of dilute exhaust based on ideal gas properties and density of air  - u values of CNG accurate within 0.2 per cent for mass composition of: C = 66 to 76 per cent; H = 22 to 25 per cent; N = 0 to 12 per cent  - u value of CNG for HC corresponds to CH2.93 (for total HC use u value of CH4) | | | | | | | |

…"

*Annex 4A, Appendix 2, paragraph 3.,* amend to read:

"3. Emissions test run

At the manufacturers request, a dummy test may be run for conditioning of the engine and exhaust system before the measurement cycle.

NG and LPG **and hydrogen** fuelled engines shall be run-in using the ETC test. The engine shall be run over a minimum of two ETC cycles and until the CO emission measured over one ETC cycle does not exceed by more than 10 per cent the CO emission measured over the previous ETC cycle."

*Annex 4A, Appendix 2, paragraph 4.2.5.,* amend to read:

"4.2.5. Air flow and air-to-fuel ratio measurement method

This involves exhaust mass calculation from the air flow and the air to fuel ratio. The calculation of the instantaneous exhaust gas mass flow is as follows:



With:

Where:

A/Fst = stoichiometric air to fuel ratio, kg/kg

**β** **is the molar carbon ratio of the fuel, with β=1 for fuels containing carbon and β=0 for fuels with a molar carbon to hydrogen ratio of 0 as defined in paragraph 4. of this annex.**

λ = excess air ratio **calculated by λi or measured by a lambda sensor**

cCO2 = dry CO2 concentration, per cent

cCO = dry CO concentration, ppm

cHC = HC concentration, ppm

**λi is not applicable if one of the fuels used has a molar carbon to hydrogen ratio of 0 as defined in paragraph 4. of this annex.**"

The air flowmeter shall meet the accuracy specifications of paragraph 2.2. of Appendix 4 to this annex, the CO2 analyzer used shall meet the specifications of paragraph 3.3.2. of Appendix 4 to this annex and the total system shall meet the accuracy specifications for the exhaust gas flow.

Optionally, air to fuel ratio measurement equipment such as a zirconia type sensor may be used for the measurement of the excess air ratio which meets the specifications of paragraph 3.3.6. of Appendix 4 to this annex."

*Annex 4A, Appendix 5, paragraph 1.9.1.,* amend to read:

"1.9.1. CO analyzer interference check

Water and CO2 can interfere with the CO analyzer performance. Therefore, a CO2 span gas having a concentration of 80 to 100 per cent of full scale of the maximum operating range used during testing shall be bubbled through water at room temperature and the analyzer response recorded. The analyzer response shall not be more than **~~1 per cent of full scale for ranges equal to or above 300 ppm or more than 3 ppm for ranges below 300 ppm~~** **2 per cent of the mean CO concentration expected during testing or 20 ppm, whichever is larger**."

*Annex 4A, Appendix 5, paragraph 3.2.2.,* amend to read:

"3.2.2. Carbon flow check

(a) A carbon flow check using actual exhaust is recommended for detecting measurement and control problems and verifying the proper operation of the partial flow system. The carbon flow check should be run at least each time a new engine is installed, or something significant is changed in the test cell configuration.

(b) The engine shall be operated at peak torque load and speed or any other steady state mode that produces 5 per cent or more of CO2. The partial flow sampling system shall be operated with a dilution factor of about 15 to 1.

(c) If a carbon flow check is conducted, the procedure given in Appendix 6 to this annex shall be applied. The carbon flow rates shall be calculated according to paragraphs 2.1. to 2.3. of Appendix 6 to this annex. All carbon flow rates should agree to within 6 per cent of each other. **In the case that a hydrogen fuelled engine is to be tested, the carbon flow check should be performed on a diesel fuelled engine prior to the installation of the hydrogen fuelled engine.**"

*Annex 4A, Appendix 6, paragraph 2.4.,* amend to read:

"2.4. The molecular mass (Mre) of the exhaust gas shall be calculated as follows:

Where:

qmf = fuel mass flow rate, kg/s

qmaw = intake air mass flow rate on wet basis, kg/s

Ha = humidity of intake air, g water per kg dry air

Mra = molecular mass of dry intake air (= 28.9 g/mol)

α, δ, ε, γ = molar ratios referring to a fuel C**β** Hα Oδ Nε Sγ.

Alternatively, the following molecular masses may be used:

Mre (diesel) = 28.9 g/mol

Mre (LPG) = 28.6 g/mol

Mre (NG) = 28.3 g/mol."

*Annex 5,* insert new paragraph 4. to read:

"4. **Technical data of the Hydrogen reference fuels for testing compression-ignition or positive ignition**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| *Characteristics* | *Units* | *Limits* | | | *Test Method* |
| *Minimum* | | *Maximum* |
| Hydrogen fuel index | % mole fraction | 99.97 | |  | (a) |
| Total non-hydrogen gases | μmol/mol |  | | 300 |  |
| Lists of non-hydrogen gases and the specification of each contaminant **(f)** | | | | |  |
| Water (H2O) | μmol/mol |  | 5 | | (e) |
| Total hydrocarbons(b) except methane (C1 equivalent) | μmol/mol |  | 2 | | (e) |
| Methane (CH4) | μmol/mol |  | 100 | | (e) |
| Oxygen (O2) | μmol/mol |  | 5 | | (e) |
| Helium (He) | μmol/mol |  | 300 | | (e) |
| Total Nitrogen (N2) and Argon (Ar) (b) | μmol/mol |  | 300 | | (e) |
| Carbon dioxide (CO2) | μmol/mol |  | 2 | | (e) |
| Carbon monoxide (CO) (c) | μmol/mol |  | 0.2 | | (e) |
| Total sulfur compounds (d) (H2S basis) | μmol/mol |  | 0.004 | | (e) |
| Formaldehyde (HCHO) | μmol/mol |  | 0.2 | | (e) |
| Formic acid (HCOOH) | μmol/mol |  | 0.2 | | (e) |
| Ammonia (NH3) | μmol/mol |  | 0.1 | | (e) |
| Total halogenated compounds (e)  (Halogenate ion basis) | μmol/mol |  | 0.05 | | (e) |
| (a)  The hydrogen fuel index is determined by subtracting the “total non-hydrogen gases” in this table, expressed in mole per cent, from 100 mole per cent.  (b) Total hydrocarbons except methane include oxygenated organic species.  (c) The sum of measured CO, HCHO and HCOOH shall not exceed 0.2 µmol/mol  (d)  As a minimum, total sulphur compounds include H2S, COS, CS2 and mercaptans, which are typically found in natural gas.  (e) Test method shall be documented. Test methods defined in ISO21087 are preferable.  (f) The analysis of specific contaminants depending on the production process shall be exempted. A vehicle manufacturer shall provide the responsible authority reasons for exempting specific contaminants." | | | | | |

*Annex 9*A*, paragraph 3.2.1.*, amend to read:

"3.2.1. Introduction

From the dates given in paragraph 5.4.2. of this Regulation, the OBD system of all **~~diesel~~ Compression Ignition (hereinafter, this is called "CI")** engines and of vehicles equipped with a **~~diesel~~ CI** engine shall indicate the failure of an emission‑related component or system when that failure results in an increase in emissions above the appropriate OBD thresholds given in the table in paragraph 5.4.4. of this Regulation."

*Annex 9*A*, paragraph 3.2.3.1.*, amend to read:

"3.2.3.1. As an alternative to monitoring against the appropriate OBD threshold limits with respect to paragraphs 3.2.2.1. to 3.2.2.4. of this annex, OBD systems of **~~diesel~~ CI** engines may in accordance with paragraph 5.4.1.1. of this Regulation monitor for major functional failure of the following components:

…"

*Annex 9*A*, paragraph 3.3.1.*, amend to read:

"3.3.1. From the dates given in paragraph 5.4.2. of this Regulation the OBD system of all **~~diesel~~ CI** or **~~gas~~** **Positive Ignition (hereinafter, this is called "PI")** engines and of vehicles equipped with a **~~diesel~~ CI** or a **~~gas~~** **PI** engine shall indicate the failure of an emission‑related component or system of the engine system when that failure results in an increase in emissions above the appropriate OBD thresholds given in the table in paragraph 5.4.4. of this Regulation.

…"

*Annex 9B, paragraph 3.36.,* amend to read:

"3.36. Abbreviations

AES Auxiliary Emission Strategy

**CI Compression Ignition**

CV Crankcase Ventilation

DOC Diesel Oxidation Catalyst

DPF Diesel Particulate Filter or Particulate Trap including catalyzed DPFs**,** ~~and~~ Continuously Regenerating Traps (CRT) **and other soot particle filters**

DTC Diagnostic trouble code

EGR Exhaust Gas Recirculation

HC Hydrocarbon

LNT Lean NOx Trap (or NOx absorber)

LPG Liquefied Petroleum Gas

MECS Malfunction Emission Control Strategy

NG Natural Gas

NOx Oxides of Nitrogen

OTL OBD Threshold Limit

**PI Positive Ignition**

PM Particulate Matter

SCR Selective Catalytic Reduction

SW Screen Wipers

TFF Total Functional Failure monitoring

VGT Variable Geometry Turbocharger

VVT Variable Valve Timing"

*Annex 9B, paragraph 5.2.3.,* amend to read:

"5.2.3. Low fuel level

Manufacturers may request approval to disable monitoring systems that are affected by low fuel level / pressure or running out of fuel (e.g. diagnosis of a malfunction of the fuelling system or misfiring) as follows:

|  |  |  |  |
| --- | --- | --- | --- |
|  | ~~Diesel~~ | ~~Gas~~ | |
|  |  | ~~NG~~ | ~~LPG~~ |
| ~~(a) The low fuel level considered for such a disablement shall not exceed 100 litres or 20 per cent of the nominal capacity of the fuel tank, whichever is lower.~~ | ~~X~~ |  | ~~X~~ |
| ~~(b) The low fuel pressure in the tank considered for such a disablement shall not exceed 20 per cent of the usable range of fuel tank pressure.~~ |  | ~~X~~ |  |

|  |  |  |
| --- | --- | --- |
|  | **Liquid fuel storage** | **Gaseous fuel storage** |
| **(a) The low fuel level considered for such a disablement shall not exceed 100 litres or 20 per cent of the nominal capacity of the fuel tank, whichever is lower.** | **X** |  |
| **(b) The low fuel pressure in the tank considered for such a disablement shall not exceed 20 per cent of the usable range of fuel tank pressure.** |  | **X** |

"

*Annex 9B, Appendix 3 – Item 6,* amend to read:

"Appendix 3 - Item 6

Exhaust Gas Recirculation (EGR) system monitoring

The OBD system shall monitor the following elements of the EGR system on engines so equipped for proper operation:

|  |  |  |
| --- | --- | --- |
|  | ~~Diesel~~  **CI engine** | ~~Gas~~  **PI engine** |
| (a1) EGR low/high flow: the EGR system's ability to maintain the commanded EGR flow rate, detecting both “flow rate too low” and “flow rate too high” conditions – emission threshold monitoring. | X |  |
| (a2) EGR low/high flow: the EGR system's ability to maintain the commanded EGR flow rate, detecting both “flow rate too low” and “flow rate too high” conditions – performance monitoring (monitoring requirement to be further discussed). |  | X |
| (b) Slow response of the EGR actuator: the EGR system's ability to achieve the commanded flow rate within a manufacturer specified time interval following the command – performance monitoring. | X | X |
| (c) EGR cooler under cooling performance: the EGR cooler system's ability to achieve the manufacturer's specified cooling performance – performance monitoring. | X | X |

…"

*Annex 9B, Appendix 3 – Item 7,* amend to read:

"Appendix 3 - Item 7

Fuel System monitoring

The OBD system shall monitor the following elements of the fuel system on engines so-equipped for proper operation:

|  |  |  |
| --- | --- | --- |
|  | ~~Diesel~~  **CI engine** | ~~Gas~~  **PI engine** |
| (a) Fuel system pressure control: fuel system ability to achieve the commanded fuel pressure in closed loop control – performance monitoring. | X |  |
| (b) Fuel system pressure control: fuel system ability to achieve the commanded fuel pressure in closed loop control in the case where the system is so constructed that the pressure can be controlled independently of other parameters – performance monitoring. | X |  |
| (c) Fuel injection timing: fuel system ability to achieve the commanded fuel timing for at least one of the injection events when the engine is equipped with the appropriate sensors – performance monitoring. | X |  |
| (d) Fuel injection system: ability to maintain the desired air-fuel ratio (incl. but not limited to self adaptation features) – performance monitoring. |  | X |

"

*Annex 9B, Appendix 3 – Item 8,* amend to read:

"Appendix 3 - Item 8

Air handling and turbocharger/Boost pressure control system

The OBD system shall monitor the following elements of the Air handling and Turbocharger/Boost pressure Control System on engines so-equipped for proper operation:

|  |  |  |
| --- | --- | --- |
|  | ~~Diesel~~  **CI engine** | ~~Gas~~  **PI engine** |
| (a1) Turbo under/over boost: turbo boost system's ability to maintain the commanded boost pressure, detecting both “boost pressure too low” and “boost pressure too high” conditions – emission threshold monitoring. | X |  |
| (a2) Turbo under/over boost: turbo boost system's ability to maintain the commanded boost pressure, detecting both “boost pressure too low” and “boost pressure too high” conditions – performance monitoring (monitoring requirement to be further discussed). |  | X |
| (b) Variable Geometry Turbo (VGT) slow response: VGT system's ability to achieve the commanded geometry within a manufacturer specified time-performance monitoring. | X | X |
| (c) Charge air cooling: Charge air cooling system efficiency - total functional failure. | X | X |

…"

*Annex 9B, Appendix 3 – Item 10,* amend to read:

"Appendix 3 - Item 10

Misfire Monitoring

|  |  |  |
| --- | --- | --- |
|  | ~~Diesel~~  **CI engine** | ~~Gas~~  **PI engine** |
| (a) No prescriptions. | X |  |
| (b) Misfire that may cause catalyst damage (e.g. by monitoring a certain percentage of misfiring in a certain period of time) – performance monitoring (monitoring requirement to be further discussed together with items 6 and 8). |  | X |

"

*Annex 9B, Appendix 3 – Item 13,* amend to read:

"Appendix 3 - Item 13

Exhaust gas and oxygen sensors monitoring

The OBD system shall monitor:

|  |  |  |
| --- | --- | --- |
|  | ~~Diesel~~  **CI engine** | ~~Gas~~  **PI engine** |
| (a) The electrical elements of the exhaust gas sensors on engines so-equipped for proper operation according to item 1 to this appendix – component monitoring. | X | X |
| (b) Both the primary and secondary (fuel control) oxygen sensors. These sensors are considered as exhaust gas sensors to be monitored for proper operation according to item 1 to this appendix – component monitoring. |  | X |

"

*Annex 9B, Appendix 3 – Item 15,* amend to read:

"Appendix 3 - Item 15

Three-way catalyst

The OBD system shall monitor the three-way catalyst on engines so-equipped for proper operation:

|  |  |  |
| --- | --- | --- |
|  | ~~Diesel~~  **CI engine** | ~~Gas~~  **PI engine** |
| (a) Three-way Catalyst Conversion efficiency: the catalyst ability to convert NOx and CO – performance monitoring |  | X |

"

**II. Justification**

1. Hydrogen-fuelled vehicles are covered by UN Regulation No. 83 and UN Regulation No. 154 (LDV emission control), and hydrogen-fuelled engines are covered by UN Regulation No. 49, Series 07 (HDV emission control). However, hydrogen-fuelled engines are not yet covered in UN Regulation No. 49, Series 05 and 06.

2. Hydrogen fuelled engines could be one complementary option to reduce CO2 emission of future heavy-duty vehicles

3. Hydrogen fuel should be included in the UN Regulation No. 49, Series 05 and 06 similarly to UN Regulation No. 49, Series 07 (HDV emission control)

4. This amendment aims to integrate only mono-fuel hydrogen engines. Further amendments integrating hydrogen dual-fuel engines are expected to follow when their validation can be accomplished.