|  |  |
| --- | --- |
| Submitted by the expert from France | Informal document GRBP-79-50  (79th GRBP, 6-9 February 2024,  agenda item 7 (d)) |

Proposal for amendments to the working document ECE/TRANS/WP.29/GRBP/2024/4 (Supplement 2 to the 04 series of amendments to UN Regulation No. 117)

The text reproduced below was prepared by the expert from the France to amend document GBRP/2024/4. The modifications are marked in bold for new or strikethrough for deleted characters.

1. Proposal

*Annex 7, Paragraph 2.*, amend to read:

"2. Spin traction method for classes C1 and C2 tyres (traction force test per paragraph ~~6.4.~~ **6.5**. (b) of this Regulation)."

*Annex 8, Paragraph 2.4.5.1.2.*, amend to read:

"2.4.5.1.2. The control tyre shall pass the ice grip index threshold defined in paragraph ~~6.4.2.~~ **6.5.2.** of this Regulation."

1. Justification

Since the introduction of the adhesion of tyres in worn state on wet surfaces, paragraph 6.4 related to snow tyre for use in severe snow conditions was renumbered to 6.5., which needs to be reflected in the Annexes 7 and 8.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_