|  |  |
| --- | --- |
|  | E/ECE/324/Rev.2/Add.124/Rev.3/Amend.3−E/ECE/TRANS/505/Rev.2/Add.124/Rev.3/Amend.3 |
|  |  | 28 November 2023 |

 Agreement

 Concerning the Adoption of Harmonized Technical United Nations Regulations for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these United Nations Regulations[[1]](#footnote-2)\*

(Revision 3, including the amendments which entered into force on 14 September 2017)

\_\_\_\_\_\_\_\_\_

 Addendum 124 – UN Regulation No. 125

Revision 3– Amendment 3

Supplement 3 to the 02 series of amendments – Date of entry into force: 24 September 2023

 Uniform provisions concerning the approval of motor vehicles with regard to the forward field of vision of the motor vehicle driver

This document is meant purely as documentation tool. The authentic and legal binding text is: ECE/TRANS/WP.29/2023/22 (as amended by paragraph 92 of the report ECE/TRANS/WP.29/1171).

**\_\_\_\_\_\_\_\_\_**

**UNITED NATIONS**

*Paragraph 5.1.3.5.5.,* amend to read:

"5.1.3.5.5. It shall be possible for the driver to switch off the FVA by a deliberate action consisting of at least one manual option with maximum of 2 consecutive steps. Intuitive action (e.g. double press, swipe and press) is considered as a single step. This provision does not apply when the vehicle is in a backing event as defined in UN Regulation No. 158."

Insert new paragraph 5.1.3.7., to read:

"5.1.3.7. Information to the driver, mandated by any UN Regulations, shall not be replaced by Information given via the FVA system. A duplication of such mandatory information via the FVA system is possible."

*Annex 5,* amend to read:

"Annex 5

Field of View Assistant

# Examples for Warning / Highlight / Information as specified in paragraph 5.3.5.1.:

|  | *Examples* |
| --- | --- |
|  |  |
| Warning/Highlight hazardous traffic situation | Abrupt braking situations or other emergency cases Oncoming traffic in turning manoeuvresOncoming Traffic Jam/vehicle break down.Vehicles leaving the lane or entering the own driving path |
| Warning/highlight vulnerable road users or other road users which may be overseen | PedestriansCyclistsCrossing road usersRoad users in blind spot or road users covered by other objectsAnimals |
| Information to maintain the distances to surrounding road user and infrastructure as well as information on the infrastructure | Distance to vehicle in front/ to side / to rearLane keep assist, lane change assist, speed limits changes |
| Information to find and maintain the correct driveway and to follow the road instructions | Navigation Information, symbols and arrows during automatic lane change(Directions, remaining distance to target, border crossings)Highlighting stop lines and pedestrian crosswalks  |
| Information to support driver’s setting | Highlighting edges of the position of the FVA area during adjustment  |
| Warnings and information to the driver that require drivers immediate action | Transition demand/ Hands-off warning Requests to stop the vehicle immediately due to safety relevant failures of the vehicle or its systemsRequests to switch off systems immediately due to safety relevant failures.  |

"

1. \* Former titles of the Agreement:

 Agreement concerning the Adoption of Uniform Conditions of Approval and Reciprocal Recognition of Approval for Motor Vehicle Equipment and Parts, done at Geneva on 20 March 1958 (original version);

 Agreement concerning the Adoption of Uniform Technical Prescriptions for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these Prescriptions, done at Geneva on 5 October 1995 (Revision 2). [↑](#footnote-ref-2)