|  |
| --- |
| E/ECE/324/Rev.1/Add.16/Rev.7/Amend.1−E/ECE/TRANS/505/Rev.1/Add.16/Rev.7/Amend.1 |
|  |  | 29 July 2024 |

 Agreement

 Concerning the Adoption of Harmonized Technical United Nations Regulations for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these United Nations Regulations[[1]](#footnote-2)\*

(Revision 3, including the amendments which entered into force on 14 September 2017)

\_\_\_\_\_\_\_\_\_

 Addendum 16: UN Regulation No. 17

 Revision 7 – Amendment 1

11 series of amendments – Date of entry into force: 15 June 2024

 Uniform provisions concerning the approval of vehicles with regard to the seats, their anchorages and any head restraints

This document is meant purely as documentation tool. The authentic and legal binding text is:

- ECE/TRANS/WP.29/2023/106

**\_\_\_\_\_\_\_\_\_**

**UNITED NATIONS**

 *Reference to Consolidated Resolution on the Construction of Vehicles (R.E.3.)*, *in all the text of the UN Regulation*, amend to read:

 "As defined in the Consolidated Resolution on the Construction of Vehicles (R.E.3.), document ECE/TRANS/WP.29/78/Rev.7, … - https://unece.org/transport/standards/transport/vehicle-regulations-wp29/resolutions"

*Paragraph 1,* amend to read:

 "1. Scope

 This Regulation applies to:

(a) Vehicles of categories M1 and N[[2]](#footnote-3) with regard to the strength of seats and their anchorages and with regard to their head restraints;

(b) Vehicles of categories M2 and M31 with regard to seats not covered by Regulation No. 80, in respect of the strength of seats and their anchorages, and in respect of their head restraints;

(c) Vehicles of category M1 with regard to the design of the rear parts of seat backs and the design of devices intended to protect the occupants from the danger resulting from the displacement of luggage in a frontal impact.

 It does not apply to vehicles with regard to side-facing or rearward-facing seats, or to any head restraint fitted to these seats, with the exception vehicles of category M2 and M3 of classes A and I, subject to the provisions of paragraph 5.1.1.

Vehicles of other categories may also be approved under this Regulation, in respect of the strength of seats and their anchorages, and in respect of their head restraints."

*Paragraphs 5.4. to 5.4.2*., amend to read:

"5.4. Mounting of head restraints

5.4.1. A head restraint shall be mounted on every outboard front seat in every vehicle of category M1.

5.4.2. A head restraint shall be mounted on every outboard front seat in every vehicle of category M2 with a maximum mass not exceeding 3500 kg and of category N1; head restraints mounted in such vehicles shall comply with the requirements of Regulation No. 25, as amended by 04 series of amendments."

Alternatively, seats fitted with head restraints in these categories of vehicles may comply with the requirements of this Regulation."

*Insert a new paragraph 5.4.3*., to read:

"5.4.3. Notwithstanding paragraphs 5.4.1. and 5.4.2. above, all forward-facing seats fitted with a head restraint or intended to be fitted with a head restraint in other seating positions and in other categories of vehicles covered by the scope of this UN Regulation shall comply with the requirements of this Regulation."

*Paragraph 5.7.4.,* amend to read:

"5.7.4. Head restraint height retention

When tested in accordance with Annex 13, the mechanism of the adjustable head restraint or any head restraint fulfilling one of the additional requirements described under paragraph 5.8.4. shall not fail in such a way as to allow downward movement of the head restraint by more than 25 mm."

*Insert new paragraphs 13.14. to 13.14.5*., to read:

"13.14. As from the official date of entry into force of the 11 series of amendments, no Contracting Party applying this Regulation shall refuse to grant or refuse to accept UN type approvals under this Regulation as amended by the 11 series of amendments.

13.14.1. As from 1 September 2026, Contracting Parties applying this Regulation shall not be obliged to accept UN type approvals to the preceding series of amendments that were first issued on or after 1 September 2026.

13.14.2. Until 1 September 2028, Contracting Parties applying this Regulation shall accept UN type approvals to the preceding series of amendments that were first issued before 1 September 2026.

13.14.3. As from 1 September 2028, Contracting Parties applying this Regulation shall not be obliged to accept type approvals issued to the preceding series of amendments to this Regulation.

13.14.4. Notwithstanding paragraph 13.14.3., Contracting Parties applying the Regulation shall continue to accept UN type approvals to the preceding series of amendments to the Regulation, for vehicles which are not affected by the changes introduced by the 11 series of amendments.

13.14.5. Contracting Parties applying this Regulation shall not refuse to grant UN type approvals according to any preceding series of amendments to this Regulation or extensions thereof."

*Paragraph 4.2.,* amend to read:

"4.2. An approval number shall be assigned to each type approved in accordance with Schedule 4 of the Agreement (E/ECE/TRANS/505/Rev.3 and Amend.1).

The same Contracting Party may not assign the same number either to the same vehicle type equipped with other types of seats or head restraints or with seats anchored differently on the vehicle (this applies both to seats with and to those without head restraints) or to another vehicle type."

*Annex 2,* amend to read:

"Annex 2

Arrangements of the Approval Mark

Model A

(see paragraphs 4.4., 4.4.1., 4.4.2. and 4.4.3. of this Regulation)

# Vehicle with at least one seat fitted or capable of being fitted with a head restraint



**17RA - 112439**

 a = 8 mm min.

 The above approval mark when affixed to a vehicle shows that the vehicle type concerned, with regard to the strength of the seats fitted or capable of being fitted with head restraints and with regard to characteristics of the head restraints, has been approved in the Netherlands (E 4) pursuant to UN Regulation No. 17, under the approval number 112439. The first two digits of the approval number indicate that the Regulation already contained the ~~10~~**11** series of amendments at the time of approval. The above approval mark also shows that the vehicle type was approved pursuant to UN Regulation No. 17 with regard to the strength of any seats on the vehicle which are not fitted or capable of being fitted with head restraints.

Model B

(see paragraphs 4.4.; 4.4.1. and 4.4.2. of this Regulation)

# Vehicle with seats not fitted or not capable of being fitted with head restraints



**17R - 112439**

 a = 8 mm min.

 The above approval mark when affixed to a vehicle shows that the vehicle type has seats not fitted or capable of being fitted with head restraints, and has, with regard to the strength of the seats and their anchorages, been approved in the Netherlands (E 4) pursuant to UN Regulation No. 17 under the approval number 112439. The first two digits of the approval number indicate that the Regulation already contained the 11 series of amendments at the time of approval.

Model C

(see paragraphs 4.5. of this Regulation)

Vehicle with at least one seat fitted or capable of being fitted with a head restraint



**11 2439**

 a = 8 mm min.

 The above approval mark when affixed to a vehicle shows that the vehicle type has at least one seat fitted or capable of being fitted with a head restraint, and was approved in the Netherlands (E 4) pursuant to UN Regulations Nos. 17 and 33.[[3]](#footnote-4)1

 The approval numbers indicate that, on the dates when approval was granted, UN Regulation No. 17 included the 11 series of amendments, but UN Regulation No. 33 was still in its original form. The above approval mark also shows that the vehicle type was approved pursuant to UN Regulation No. 17 with regard to the strength of any seats on the vehicle which are not fitted or capable of being fitted with head restraints.

Model D

(see paragraphs 4.5. of this Regulation)

# Vehicle with seats not fitted or not capable of being fitted with head restraints



**11 2439**

 a = 8 mm min.

The above approval mark when affixed to a vehicle shows that the vehicle type has seats not fitted or capable of being fitted with head restraints, and was approved in the Netherlands (E 4) pursuant to UN Regulations Nos. 17 and 33.[[4]](#footnote-5)1 The approval numbers indicate that, on the dates when approval was granted, UN Regulation No. 17 included the 11 series of amendments but UN Regulation No. 33 was still in its original form."

*Annex 13, paragraph 2.1.,* amend to read:

"2.1. Seat set-up

Adjust the head restraint in the normal position of use or in case of an adjustable head restraint so that its effective top is at any of the following height positions at any backset position:"

1. \* Former titles of the Agreement:

 Agreement Concerning the Adoption of Uniform Conditions of Approval and Reciprocal Recognition of Approval for Motor Vehicle Equipment and Parts, done at Geneva on 20 March 1958 (original version);

 Agreement concerning the Adoption of Uniform Technical Prescriptions for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these Prescriptions, done at Geneva on 5 October 1995 (Revision 2). [↑](#footnote-ref-2)
2. As defined in the Consolidated Resolution on the Construction of Vehicles (R.E.3.), document ECE/TRANS/WP.29/78/Rev.7, para. 2 -
https://unece.org/transport/standards/transport/vehicle-regulations-wp29/resolutions [↑](#footnote-ref-3)
3. 1 The second number is given merely as an example. [↑](#footnote-ref-4)
4. 1 The second number is given merely as an example. [↑](#footnote-ref-5)