Proposal for amendments to GRVA-20-09

(Proposal for a new UN Regulation on [...] Emergency Lane Keeping System (ELKS))

The text reproduced below was prepared by the experts from China. It is based on working document GRVA-20-09. The modifications to the existing text of the document are marked in **bold** for new or strikethrough for deleted characters..

I. Proposal

*Paragraph 8.2.2.1.,* amend to read:

“8.2.2.1. … The vehicle manufacturer shall demonstrate, through the use of documentation, that the system works at all load conditions (**including at the mass of a vehicle in running order**)”

So does 9.2.2.1.

Delete the “-” between “in” and “load” in *9.2.2.1.*, amend to read:

“9.2.2.1. Test mass

The subject vehicle shall be tested in load condition agreed between the manufacturer and the Technical Service.”

II. Justification

1. The amendment reminds to use definition of para. *2.6. ‘Mass of a vehicle in running order’*.

1. The definition of *‘Mass of a vehicle in running order’* is described in para. 2.6, but it is not quoted in the original text.
2. It is suggested that it be quoted in the requirements for test mass in 8.2.2.1 and 9.2.2.1.

2. Para. 9.2.2.1. mentioned “in-load condition”. It should be consistent with the text in para. 8.2.2.1 “in load condition”.

\_\_\_\_\_\_\_\_\_\_\_