|  |  |  |
| --- | --- | --- |
|  | E/ECE/324/Rev.1/Add.36/Rev.7/Amend.12−E/ECE/TRANS/505/Rev.1/Add.36/Rev.7/Amend.12 | |
|  |  | 16 December 2024 |

Agreement

Concerning the Adoption of Harmonized Technical United Nations Regulations for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these United Nations Regulations[[1]](#footnote-2)\*

(Revision 3, including the amendments which entered into force on 14 September 2017)

\_\_\_\_\_\_\_\_\_

Addendum 36 – UN Regulation No. 37

Revision 7 - Amendment 12

Supplement 49 to the 03 series of amendments – Date of entry into force: 22 September 2024

Uniform provisions concerning the approval of filament light sources for use in approved lamps of power-driven vehicles and of their trailers

This document is meant purely as documentation tool. The authentic and legal binding text is: ECE/TRANS/WP.29/2024/17

**\_\_\_\_\_\_\_\_\_**

**UNITED NATIONS**

*Paragraph 3.3.3.3.,* amend to read:

"3.3.3.3. The colour of the light emitted shall be measured by the method specified in Annex 5. Each measured value shall lie within the required chromaticity area.1[[2]](#footnote-3) Moreover, in the case of filament light sources emitting white light, the measured values shall not deviate more than 0.020 unit in the x and/or y direction from a point of choice on the Planckian locus (CIE015 :2018, 4th edition). Filament light sources for use in light-signalling devices shall meet the requirements as specified in paragraph 4.4.2. of IEC Publication 60809, Edition 4: 2021."

1. \* Former titles of the Agreement:

   Agreement concerning the Adoption of Uniform Conditions of Approval and Reciprocal Recognition of Approval for Motor Vehicle Equipment and Parts, done at Geneva on 20 March 1958 (original version);

   Agreement concerning the Adoption of Uniform Technical Prescriptions for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these Prescriptions, done at Geneva on 5 October 1995 (Revision 2). [↑](#footnote-ref-2)
2. For conformity of production purposes of amber and red colour only, at least 80 per cent of the measuring results shall lie within the required chromaticity area. [↑](#footnote-ref-3)