|  |  |  |
| --- | --- | --- |
|  |  | **INF.7** |

**Economic Commission for Europe**

Inland Transport Committee

**Working Party on the Transport of Dangerous Goods**

**100th session 14 April 2016**

Geneva, 9-13 May 2016

Item 6 (a) of the provisional agenda

**Proposals for amendments to Annexes A and B of ADR:**

**Construction and approval of vehicles**

 Transitional measure

 Transmitted by the Government of France

 Introduction

1. In May 2014, adding a new provision to require that fuel tanks for liquid fuels shall comply with ECE Regulation No. 34, the Working Party adopted the following transitional measure:

“1.6.5.16 EX/II, EX/III, FL and OX vehicles registered before 1 July 2017, fitted with fuel tanks not approved according to ECE Regulation No. 34 may still be used.”

2. As a general principle, 1.6.5.4 gives a 15-month transitional period for the construction of vehicles to be in line with ECE Regulation No. 105 on the approval of vehicles:

“1.6.5.4 As regards the construction of EX/II, EX/III, FL, OX and AT vehicles, the requirements of Part 9 in force up to 31 December 2016 may be applied until 31 March 2018.”

3. 1.6.5.4 will allow to apply ADR 2015 where ECE R 34 is not referenced until 31 March 2018 while 1.6.5.16 will require the conformity to ECE R 34 from 1 July 2017.

4. To solve this problem, we propose to extend the period for the transitional measure for compliance with ECE R 34 to 31 March 2018.

 Proposal

5. Amend 1.6.5.16 as follows:

“1.6.5.16 EX/II, EX/III, FL and OX vehicles registered before 1 April 2018, fitted with fuel tanks not approved according to ECE Regulation No. 34 may still be used.”.