|  |  |  |
| --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.29/2016/9 |
| Description: _unlogo | **Economic and Social Council** | Distr.: General23 December 2015Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**168th session**

Geneva, 8-11 March 2016

Item 4.8.2 of the provisional agenda

**1958 Agreement – Consideration of draft amendments**

**to existing Regulations submitted by GRSG**

Proposal for Supplement 3 to the 04 series of amendments to Regulation No. 46 (Devices for indirect vision)

**Submitted by the Working Party on General Safety Provisions**[[1]](#footnote-2)\*

The text reproduced below was adopted by the Working Party on General Safety Provisions (GRSG) at its 109th session (ECE/TRANS/WP.29/GRSG/88, para. 23). It is mainly based on ECE/TRANS/WP.29/GRSG/2015/23. It is submitted to the World Forum for Harmonization of Vehicle Regulations (WP.29) and to the Administrative Committee AC.1 for consideration at their March 2016 sessions.

*Paragraph 15.2.1.2*., amend to read:

"15.2.1.2. The provisions of this Regulation do not apply to the surveillance mirrors defined in paragraph 2.1.1.3. Nevertheless, the exterior surveillance mirrors shall be mounted at least 2 m above the ground when the vehicle is under a load corresponding to its maximum technical permissible mass or shall be fully integrated in a housing including Class II or III mirror(s) which is (are) type approved to this Regulation."

1. \* In accordance with the programme of work of the Inland Transport Committee for 2014–2018 (ECE/TRANS/240, para. 105 and ECE/TRANS/2014/26, programme activity 02.4), the World Forum will develop, harmonize and update Regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)