Proposal for amendments to Regulations No. 13

The modifications to the existing text of the Regulation are marked in bold for new and strikethrough for deleted characters.

1. Proposal

 *Footnote 12 in paragraph 5.2.1.32.*, amend to read:

12 Off-road vehicles, special purpose vehicles (e.g. mobile plantusing nonstandard vehicle chassis, mobile cranes, hydro-static driven vehicles in which the hydraulic drive system is also used for braking and auxiliary functions, **vehicles where a sensor(s) necessary for the function of the stability control cannot be installed due to the design of the vehicle chassis,** N2 vehicles which have all of the following features: a gross vehicle mass between 3.5 and 7.5 tonnes, a non-standard low-frame chassis, more than 2 axles and hydraulic transmission), Class I and Class A buses of categories M2 and M3, articulated buses and coaches, N2 tractors for semi-trailer with a gross vehicle mass (GVM) between 3.5 and 7.5 tonnes shall be excluded from this requirement.