|  |  |  |  |
| --- | --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.29/GRSG/2017/25/Corr.1 | |
| _unlogo | **Economic and Social Council** | | Distr.: General  28 August 2017  Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**Working Party on General Safety Provisions**

**113th session**

Geneva, 10-13 October 2017

Item 9 of the provisional agenda

**Regulation No. 116 (Anti-theft and alarm systems)**

Proposal for a new UN Regulation on uniform provisions concerning the approval of vehicle alarm systems and approval of a vehicle with regard to its vehicle alarm system

Note by the secretariat [[1]](#footnote-2)\*

**Corrigendum**

*Page 20, paragraph 11.9.1.,* correct to read:

"11.9.1. To provide information on the status of the AS (set, unset, alarm setting period, alarm has been activated), the installation of optical displays is allowed inside and optical signals outside the passenger compartment is allowed. Any optical signal or any use of lighting and light-signalling devices outside the passenger compartment shall fulfil the requirements of UN Regulation No. 48."

1. \* In accordance with the programme of work of the Inland Transport Committee for 2016–2017 (ECE/TRANS/254, para. 159 and ECE/TRANS/2016/28/Add.1, cluster 3.1), the World Forum will develop, harmonize and update Regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)