|  |  |
| --- | --- |
| Submitted by the expert from France | Informal document **GRSP-64-11**  (64th GRSP, 11-14 December 2018  agenda item 19) |

**Proposal for Corrigendum 1 to 03 Series of amendments of Regulation No. 129 (Enhanced Child Restraint Systems)**

The text reproduced below was prepared by the experts from France. It proposes a corrigendum to UN Regulation No. 129 to align the french version to the english version of document ECE/TRANS/WP.29/2018/45 already adopted during the WP29 175th session (ECE/TRANS/WP.29/1139, para. 80). The modifications to the current text of UN Regulation No. 129 are marked in bold for new characters and strikethrough for deleted characters.

**I. Proposal**

*Paragraphe 4.3 of the french version*, amend to read :

« 4.3 Les informations suivantes doivent être clairement indiquées sur le produit :

a) L’orientation du dispositif amélioré de retenue pour enfants par rapport au véhicule ;

b) La (les) gamme(s) de taille pour lesquelles le dispositif amélioré de retenue pour enfants est prévu en centimètres ;

c) La masse corporelle maximum admissible pour le dispositif **intégral** amélioré de retenue pour enfants, en kilogrammes. ».

**II. Justification**

Proposal of alignment of the french version based on the english version and on the previous series of the Regulation.

\_\_\_\_\_\_\_\_\_\_