UNITED

NATIONS

Distr.

Economic and Social	GENERAL

Council	TRANS/WP.29/2001/13
19 December 2000

Original: ENGLISH

ECONOMIC COMMISSION FOR EUROPE

INLAND TRANSPORT COMMITTEE

World Forum for Harmonization of Vehicle Regulations (WP.29)

(One-hundred-and-twenty-third session,

6-9 March 2001, agenda item 4.2.2.)

DRAFT CORRIGENDUM 1 TO SUPPLEMENT 3 TO THE 03 SERIES OF AMENDMENTS

TO REGULATION No. 36

(Large capacity passenger vehicles)

Transmitted by the Working Party on General Safety Provisions (GRSG)

Note: The text reproduced below was adopted by GRSG at its seventy-ninth session, and is transmitted for consideration to WP.29 and to AC.1. It is based on the text reproduced in the session report (TRANS/WP.29/GRSG/58, para. 18).

__________

Paragraph 5.6.4.9., correct to read (English and Russian only):

"5.6.4.9.	The service door in any open position shall not obstruct the use of, or required access to any mandatory exit."

___________

This document is a working document circulated for discussion and comments. The use of this document for other purposes is the entire responsibility of the user. Documents are also available via the INTERNET:

http://www.unece.org/trans/main/welcwp29.htm

GE.00-