UNITED

NATIONS

Distr.	GENERAL

TRANS/WP.29/607	12 December 1997

ENGLISH

Original:	ENGLISH

and FRENCH

INLAND TRANSPORT COMMITTEE

Working Party on the Construction of Vehicles

CORRIGENDUM 1 TO REGULATION No. 97

(Vehicle alarm systems)

Note: The text reproduced below was adopted by the Administrative Committee (AC.1) of the amended 1958 Agreement at its seventh session, following the recommendation by the Working Party at its one-hundred-and-thirteenth session. It is based on document TRANS/WP.29/1997/3, not amended (TRANS/WP.29/599, para. 102).

______________

Paragraph 7.2.5., add at the end the following words:

"... with fuses changed, if necessary."

Paragraph 7.2.7., amend the value of "20 mA" to read "20 mA in average".

______________

GE.97-