UNITED

NATIONS

Distr.

Economic and Social	GENERAL

Council	TRANS/WP.29/667
16 April 1999

ENGLISH

Original: ENGLISH and

FRENCH

ECONOMIC COMMISSION FOR EUROPE

INLAND TRANSPORT COMMITTEE

Working Party on the Construction of Vehicles

DRAFT SUPPLEMENT 2 TO THE 04 SERIES OF

AMENDMENTS TO REGULATION No. 22

(Protective helmets)

Note:	The text reproduced below was adopted by the Administrative Committee (AC.1) of the amended 1958 Agreement at its eleventh session, following the recommendation by the Working Party at its one-hundred-and- seventeenth session. It is based on document TRANS/WP.29/1999/17, not amended (TRANS/WP.29/663, para. 116).

__________

Paragraph 6.15.3.1., amend to read:

"6.15.3.1.	The visor shall not comprise any part liable to impair the user's peripheral vision as defined in paragraph 6.14., when the visor is in the totally opened position. Furthermore, the lower edge of the visor shall not be situated ....."

_________

GE.99-