UNITED

NATIONS

Distr.

Economic and Social	GENERAL

Council	TRANS/WP.29/678
16 April 1999

ENGLISH

Original: ENGLISH and

FRENCH

ECONOMIC COMMISSION FOR EUROPE

INLAND TRANSPORT COMMITTEE

Working Party on the Construction of Vehicles

CORRIGENDUM 1 TO REGULATION No. 109

(Retreaded pneumatic tyres for commercial vehicles and their trailers)

Note:	The text reproduced below was adopted by the Administrative Committee (AC.1) of the amended 1958 Agreement at its eleventh session, following the recommendation by the Working Party at its one-hundred-and- seventeenth session. It is based on document TRANS/WP.29/1999/8, not amended (TRANS/WP.29/663, para. 127).

__________

GE.99-

Paragraph 5.3., (French and Russian only).

Paragraph 6.2.4.2., (French only).

Annex 6,

Paragraph 1, amend to read:

".... and inflated to the Nominal Inflation Pressure quoted in the nominated International Tyre Standard (see paragraph 4.1.4.7. of this Regulation) in relation to the Maximum load carrying capacity for that Size and Load index."

_________