UNITED

NATIONS

Distr.

Economic and Social	GENERAL

Council	TRANS/WP.29/707

11 April 2000

ENGLISH

Original: ENGLISH and

FRENCH

ECONOMIC COMMISSION FOR EUROPE

INLAND TRANSPORT COMMITTEE

World Forum for Harmonization of Vehicle Regulations (WP.29)

DRAFT SUPPLEMENT 5 TO THE 02 SERIES OF AMENDMENTS TO REGULATION No. 7

(Position, stop, and end-outline marker lamps)

Note:	The text reproduced below was adopted by the Administrative Committee (AC.1) of the amended 1958 Agreement at its fourteenth session, following the recommendation by WP.29 at its one-hundred-and-twentieth session. It is based on document TRANS/WP.29/2000/10, not amended (TRANS/WP.29/703, para. 155).

___________

Paragraph 8., amend to read:

"8.	COLOUR OF LIGHT EMITTED

The colour of the light emitted inside the field of the light distribution grid defined in paragraph 2 of annex 4 shall be within the limits of the coordinates prescribed in annex 5 to this Regulation. Outside this field, no sharp variation of colour shall be observed."

___________

GE.00-