UNITED

NATIONS

Distr.

Economic and Social	GENERAL

Council	TRANS/WP.29/715
13 April 2000

ENGLISH

Original: ENGLISH

and FRENCH

ECONOMIC COMMISSION FOR EUROPE

INLAND TRANSPORT COMMITTEE

World Forum for Harmonization of Vehicle Regulations (WP.29)

DRAFT SUPPLEMENT 7	TO REGULATION No. 23

(Reversing lamps)

Note: The text reproduced below was adopted by the Administrative Committee (AC.1) of the amended 1958 Agreement at its fourteenth session, following the recommendation by WP.29 at its one-hundred-and-twentieth session. It is based on document TRANS/WP.29/2000/11, not amended (TRANS/WP.29/703, para. 160).

__________

Paragraph 8., amend to read:

"8.	COLOUR OF LIGHT EMITTED

The colour of the light emitted inside the field of the light distribution grid defined at paragraph 2 of annex 3 shall be white and, in case of doubt, may be checked on the basis of the definition of the colour of white light given in annex 4 to this Regulation. Outside this field no sharp variation of colour shall be observed."

__________

GE.00-