UNITED

NATIONS

Distr.

Economic and Social	GENERAL

Council	TRANS/WP.29/721
3 May 2000

ENGLISH

Original: ENGLISH

and FRENCH

ECONOMIC COMMISSION FOR EUROPE

INLAND TRANSPORT COMMITTEE

World Forum for Harmonization of Vehicle Regulations (WP.29)

CORRIGENDUM 1 TO SUPPLEMENT 4 TO REGULATION No. 43

(Safety glazing)

Note: The text reproduced below was adopted by the Administrative Committee (AC.1) of the amended 1958 Agreement at its fourteenth session, following the recommendation by WP.29 at its one-hundred-and-twentieth session. It is based on document TRANS/WP.29/2000/20, not amended (TRANS/WP.29/703, para. 166).

__________

Annex 14, paragraph 6.2.1., Annex 15, paragraph 5.1.1. and Annex 16,

paragraph 6.2.1., amend the value of "1 600 MJ/m2" to read "500 MJ/m2".

____________

GE.00-