Suggestion for amendment of UN Regulation No. 118

(Burning behaviour of materials)

The text reproduced below was prepared by the expert from Germany to amend informal document GRSG-118-04e by the BMFE Informal Working Group to improve the text.

The modifications to informal document GRSG-118-04e are marked in bold for new characters and strikethrough for deleted characters.

**I Proposal**

*Annex 2*, amend 5.1. to read:

“5. Adhesive agents

5.1. ~~In cases where adhesive agents are used to affix the material to supporting structures or bonding materials together, l~~**L**ist of the adhesive agents that can be used without deterioration of the burning behaviour of the material(s): …“

*Part I,* amend paragraph 5.2.4.1. to read:

“5.2.4.1 Single materials fulfilling the relevant requirements of paragraphs 6.2.1. to 6.2.7., that are bonded together by an adhesive agent not exacerbating the burning behaviour are considered to fulfil the requirements as a composite material. **The information document in annex 2 shall contain a list of adhesive agents that can be used without deterioration of the burning behaviour of the material.**

**II Justifications**

In order not to have requirements in the information document in Annex 2 of the regulation the proposed text was added as requirement to the main part of the regulation.