|  |  |  |
| --- | --- | --- |
|  | E/ECE/324/Rev.1/Add.36/Rev.7/Amend.6−E/ECE/TRANS/505/Rev.1/Add.36/Rev.7/Amend.6 | |
|  |  | 22 June 2015 |

Agreement

Concerning the Adoption of Uniform Technical Prescriptions for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these Prescriptions[[1]](#footnote-2)\*

(Revision 2, including the amendments which entered into force on 16 October 1995)

\_\_\_\_\_\_\_\_\_

Addendum 36 – Regulation No. 37

Revision 7 - Amendment 6

Supplement 43 to the 03 series of amendments – Date of entry into force: 15 June 2015

Uniform provisions concerning the approval of filament lamps for use in approved lamp units of power-driven vehicles and of their trailers

This document is meant purely as documentation tool. The authentic and legal binding text is: ECE/TRANS/WP.29/2014/56.

**\_\_\_\_\_\_\_\_\_**



**UNITED NATIONS**

*Annex 1,*

*Sheet WT21W/1, the table,* amend to read:

"

|  |  |  |  |
| --- | --- | --- | --- |
| Cap: | WT21W: WUX2.5x16d  WTY21W: WUY2.5x16d | in accordance with IEC Publication 60061 | (sheet 7004-176-1)  (sheet 7004-177-1) |

"

*Sheet WT21/7W/1, the table,* amend to read:

"

|  |  |  |  |
| --- | --- | --- | --- |
| Cap: | WT21/7W: WZX2.5x16q  WTY21/7W: WZY2.5x16q | in accordance with IEC Publication 60061 | (sheet 7004-180-1)  (sheet 7004-181-1) |

"

1. \* Former title of the Agreement: Agreement Concerning the Adoption of Uniform Conditions of Approval and Reciprocal Recognition of Approval for Motor Vehicle Equipment and Parts, done at Geneva on 20 March 1958. [↑](#footnote-ref-2)