|  |  |  |
| --- | --- | --- |
|  | E/ECE/324/Rev.1/Add.45/Rev.6/Amend.1−E/ECE/TRANS/505/Rev.1/Add.45/Rev.6/Amend.1 | |
|  |  | 28 October 2016 |

Agreement

Concerning the Adoption of Uniform Technical Prescriptions for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these Prescriptions[[1]](#footnote-2)\*

(Revision 2, including the amendments which entered into force on 16 October 1995)

\_\_\_\_\_\_\_\_\_

Addendum 45 – Regulation No. 46

Revision 6 - Amendment 1

Supplement 3 to the 04 series of amendments – Date of entry into force: 8 October 2016

Uniform provisions concerning the approval of devices for indirect vision and of motor vehicles with regard to the installation of these devices

This document is meant purely as documentation tool. The authentic and legal binding text is: ECE/TRANS/WP.29/2016/9.

**\_\_\_\_\_\_\_\_\_**

**UNITED NATIONS**

*Paragraph 15.2.1.2*., amend to read:

"15.2.1.2. The provisions of this Regulation do not apply to the surveillance mirrors defined in paragraph 2.1.1.3. Nevertheless, the exterior surveillance mirrors shall be mounted at least 2 m above the ground when the vehicle is under a load corresponding to its maximum technical permissible mass or shall be fully integrated in a housing including Class II or III mirror(s) which is (are) type approved to this Regulation."

1. \* Former title of the Agreement: Agreement Concerning the Adoption of Uniform Conditions of Approval and Reciprocal Recognition of Approval for Motor Vehicle Equipment and Parts, done at Geneva on 20 March 1958. [↑](#footnote-ref-2)