|  |  |  |
| --- | --- | --- |
|  | E/ECE/324/Rev.1/Add.36/Rev.7/Amend.9−E/ECE/TRANS/505/ Rev.1/Add.36/Rev.7/Amend.9 | |
|  |  | 2 November 2018 |

Agreement

Concerning the Adoption of Harmonized Technical United Nations Regulations for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these United Nations Regulations[[1]](#footnote-2)\*

(Revision 3, including the amendments which entered into force on 14 September 2017)

\_\_\_\_\_\_\_\_\_

Addendum 36 – UN Regulation No. 37

Revision 7 - Amendment 9

Supplement 46 to the 03 series of amendments – Date of entry into force: 16 October 2018

Uniform provisions concerning the approval of filament lamps for use in approved lamp units of power-driven vehicles and of their trailers

This document is meant purely as documentation tool. The authentic and legal binding text is: ECE/TRANS/WP.29/2018/29.

**\_\_\_\_\_\_\_\_\_**

**UNITED NATIONS**

*Paragraph 3.6.3.,* amend to read:

"3.6.3. The colour of the light emitted shall be measured by the method specified in Annex 5. Each measured value shall lie within the required chromaticity area5. Moreover, in the case of filament light sources emitting white light, the measured values shall not deviate more than 0.020 unit in the x and/or y direction from a point of choice on the Planckian locus (CIE [015:2004](http://www.cie.co.at/index.php/Publications/index.php?i_ca_id=304), 3rd edition). Filament light sources for use in light signalling devices shall meet the requirements as specified in paragraph 4.4.2. of IEC Publication 60809, Edition 3.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

5 For conformity of production purposes of amber and red colour only, at least 80 per cent of the measuring results shall lie within the required chromaticity area."

1. \* Former titles of the Agreement:

   Agreement concerning the Adoption of Uniform Conditions of Approval and Reciprocal Recognition of Approval for Motor Vehicle Equipment and Parts, done at Geneva on 20 March 1958 (original version);

   Agreement concerning the Adoption of Uniform Technical Prescriptions for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these Prescriptions, done at Geneva on 5 October 1995 (Revision 2). [↑](#footnote-ref-2)