E/ECE/324

Rev.1/Add. 25 / Corr. 1

E/ECE/TRANS/505

23 June 1986

AGREEMENT

CONCERNING THE ADOPTION OF UNIFORM CONDITIONS OF APPROVAL

AND RECIPROCAL RECOGNITION OF APPROVAL

FOR MOTOR VEHICLE EQUIPMENT AND PARTS

done at Geneva on 20 March 1958

---------------

Addendum 25: Regulation No. 26

date of entry into force as an annex to the Agreement

1 July 1972

Corrigendum 1 *

UNIFORM PROVISIONS CONCERNING THE APPROVAL OF VEHICLES

WITH REGARD TO THEIR EXTERNAL PROJECTIONS

________________________________

UNITED NATIONS

------------------------

Depositary notification CN.92.1986.TREATIES-21 dated 23 May 1986

GE.86-22109/1367e

Paragraph 6.5.2., amend to read:

"6.5.2.	If the line of the bumper which corresponds to the outline contour of the car vertical projection is on a rigid surface, that surface shall have a minimum radius of curvature of 5 mm at all its points lying from the contour line to 20 mm inward, and a minimum radius of curvature of 2.5 mm in all other cases."

_________________