E/ECE/324

Rev.1/Add.80/Amend.1

E/ECE/TRANS/505

7 May 1998

AGREEMENT

CONCERNING THE ADOPTION OF UNIFORM TECHNICAL PRESCRIPTIONS

FOR WHEELED VEHICLES, EQUIPMENT AND PARTS WHICH CAN BE FITTED AND/OR

BE USED ON WHEELED VEHICLES AND THE CONDITIONS FOR RECIPROCAL RECOGNITION

OF APPROVALS GRANTED ON THE BASIS OF THESE PRESCRIPTIONS */

(Revision 2, including the amendments entered into force on 16 October 1995)

__________

Addendum 80: Regulation No. 81

Amendment 1

Supplement 1 to the original version of the Regulation - Date of entry into force: 3 January 1998

UNIFORM PROVISIONS CONCERNING THE APPROVAL OF REAR-VIEW MIRRORS OF TWO-WHEELED POWER-DRIVEN VEHICLES WITH OR WITHOUT SIDE CAR, WITH REGARD TO THE MOUNTING OF REAR-VIEW MIRRORS ON HANDLEBARS

__________

UNITED NATIONS

_____________

*/	Former title of the Agreement:

Agreement Concerning the Adoption of Uniform Conditions of Approval and Reciprocal Recognition of Approval for Motor Vehicle Equipment and Parts, done at Geneva on 20 March 1958.

GE.98-

Paragraph 5.4.1., footnote 1/, amend to read:

"1/	1 for Germany, ..... 8 for the Czech Republic, ..... 15 (vacant), ..... 22 for the Russian Federation, 23 for Greece, 24 (vacant), 25 for Croatia, 26 for Slovenia, 27 for Slovakia, 28 for Belarus, 29 for Estonia, 30 (vacant), 31 for Bosnia and Herzegovina, 32-36 (vacant) and 37 for Turkey. Subsequent numbers ....."

Paragraph 16.2.1., amend to read:

"16.2.1.	All two-wheeled vehicles with a maximum design speed not exceeding 50 km/h must be fitted with at least one rear-view mirror. If one only, this rear-view mirror must be fitted ....."

Paragraph 16.2.2., amend to read:

"16.2.2.	All two-wheeled vehicles with a maximum design speed exceeding 50 km/h and all three-wheeled vehicles must be fitted with two rear-view mirrors, ....."

Annex 2, item 3, amend to read:

"3.	Vehicle maximum design speed: 2/ ≤ 50 km/h / > 50 km/h"

__________