Proposal of corrections to ECE/TRANS/WP.29/GRSP/2021/2

**Proposal for Addendum 1 to Mutual Resolution No. 1 (Specifications for the Construction, Preparation and Certification of the 50th percentile male Biofidelic Rear Impact Dummy, (BioRID-II UN) anthropomorphic test Device)**

I. Proposal

*Contents, list of Appendices,*

*Appendix 7*, amend to read:

“Appendix 7. – ~~Limbs~~ **Arms and Hands**”

*Appendix 8.*, amend to read:

“Appendix 8. – ~~Tools~~ **Legs and Feet**”

*Insert new Appendix 9*, to read:

“**Appendix 9. – Tools**”

*Text of the Resolution,*

*Annex 2, Engineering Drawings and Parts List*, *paragraph 4*, amend to read:

"4. List of Appendices

Appendix 1. Assembly Drawings

Appendix 2. Head

Appendix 3. Cervical Spine

Appendix 4. Thoracic and Lumbar Spine

Appendix 5. Torso and Pelvis

Appendix 6. Muscle Substitute


Appendix 7. ~~Limbs~~ **Arms and Hands**

Appendix 8. ~~Tools~~ **Legs and Feet**

**Appendix 9. – Tools**."

*Figure 81*, amend to read:

"Figure 81  
**Inserting the Bumper in the Vertebra**~~Remove the two M2.5 SHCS that retain the T1 pin at the C7-T1 joint (Figure 82). Slide the T1 pin out of the vertebrae joint (Figure 83) and set it aside along with the two M2.5-0.45 x 8 SHCS for re-installation later.~~



**Remove the two M2.5 SHCS that retain the T1 pin at the C7-T1 joint (Figure 82). Slide the T1 pin out of the vertebrae joint (Figure 83) and set it aside along with the two M2.5-0.45 x 8 SHCS for re-installation later**."

|  |  |
| --- | --- |
|  |  |